From e3f9f86ddec3e4a07333fa7f368440e09a7252ce Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 19 Apr 2016 14:40:08 -0700
Subject: [PATCH 270/423] bcm2708: Reference the HDMI power domain for the HDMI
 driver.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
+++ b/arch/arm/boot/dts/overlays/vc4-kms-v3d-overlay.dts
@@ -6,6 +6,7 @@
 /plugin/;
 
 #include "dt-bindings/clock/bcm2835.h"
+#include "dt-bindings/power/raspberrypi-power.h"
 #include "dt-bindings/gpio/gpio.h"
 
 / {
@@ -72,6 +73,7 @@
 				clocks = <&cprman BCM2835_PLLH_PIX>,
 					 <&cprman BCM2835_CLOCK_HSM>;
 				clock-names = "pixel", "hdmi";
+				power-domains = <&power RPI_POWER_DOMAIN_HDMI>;
 			};
 
 			v3d@7ec00000 {
