From f1e53ac0a99e3754465bd87ae1a6fdbfb8340d15 Mon Sep 17 00:00:00 2001
From: Alexey Brodkin <abrodkin@synopsys.com>
Date: Mon, 15 Aug 2016 14:42:44 +0300
Subject: [PATCH] arc: Add "model" properly in device tree description of all
 boards

As it was discussed quite some time ago (see
https://lkml.org/lkml/2015/11/5/862) it's a good practice to add
"model" property in .dts. Moreover as per ePAPR "model" property is
required and should look like "manufacturer,model" so we do here.

Signed-off-by: Alexey Brodkin <abrodkin@synopsys.com>
Cc: Vineet Gupta <vgupta@synopsys.com>
Cc: Jonas Gorski <jonas.gorski@gmail.com>
Cc: Arnd Bergmann <arnd@arndb.de>
Cc: Rob Herring <robh@kernel.org>
Cc: Christian Ruppert <christian.ruppert@alitech.com>
---
 arch/arc/boot/dts/abilis_tb100_dvk.dts | 1 +
 arch/arc/boot/dts/abilis_tb101_dvk.dts | 1 +
 arch/arc/boot/dts/axs101.dts           | 1 +
 arch/arc/boot/dts/axs103.dts           | 1 +
 arch/arc/boot/dts/axs103_idu.dts       | 1 +
 arch/arc/boot/dts/nsim_700.dts         | 1 +
 arch/arc/boot/dts/nsim_hs.dts          | 1 +
 arch/arc/boot/dts/nsim_hs_idu.dts      | 1 +
 arch/arc/boot/dts/nsimosci.dts         | 1 +
 arch/arc/boot/dts/nsimosci_hs.dts      | 1 +
 arch/arc/boot/dts/nsimosci_hs_idu.dts  | 1 +
 arch/arc/boot/dts/vdk_hs38.dts         | 1 +
 arch/arc/boot/dts/vdk_hs38_smp.dts     | 1 +
 13 files changed, 13 insertions(+)

diff --git a/arch/arc/boot/dts/abilis_tb100_dvk.dts b/arch/arc/boot/dts/abilis_tb100_dvk.dts
index 3dd6ed9..3acf04d 100644
--- a/arch/arc/boot/dts/abilis_tb100_dvk.dts
+++ b/arch/arc/boot/dts/abilis_tb100_dvk.dts
@@ -24,6 +24,7 @@
 /include/ "abilis_tb100.dtsi"
 
 / {
+	model = "abilis,tb100";
 	chosen {
 		bootargs = "earlycon=uart8250,mmio32,0xff100000,9600n8 console=ttyS0,9600n8";
 	};
diff --git a/arch/arc/boot/dts/abilis_tb101_dvk.dts b/arch/arc/boot/dts/abilis_tb101_dvk.dts
index 1cf51c2..37d88c5 100644
--- a/arch/arc/boot/dts/abilis_tb101_dvk.dts
+++ b/arch/arc/boot/dts/abilis_tb101_dvk.dts
@@ -24,6 +24,7 @@
 /include/ "abilis_tb101.dtsi"
 
 / {
+	model = "abilis,tb101";
 	chosen {
 		bootargs = "earlycon=uart8250,mmio32,0xff100000,9600n8 console=ttyS0,9600n8";
 	};
diff --git a/arch/arc/boot/dts/axs101.dts b/arch/arc/boot/dts/axs101.dts
index 3f9b058..d9b9b9d 100644
--- a/arch/arc/boot/dts/axs101.dts
+++ b/arch/arc/boot/dts/axs101.dts
@@ -13,6 +13,7 @@
 /include/ "axs10x_mb.dtsi"
 
 / {
+	model = "snps,axs101";
 	compatible = "snps,axs101", "snps,arc-sdp";
 
 	chosen {
diff --git a/arch/arc/boot/dts/axs103.dts b/arch/arc/boot/dts/axs103.dts
index e6d0e31..ec7fb27 100644
--- a/arch/arc/boot/dts/axs103.dts
+++ b/arch/arc/boot/dts/axs103.dts
@@ -16,6 +16,7 @@
 /include/ "axs10x_mb.dtsi"
 
 / {
+	model = "snps,axs103";
 	compatible = "snps,axs103", "snps,arc-sdp";
 
 	chosen {
diff --git a/arch/arc/boot/dts/axs103_idu.dts b/arch/arc/boot/dts/axs103_idu.dts
index f999fef..070c297 100644
--- a/arch/arc/boot/dts/axs103_idu.dts
+++ b/arch/arc/boot/dts/axs103_idu.dts
@@ -16,6 +16,7 @@
 /include/ "axs10x_mb.dtsi"
 
 / {
+	model = "snps,axs103-smp";
 	compatible = "snps,axs103", "snps,arc-sdp";
 
 	chosen {
diff --git a/arch/arc/boot/dts/nsim_700.dts b/arch/arc/boot/dts/nsim_700.dts
index 105a001..97a9a91 100644
--- a/arch/arc/boot/dts/nsim_700.dts
+++ b/arch/arc/boot/dts/nsim_700.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsim";
 	compatible = "snps,nsim";
 	clock-frequency = <80000000>;	/* 80 MHZ */
 	#address-cells = <1>;
diff --git a/arch/arc/boot/dts/nsim_hs.dts b/arch/arc/boot/dts/nsim_hs.dts
index fc81879..1d47b14 100644
--- a/arch/arc/boot/dts/nsim_hs.dts
+++ b/arch/arc/boot/dts/nsim_hs.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsim_hs";
 	compatible = "snps,nsim_hs";
 	#address-cells = <2>;
 	#size-cells = <2>;
diff --git a/arch/arc/boot/dts/nsim_hs_idu.dts b/arch/arc/boot/dts/nsim_hs_idu.dts
index 46ab319..b3a69a8 100644
--- a/arch/arc/boot/dts/nsim_hs_idu.dts
+++ b/arch/arc/boot/dts/nsim_hs_idu.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsim_hs-smp";
 	compatible = "snps,nsim_hs";
 	interrupt-parent = <&core_intc>;
 
diff --git a/arch/arc/boot/dts/nsimosci.dts b/arch/arc/boot/dts/nsimosci.dts
index 1c169dc..80f3c33 100644
--- a/arch/arc/boot/dts/nsimosci.dts
+++ b/arch/arc/boot/dts/nsimosci.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsimosci";
 	compatible = "snps,nsimosci";
 	clock-frequency = <20000000>;	/* 20 MHZ */
 	#address-cells = <1>;
diff --git a/arch/arc/boot/dts/nsimosci_hs.dts b/arch/arc/boot/dts/nsimosci_hs.dts
index d64a96f..f680f1e 100644
--- a/arch/arc/boot/dts/nsimosci_hs.dts
+++ b/arch/arc/boot/dts/nsimosci_hs.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsimosci_hs";
 	compatible = "snps,nsimosci_hs";
 	clock-frequency = <20000000>;	/* 20 MHZ */
 	#address-cells = <1>;
diff --git a/arch/arc/boot/dts/nsimosci_hs_idu.dts b/arch/arc/boot/dts/nsimosci_hs_idu.dts
index f6bf0ca..6e46b11 100644
--- a/arch/arc/boot/dts/nsimosci_hs_idu.dts
+++ b/arch/arc/boot/dts/nsimosci_hs_idu.dts
@@ -10,6 +10,7 @@
 /include/ "skeleton.dtsi"
 
 / {
+	model = "snps,nsimosci_hs-smp";
 	compatible = "snps,nsimosci_hs";
 	clock-frequency = <5000000>;	/* 5 MHZ */
 	#address-cells = <1>;
diff --git a/arch/arc/boot/dts/vdk_hs38.dts b/arch/arc/boot/dts/vdk_hs38.dts
index 5d803dd..3c51103 100644
--- a/arch/arc/boot/dts/vdk_hs38.dts
+++ b/arch/arc/boot/dts/vdk_hs38.dts
@@ -13,6 +13,7 @@
 /include/ "vdk_axs10x_mb.dtsi"
 
 / {
+	model = "snps,vdk_archs";
 	compatible = "snps,axs103";
 
 	chosen {
diff --git a/arch/arc/boot/dts/vdk_hs38_smp.dts b/arch/arc/boot/dts/vdk_hs38_smp.dts
index 031a5bc..0054684 100644
--- a/arch/arc/boot/dts/vdk_hs38_smp.dts
+++ b/arch/arc/boot/dts/vdk_hs38_smp.dts
@@ -13,6 +13,7 @@
 /include/ "vdk_axs10x_mb.dtsi"
 
 / {
+	model = "snps,vdk_archs-smp";
 	compatible = "snps,axs103";
 
 	chosen {
-- 
2.7.4

