From a8135d0d79e9d0ad3a4ff494fceeaae838becf38 Mon Sep 17 00:00:00 2001
From: Peter Ujfalusi <peter.ujfalusi@ti.com>
Date: Mon, 14 Dec 2015 22:47:40 +0200
Subject: [PATCH 2/3] dmaengine: core: Introduce new, universal API to request
 a channel

The two API function can cover most, if not all current APIs used to
request a channel. With minimal effort dmaengine drivers, platforms and
dmaengine user drivers can be converted to use the two function.

struct dma_chan *dma_request_chan_by_mask(const dma_cap_mask_t *mask);

To request any channel matching with the requested capabilities, can be
used to request channel for memcpy, memset, xor, etc where no hardware
synchronization is needed.

struct dma_chan *dma_request_chan(struct device *dev, const char *name);
To request a slave channel. The dma_request_chan() will try to find the
channel via DT, ACPI or in case if the kernel booted in non DT/ACPI mode
it will use a filter lookup table and retrieves the needed information from
the dma_slave_map provided by the DMA drivers.
This legacy mode needs changes in platform code, in dmaengine drivers and
finally the dmaengine user drivers can be converted:

For each dmaengine driver an array of DMA device, slave and the parameter
for the filter function needs to be added:

static const struct dma_slave_map da830_edma_map[] = {
	{ "davinci-mcasp.0", "rx", EDMA_FILTER_PARAM(0, 0) },
	{ "davinci-mcasp.0", "tx", EDMA_FILTER_PARAM(0, 1) },
	{ "davinci-mcasp.1", "rx", EDMA_FILTER_PARAM(0, 2) },
	{ "davinci-mcasp.1", "tx", EDMA_FILTER_PARAM(0, 3) },
	{ "davinci-mcasp.2", "rx", EDMA_FILTER_PARAM(0, 4) },
	{ "davinci-mcasp.2", "tx", EDMA_FILTER_PARAM(0, 5) },
	{ "spi_davinci.0", "rx", EDMA_FILTER_PARAM(0, 14) },
	{ "spi_davinci.0", "tx", EDMA_FILTER_PARAM(0, 15) },
	{ "da830-mmc.0", "rx", EDMA_FILTER_PARAM(0, 16) },
	{ "da830-mmc.0", "tx", EDMA_FILTER_PARAM(0, 17) },
	{ "spi_davinci.1", "rx", EDMA_FILTER_PARAM(0, 18) },
	{ "spi_davinci.1", "tx", EDMA_FILTER_PARAM(0, 19) },
};

This information is going to be needed by the dmaengine driver, so
modification to the platform_data is needed, and the driver map should be
added to the pdata of the DMA driver:

da8xx_edma0_pdata.slave_map = da830_edma_map;
da8xx_edma0_pdata.slavecnt = ARRAY_SIZE(da830_edma_map);

The DMA driver then needs to configure the needed device -> filter_fn
mapping before it registers with dma_async_device_register() :

ecc->dma_slave.filter_map.map = info->slave_map;
ecc->dma_slave.filter_map.mapcnt = info->slavecnt;
ecc->dma_slave.filter_map.fn = edma_filter_fn;

When neither DT or ACPI lookup is available the dma_request_chan() will
try to match the requester's device name with the filter_map's list of
device names, when a match found it will use the information from the
dma_slave_map to get the channel with the dma_get_channel() internal
function.

Signed-off-by: Peter Ujfalusi <peter.ujfalusi@ti.com>
Reviewed-by: Arnd Bergmann <arnd@arndb.de>
Signed-off-by: Vinod Koul <vinod.koul@intel.com>
---
 Documentation/dmaengine/client.txt | 23 +++-------
 drivers/dma/dmaengine.c            | 89 +++++++++++++++++++++++++++++++++-----
 include/linux/dmaengine.h          | 51 +++++++++++++++++++---
 3 files changed, 127 insertions(+), 36 deletions(-)

diff --git a/Documentation/dmaengine/client.txt b/Documentation/dmaengine/client.txt
index 11fb87f..4b04d89 100644
--- a/Documentation/dmaengine/client.txt
+++ b/Documentation/dmaengine/client.txt
@@ -22,25 +22,14 @@ The slave DMA usage consists of following steps:
    Channel allocation is slightly different in the slave DMA context,
    client drivers typically need a channel from a particular DMA
    controller only and even in some cases a specific channel is desired.
-   To request a channel dma_request_channel() API is used.
+   To request a channel dma_request_chan() API is used.
 
    Interface:
-	struct dma_chan *dma_request_channel(dma_cap_mask_t mask,
-			dma_filter_fn filter_fn,
-			void *filter_param);
-   where dma_filter_fn is defined as:
-	typedef bool (*dma_filter_fn)(struct dma_chan *chan, void *filter_param);
-
-   The 'filter_fn' parameter is optional, but highly recommended for
-   slave and cyclic channels as they typically need to obtain a specific
-   DMA channel.
-
-   When the optional 'filter_fn' parameter is NULL, dma_request_channel()
-   simply returns the first channel that satisfies the capability mask.
-
-   Otherwise, the 'filter_fn' routine will be called once for each free
-   channel which has a capability in 'mask'.  'filter_fn' is expected to
-   return 'true' when the desired DMA channel is found.
+	struct dma_chan *dma_request_chan(struct device *dev, const char *name);
+
+   Which will find and return the 'name' DMA channel associated with the 'dev'
+   device. The association is done via DT, ACPI or board file based
+   dma_slave_map matching table.
 
    A channel allocated via this interface is exclusive to the caller,
    until dma_release_channel() is called.
diff --git a/drivers/dma/dmaengine.c b/drivers/dma/dmaengine.c
index 81a36fc..a094dbb 100644
--- a/drivers/dma/dmaengine.c
+++ b/drivers/dma/dmaengine.c
@@ -43,6 +43,7 @@
 
 #define pr_fmt(fmt) KBUILD_MODNAME ": " fmt
 
+#include <linux/platform_device.h>
 #include <linux/dma-mapping.h>
 #include <linux/init.h>
 #include <linux/module.h>
@@ -665,27 +666,73 @@ struct dma_chan *__dma_request_channel(const dma_cap_mask_t *mask,
 }
 EXPORT_SYMBOL_GPL(__dma_request_channel);
 
+static const struct dma_slave_map *dma_filter_match(struct dma_device *device,
+						    const char *name,
+						    struct device *dev)
+{
+	int i;
+
+	if (!device->filter.mapcnt)
+		return NULL;
+
+	for (i = 0; i < device->filter.mapcnt; i++) {
+		const struct dma_slave_map *map = &device->filter.map[i];
+
+		if (!strcmp(map->devname, dev_name(dev)) &&
+		    !strcmp(map->slave, name))
+			return map;
+	}
+
+	return NULL;
+}
+
 /**
- * dma_request_slave_channel_reason - try to allocate an exclusive slave channel
+ * dma_request_chan - try to allocate an exclusive slave channel
  * @dev:	pointer to client device structure
  * @name:	slave channel name
  *
  * Returns pointer to appropriate DMA channel on success or an error pointer.
  */
-struct dma_chan *dma_request_slave_channel_reason(struct device *dev,
-						  const char *name)
+struct dma_chan *dma_request_chan(struct device *dev, const char *name)
 {
+	struct dma_device *d, *_d;
+	struct dma_chan *chan = NULL;
+
 	/* If device-tree is present get slave info from here */
 	if (dev->of_node)
-		return of_dma_request_slave_channel(dev->of_node, name);
+		chan = of_dma_request_slave_channel(dev->of_node, name);
 
 	/* If device was enumerated by ACPI get slave info from here */
-	if (ACPI_HANDLE(dev))
-		return acpi_dma_request_slave_chan_by_name(dev, name);
+	if (has_acpi_companion(dev) && !chan)
+		chan = acpi_dma_request_slave_chan_by_name(dev, name);
+
+	if (chan) {
+		/* Valid channel found or requester need to be deferred */
+		if (!IS_ERR(chan) || PTR_ERR(chan) == -EPROBE_DEFER)
+			return chan;
+	}
+
+	/* Try to find the channel via the DMA filter map(s) */
+	mutex_lock(&dma_list_mutex);
+	list_for_each_entry_safe(d, _d, &dma_device_list, global_node) {
+		dma_cap_mask_t mask;
+		const struct dma_slave_map *map = dma_filter_match(d, name, dev);
+
+		if (!map)
+			continue;
+
+		dma_cap_zero(mask);
+		dma_cap_set(DMA_SLAVE, mask);
 
-	return ERR_PTR(-ENODEV);
+		chan = find_candidate(d, &mask, d->filter.fn, map->param);
+		if (!IS_ERR(chan))
+			break;
+	}
+	mutex_unlock(&dma_list_mutex);
+
+	return chan ? chan : ERR_PTR(-EPROBE_DEFER);
 }
-EXPORT_SYMBOL_GPL(dma_request_slave_channel_reason);
+EXPORT_SYMBOL_GPL(dma_request_chan);
 
 /**
  * dma_request_slave_channel - try to allocate an exclusive slave channel
@@ -697,17 +744,35 @@ EXPORT_SYMBOL_GPL(dma_request_slave_channel_reason);
 struct dma_chan *dma_request_slave_channel(struct device *dev,
 					   const char *name)
 {
-	struct dma_chan *ch = dma_request_slave_channel_reason(dev, name);
+	struct dma_chan *ch = dma_request_chan(dev, name);
 	if (IS_ERR(ch))
 		return NULL;
 
-	dma_cap_set(DMA_PRIVATE, ch->device->cap_mask);
-	ch->device->privatecnt++;
-
 	return ch;
 }
 EXPORT_SYMBOL_GPL(dma_request_slave_channel);
 
+/**
+ * dma_request_chan_by_mask - allocate a channel satisfying certain capabilities
+ * @mask: capabilities that the channel must satisfy
+ *
+ * Returns pointer to appropriate DMA channel on success or an error pointer.
+ */
+struct dma_chan *dma_request_chan_by_mask(const dma_cap_mask_t *mask)
+{
+	struct dma_chan *chan;
+
+	if (!mask)
+		return ERR_PTR(-ENODEV);
+
+	chan = __dma_request_channel(mask, NULL, NULL);
+	if (!chan)
+		chan = ERR_PTR(-ENODEV);
+
+	return chan;
+}
+EXPORT_SYMBOL_GPL(dma_request_chan_by_mask);
+
 void dma_release_channel(struct dma_chan *chan)
 {
 	mutex_lock(&dma_list_mutex);
diff --git a/include/linux/dmaengine.h b/include/linux/dmaengine.h
index c47c68e..d50a6b51 100644
--- a/include/linux/dmaengine.h
+++ b/include/linux/dmaengine.h
@@ -607,11 +607,38 @@ enum dmaengine_alignment {
 };
 
 /**
+ * struct dma_slave_map - associates slave device and it's slave channel with
+ * parameter to be used by a filter function
+ * @devname: name of the device
+ * @slave: slave channel name
+ * @param: opaque parameter to pass to struct dma_filter.fn
+ */
+struct dma_slave_map {
+	const char *devname;
+	const char *slave;
+	void *param;
+};
+
+/**
+ * struct dma_filter - information for slave device/channel to filter_fn/param
+ * mapping
+ * @fn: filter function callback
+ * @mapcnt: number of slave device/channel in the map
+ * @map: array of channel to filter mapping data
+ */
+struct dma_filter {
+	dma_filter_fn fn;
+	int mapcnt;
+	const struct dma_slave_map *map;
+};
+
+/**
  * struct dma_device - info on the entity supplying DMA services
  * @chancnt: how many DMA channels are supported
  * @privatecnt: how many DMA channels are requested by dma_request_channel
  * @channels: the list of struct dma_chan
  * @global_node: list_head for global dma_device_list
+ * @filter: information for device/slave to filter function/param mapping
  * @cap_mask: one or more dma_capability flags
  * @max_xor: maximum number of xor sources, 0 if no capability
  * @max_pq: maximum number of PQ sources and PQ-continue capability
@@ -666,6 +693,7 @@ struct dma_device {
 	unsigned int privatecnt;
 	struct list_head channels;
 	struct list_head global_node;
+	struct dma_filter filter;
 	dma_cap_mask_t  cap_mask;
 	unsigned short max_xor;
 	unsigned short max_pq;
@@ -1140,9 +1168,11 @@ enum dma_status dma_wait_for_async_tx(struct dma_async_tx_descriptor *tx);
 void dma_issue_pending_all(void);
 struct dma_chan *__dma_request_channel(const dma_cap_mask_t *mask,
 					dma_filter_fn fn, void *fn_param);
-struct dma_chan *dma_request_slave_channel_reason(struct device *dev,
-						  const char *name);
 struct dma_chan *dma_request_slave_channel(struct device *dev, const char *name);
+
+struct dma_chan *dma_request_chan(struct device *dev, const char *name);
+struct dma_chan *dma_request_chan_by_mask(const dma_cap_mask_t *mask);
+
 void dma_release_channel(struct dma_chan *chan);
 int dma_get_slave_caps(struct dma_chan *chan, struct dma_slave_caps *caps);
 #else
@@ -1166,16 +1196,21 @@ static inline struct dma_chan *__dma_request_channel(const dma_cap_mask_t *mask,
 {
 	return NULL;
 }
-static inline struct dma_chan *dma_request_slave_channel_reason(
-					struct device *dev, const char *name)
-{
-	return ERR_PTR(-ENODEV);
-}
 static inline struct dma_chan *dma_request_slave_channel(struct device *dev,
 							 const char *name)
 {
 	return NULL;
 }
+static inline struct dma_chan *dma_request_chan(struct device *dev,
+						const char *name)
+{
+	return ERR_PTR(-ENODEV);
+}
+static inline struct dma_chan *dma_request_chan_by_mask(
+						const dma_cap_mask_t *mask)
+{
+	return ERR_PTR(-ENODEV);
+}
 static inline void dma_release_channel(struct dma_chan *chan)
 {
 }
@@ -1186,6 +1221,8 @@ static inline int dma_get_slave_caps(struct dma_chan *chan,
 }
 #endif
 
+#define dma_request_slave_channel_reason(dev, name) dma_request_chan(dev, name)
+
 static inline int dmaengine_desc_set_reuse(struct dma_async_tx_descriptor *tx)
 {
 	struct dma_slave_caps caps;
-- 
2.8.1

