From: Gregory CLEMENT <gregory.clement@free-electrons.com>
Date: Thu, 4 Feb 2016 22:09:23 +0100
Subject: [PATCH] net: mvneta: Fix for_each_present_cpu usage

This patch convert the for_each_present in on_each_cpu, instead of
applying on the present cpus it will be applied only on the online cpus.
This fix a bug reported on
http://thread.gmane.org/gmane.linux.ports.arm.kernel/468173.

Using the macro on_each_cpu (instead of a for_each_* loop) also ensures
that all the calls will be done all at once.

Fixes: f86428854480 ("net: mvneta: Statically assign queues to CPUs")
Reported-by: Stefan Roese <stefan.roese@gmail.com>
Suggested-by: Jisheng Zhang <jszhang@marvell.com>
Suggested-by: Russell King <rmk+kernel@arm.linux.org.uk>
Signed-off-by: Gregory CLEMENT <gregory.clement@free-electrons.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -2562,7 +2562,7 @@ static void mvneta_start_dev(struct mvne
 	mvneta_port_enable(pp);
 
 	/* Enable polling on the port */
-	for_each_present_cpu(cpu) {
+	for_each_online_cpu(cpu) {
 		struct mvneta_pcpu_port *port = per_cpu_ptr(pp->ports, cpu);
 
 		napi_enable(&port->napi);
@@ -2587,7 +2587,7 @@ static void mvneta_stop_dev(struct mvnet
 
 	phy_stop(pp->phy_dev);
 
-	for_each_present_cpu(cpu) {
+	for_each_online_cpu(cpu) {
 		struct mvneta_pcpu_port *port = per_cpu_ptr(pp->ports, cpu);
 
 		napi_disable(&port->napi);
@@ -3055,13 +3055,11 @@ err_cleanup_rxqs:
 static int mvneta_stop(struct net_device *dev)
 {
 	struct mvneta_port *pp = netdev_priv(dev);
-	int cpu;
 
 	mvneta_stop_dev(pp);
 	mvneta_mdio_remove(pp);
 	unregister_cpu_notifier(&pp->cpu_notifier);
-	for_each_present_cpu(cpu)
-		smp_call_function_single(cpu, mvneta_percpu_disable, pp, true);
+	on_each_cpu(mvneta_percpu_disable, pp, true);
 	free_percpu_irq(dev->irq, pp->ports);
 	mvneta_cleanup_rxqs(pp);
 	mvneta_cleanup_txqs(pp);
