From 58d35c928d3fad63627f4bd84126746a08e6ff6c Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 26 Apr 2016 12:39:45 -0700
Subject: [PATCH 348/423] clk: bcm2835: Skip PLLC clocks when deciding on a new
 clock parent

If the firmware had set up a clock to source from PLLC, go along with
it.  But if we're looking for a new parent, we don't want to switch it
to PLLC because the firmware will force PLLC (and thus the AXI bus
clock) to different frequencies during over-temp/under-voltage,
without notification to Linux.

On my system, this moves the Linux-enabled HDMI state machine and DSI1
escape clock over to plld_per from pllc_per.  EMMC still ends up on
pllc_per, because the firmware had set it up to use that.

Signed-off-by: Eric Anholt <eric@anholt.net>
Fixes: 41691b8862e2 ("clk: bcm2835: Add support for programming the audio domain clocks")
---
 drivers/clk/bcm/clk-bcm2835.c | 23 +++++++++++++++++++++++
 1 file changed, 23 insertions(+)

--- a/drivers/clk/bcm/clk-bcm2835.c
+++ b/drivers/clk/bcm/clk-bcm2835.c
@@ -1020,16 +1020,28 @@ static int bcm2835_clock_set_rate(struct
 	return 0;
 }
 
+static bool
+bcm2835_clk_is_pllc(struct clk_hw *hw)
+{
+	if (!hw)
+		return false;
+
+	return strncmp(clk_hw_get_name(hw), "pllc", 4) == 0;
+}
+
 static int bcm2835_clock_determine_rate(struct clk_hw *hw,
 					struct clk_rate_request *req)
 {
 	struct bcm2835_clock *clock = bcm2835_clock_from_hw(hw);
 	struct clk_hw *parent, *best_parent = NULL;
+	bool current_parent_is_pllc;
 	unsigned long rate, best_rate = 0;
 	unsigned long prate, best_prate = 0;
 	size_t i;
 	u32 div;
 
+	current_parent_is_pllc = bcm2835_clk_is_pllc(clk_hw_get_parent(hw));
+
 	/*
 	 * Select parent clock that results in the closest but lower rate
 	 */
@@ -1037,6 +1049,17 @@ static int bcm2835_clock_determine_rate(
 		parent = clk_hw_get_parent_by_index(hw, i);
 		if (!parent)
 			continue;
+
+		/*
+		 * Don't choose a PLLC-derived clock as our parent
+		 * unless it had been manually set that way.  PLLC's
+		 * frequency gets adjusted by the firmware due to
+		 * over-temp or under-voltage conditions, without
+		 * prior notification to our clock consumer.
+		 */
+		if (bcm2835_clk_is_pllc(parent) && !current_parent_is_pllc)
+			continue;
+
 		prate = clk_hw_get_rate(parent);
 		div = bcm2835_clock_choose_div(hw, req->rate, prate, true);
 		rate = bcm2835_clock_rate_from_divisor(clock, prate, div);
