From ec66f897c2625ff0764c64229b4756b0b6f88a03 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 27 Feb 2015 15:10:24 +0000
Subject: [PATCH 074/423] enc28j60: Add device tree compatible string and an
 overlay

---
 drivers/net/ethernet/microchip/enc28j60.c | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/drivers/net/ethernet/microchip/enc28j60.c
+++ b/drivers/net/ethernet/microchip/enc28j60.c
@@ -1630,9 +1630,16 @@ static int enc28j60_remove(struct spi_de
 	return 0;
 }
 
+static const struct of_device_id enc28j60_of_match[] = {
+	{ .compatible = "microchip,enc28j60", },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, enc28j60_of_match);
+
 static struct spi_driver enc28j60_driver = {
 	.driver = {
 		   .name = DRV_NAME,
+		   .of_match_table = enc28j60_of_match,
 	 },
 	.probe = enc28j60_probe,
 	.remove = enc28j60_remove,
