From 5780349e26ba486276936393f666bea55c5dbf1e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Noralf=20Tr=C3=B8nnes?= <noralf@tronnes.org>
Date: Sat, 3 Oct 2015 15:58:59 +0200
Subject: [PATCH 021/423] dmaengine: bcm2835: set residue_granularity field
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

bcm2835-dma supports residue reporting at burst level but didn't report
this via the residue_granularity field.

Without this field set properly we get playback issues with I2S cards.

[by HiassofT, taken from bcm2708-dmaengine]
Signed-off-by: Noralf Trønnes <noralf@tronnes.org>
---
 drivers/dma/bcm2835-dma.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/dma/bcm2835-dma.c
+++ b/drivers/dma/bcm2835-dma.c
@@ -802,6 +802,7 @@ static int bcm2835_dma_probe(struct plat
 	od->ddev.src_addr_widths = BIT(DMA_SLAVE_BUSWIDTH_4_BYTES);
 	od->ddev.dst_addr_widths = BIT(DMA_SLAVE_BUSWIDTH_4_BYTES);
 	od->ddev.directions = BIT(DMA_DEV_TO_MEM) | BIT(DMA_MEM_TO_DEV);
+	od->ddev.residue_granularity = DMA_RESIDUE_GRANULARITY_BURST;
 	od->ddev.dev = &pdev->dev;
 	INIT_LIST_HEAD(&od->ddev.channels);
 	spin_lock_init(&od->lock);
