From 62f0d8320a176602d37c51fad03cafc736441ad4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 23 Jun 2016 16:37:46 +0100
Subject: [PATCH 414/423] mmc: Apply ERASE_BROKEN quirks correctly

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/mmc/card/block.c | 9 +++------
 1 file changed, 3 insertions(+), 6 deletions(-)

--- a/drivers/mmc/card/block.c
+++ b/drivers/mmc/card/block.c
@@ -2563,12 +2563,9 @@ static const struct mmc_fixup blk_fixups
 	 *  On some Kingston SD cards, multiple erases of less than 64
 	 *  sectors can cause corruption.
 	 */
-	MMC_FIXUP("SD16G", 0x41, 0x3432, add_quirk_mmc,
-		  MMC_QUIRK_ERASE_BROKEN),
-	MMC_FIXUP("SD32G", 0x41, 0x3432, add_quirk_mmc,
-		  MMC_QUIRK_ERASE_BROKEN),
-	MMC_FIXUP("SD64G", 0x41, 0x3432, add_quirk_mmc,
-		  MMC_QUIRK_ERASE_BROKEN),
+	MMC_FIXUP("SD16G", 0x41, 0x3432, add_quirk, MMC_QUIRK_ERASE_BROKEN),
+	MMC_FIXUP("SD32G", 0x41, 0x3432, add_quirk, MMC_QUIRK_ERASE_BROKEN),
+	MMC_FIXUP("SD64G", 0x41, 0x3432, add_quirk, MMC_QUIRK_ERASE_BROKEN),
 
 	END_FIXUP
 };
