From 3793554fcc4a8aa0545f109b5e8413c3ba42b823 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Mon, 15 Feb 2016 17:06:02 -0800
Subject: [PATCH 287/423] drm/vc4: Fix the name of the VSYNCD_EVEN register.

It's used for delaying vsync in interlaced mode.

Signed-off-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit c31806fbdda910d337b60896040afa708bdfa2bd)
---
 drivers/gpu/drm/vc4/vc4_crtc.c | 2 +-
 drivers/gpu/drm/vc4/vc4_regs.h | 2 +-
 2 files changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_crtc.c
+++ b/drivers/gpu/drm/vc4/vc4_crtc.c
@@ -88,7 +88,7 @@ static const struct {
 } crtc_regs[] = {
 	CRTC_REG(PV_CONTROL),
 	CRTC_REG(PV_V_CONTROL),
-	CRTC_REG(PV_VSYNCD),
+	CRTC_REG(PV_VSYNCD_EVEN),
 	CRTC_REG(PV_HORZA),
 	CRTC_REG(PV_HORZB),
 	CRTC_REG(PV_VERTA),
--- a/drivers/gpu/drm/vc4/vc4_regs.h
+++ b/drivers/gpu/drm/vc4/vc4_regs.h
@@ -187,7 +187,7 @@
 # define PV_VCONTROL_CONTINUOUS			BIT(1)
 # define PV_VCONTROL_VIDEN			BIT(0)
 
-#define PV_VSYNCD				0x08
+#define PV_VSYNCD_EVEN				0x08
 
 #define PV_HORZA				0x0c
 # define PV_HORZA_HBP_MASK			VC4_MASK(31, 16)
