#!/bin/sh

. /lib/functions/uci-defaults.sh
. /lib/apm821xx.sh

board_config_update

board=$(apm821xx_board_name)

case "$board" in
mr24)
	ucidef_set_led_netdev "wan" "WAN" "mr24:green:wan" "eth0"
	ucidef_set_led_wlan "wlan1" "WLAN1" "mr24:green:wifi1" "phy0assoc"
	ucidef_set_led_wlan "wlan2" "WLAN2" "mr24:green:wifi2" "phy0assoc"
	ucidef_set_led_wlan "wlan3" "WLAN3" "mr24:green:wifi3" "phy0assoc"
	ucidef_set_led_wlan "wlan4" "WLAN4" "mr24:green:wifi4" "phy0tpt"
	;;

mbl)
	;;

wndr4700)
	ucidef_set_led_netdev "wan" "WAN (green)" "wndr4700:green:wan" "eth0.2"
	ucidef_set_led_usbdev "usb3-1" "USB3-1" "wndr4700:blue:usb" "2-1"
	ucidef_set_led_usbdev "usb3-2" "USB3-2" "wndr4700:blue:usb" "3-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "wndr4700:blue:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "wndr4700:blue:wlan" "phy1tpt"
	;;

*)
	;;
esac

board_config_flush

exit 0
