From 8a2725220ebcc2207c979e2c816a911aa20fa3f3 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 7 Mar 2016 09:53:03 +0000
Subject: [PATCH 164/423] BCM270X_DT: Add pi3-miniuart-bt DT overlay

Switch Pi3 Bluetooth function to use the mini-UART (ttyS0) and restore
UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
usable baudrate.

It is also necessary to edit /lib/systemd/system/hciuart.server and
replace ttyAMA0 with ttyS0.

If cmdline.txt uses the alias serial0 to refer to the user-accessable port
then the firmware will replace with the appropriate port whether or not
this overlay is used.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/Makefile                |  1 +
 arch/arm/boot/dts/overlays/README                  | 10 ++++
 .../boot/dts/overlays/pi3-miniuart-bt-overlay.dts  | 61 ++++++++++++++++++++++
 3 files changed, 72 insertions(+)
 create mode 100644 arch/arm/boot/dts/overlays/pi3-miniuart-bt-overlay.dts

--- a/arch/arm/boot/dts/overlays/Makefile
+++ b/arch/arm/boot/dts/overlays/Makefile
@@ -40,6 +40,7 @@ dtb-$(RPI_DT_OVERLAYS) += mcp2515-can1-o
 dtb-$(RPI_DT_OVERLAYS) += mmc-overlay.dtb
 dtb-$(RPI_DT_OVERLAYS) += mz61581-overlay.dtb
 dtb-$(RPI_DT_OVERLAYS) += pi3-disable-bt-overlay.dtb
+dtb-$(RPI_DT_OVERLAYS) += pi3-miniuart-bt-overlay.dtb
 dtb-$(RPI_DT_OVERLAYS) += piscreen-overlay.dtb
 dtb-$(RPI_DT_OVERLAYS) += piscreen2r-overlay.dtb
 dtb-$(RPI_DT_OVERLAYS) += pitft28-capacitive-overlay.dtb
--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -504,6 +504,16 @@ Load:   dtoverlay=pi3-disable-bt
 Params: <None>
 
 
+Name:   pi3-miniuart-bt
+Info:   Switch Pi3 Bluetooth function to use the mini-UART (ttyS0) and restore
+        UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
+        usable baudrate.
+        N.B. It is also necessary to edit /lib/systemd/system/hciuart.server
+        and replace ttyAMA0 with ttyS0.
+Load:   dtoverlay=pi3-miniuart-bt
+Params: <None>
+
+
 Name:   piscreen
 Info:   PiScreen display by OzzMaker.com
 Load:   dtoverlay=piscreen,<param>=<val>
--- /dev/null
+++ b/arch/arm/boot/dts/overlays/pi3-miniuart-bt-overlay.dts
@@ -0,0 +1,61 @@
+/dts-v1/;
+/plugin/;
+
+/* Switch Pi3 Bluetooth function to use the mini-UART (ttyS0) and restore
+   UART0/ttyAMA0 over GPIOs 14 & 15. Note that this may reduce the maximum
+   usable baudrate.
+
+   It is also necessary to edit /lib/systemd/system/hciuart.server and
+   replace ttyAMA0 with ttyS0.
+
+   If cmdline.txt uses the alias serial0 to refer to the user-accessable port
+   then the firmware will replace with the appropriate port whether or not
+   this overlay is used.
+*/
+
+/{
+	compatible = "brcm,bcm2708";
+
+	fragment@0 {
+		target = <&uart0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&gpio>;
+		__overlay__ {
+			uart0_pins: uart0_pins {
+				brcm,pins = <14 15>;
+				brcm,function = <4>; /* alt0 */
+				brcm,pull = <0 2>;
+			};
+
+			uart1_pins: uart1_pins {
+				brcm,pins = <32 33>;
+				brcm,function = <2>; /* alt5=UART1 */
+				brcm,pull = <0 0>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial0 = "/soc/uart@7e201000";
+			serial1 = "/soc/uart@7e215040";
+		};
+	};
+};
