From d832db5de5893d3d6020a9d3e32aa4cd80490cc9 Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Tue, 24 May 2016 16:20:09 +0100
Subject: [PATCH 364/423] bcm2835-camera: Fix max/min error when looping over
 cameras/resolutions

See: https://github.com/raspberrypi/linux/issues/1447#issuecomment-221303506
---
 drivers/media/platform/bcm2835/bcm2835-camera.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-camera.c
+++ b/drivers/media/platform/bcm2835/bcm2835-camera.c
@@ -1530,8 +1530,8 @@ static int get_num_cameras(struct vchiq_
 	}
 	for (i = 0;
 	     i < (cam_info.num_cameras > num_resolutions ?
-			cam_info.num_cameras :
-			num_resolutions);
+			num_resolutions :
+			cam_info.num_cameras);
 	     i++) {
 		resolutions[i][0] = cam_info.cameras[i].max_width;
 		resolutions[i][1] = cam_info.cameras[i].max_height;
