From 2d65549219b48c5da3bcc743477567b41017c96f Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 1 Dec 2015 16:49:12 -0800
Subject: [PATCH 264/423] ARM: bcm2835: Define two new packets from the latest
 firmware.

These packets give us direct access to the firmware's power management
code, as opposed to GET/SET_POWER_STATE packets that only had a couple
of domains implemented.

Signed-off-by: Eric Anholt <eric@anholt.net>
Reviewed-by: Kevin Hilman <khilman@linaro.org>
(cherry picked from commit 60d56333e869be6ad6926cdba3ba974512b2183b)
---
 include/soc/bcm2835/raspberrypi-firmware.h | 2 ++
 1 file changed, 2 insertions(+)

--- a/include/soc/bcm2835/raspberrypi-firmware.h
+++ b/include/soc/bcm2835/raspberrypi-firmware.h
@@ -74,11 +74,13 @@ enum rpi_firmware_property_tag {
 	RPI_FIRMWARE_GET_DISPMANX_RESOURCE_MEM_HANDLE =       0x00030014,
 	RPI_FIRMWARE_GET_EDID_BLOCK =                         0x00030020,
 	RPI_FIRMWARE_GET_CUSTOMER_OTP =                       0x00030021,
+	RPI_FIRMWARE_GET_DOMAIN_STATE =                       0x00030030,
 	RPI_FIRMWARE_SET_CLOCK_STATE =                        0x00038001,
 	RPI_FIRMWARE_SET_CLOCK_RATE =                         0x00038002,
 	RPI_FIRMWARE_SET_VOLTAGE =                            0x00038003,
 	RPI_FIRMWARE_SET_TURBO =                              0x00038009,
 	RPI_FIRMWARE_SET_CUSTOMER_OTP =                       0x00038021,
+	RPI_FIRMWARE_SET_DOMAIN_STATE =                       0x00038030,
 	RPI_FIRMWARE_SET_SDHOST_CLOCK =                       0x00038042,
 
 	/* Dispmanx TAGS */
