From bcd71e5dd7b7f9ad1a5b7b77edc3350feede7bfb Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 7 Mar 2016 13:38:39 +0000
Subject: [PATCH 165/423] Pi3 DT: Add dtparams for the SD interface

Add new base dtparams sd_overclock, sd_force_pio, sd_pio_limit
and sd_debug. These were missed out of the initial Pi3 DTB.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2710-rpi-3-b.dts | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
+++ b/arch/arm/boot/dts/bcm2710-rpi-3-b.dts
@@ -188,5 +188,9 @@
 		audio = <&audio>,"status";
 		watchdog = <&watchdog>,"status";
 		random = <&random>,"status";
+		sd_overclock = <&sdhost>,"brcm,overclock-50:0";
+		sd_force_pio = <&sdhost>,"brcm,force-pio?";
+		sd_pio_limit = <&sdhost>,"brcm,pio-limit:0";
+		sd_debug     = <&sdhost>,"brcm,debug";
 	};
 };
