/*
 * Copyright (C) 2014 Daniel Golle <daniel@makrotopia.org>
 * Copyright (C) 2013 Ma Haijun <mahaijuns@gmail.com>
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
 */

/dts-v1/;
#include "ox820.dtsi"

/ {
	model = "Pogoplug V3";

	chosen {
		bootargs = "console=ttyS0,115200n8 earlyprintk=serial";
	};

	uart@44200000 {
		status = "okay";
	};

	sata@45900000 {
		status = "okay";
	};

	nand@41000000 {
		status = "okay";

		partition@0 {
			label = "boot";
			reg = <0x00000000 0x00e00000>;
			/*read-only;*/
		};

		partition@e00000 {
			label = "ubi";
			reg = <0x00e00000 0x07200000>;
		};
	};

	ethernet@40400000 {
		status = "okay";
	};

	ehci@40200100 {
		status = "okay";
	};

	pinctrl {
		leds {
			pinctrl_leds: leds-0 {
				plxtech,pins =
					<0 2 0 0	/* MF_A2 */
					 1 16 0 0	/* MF_B16 */
					 1 17 0 0>;	/* MF_B17 */
			};
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_leds>;

		blue {
			label = "pogoplug:blue:internal";
			gpios = <&GPIOA 2 0>;
		};

		orange {
			label = "pogoplug:orange:usr";
			gpios = <&GPIOB 16 1>;
		};

		green {
			label = "pogoplug:green:usr";
			gpios = <&GPIOB 17 1>;
		};
	};

};
