From b7c2738cecfa7e32e689f9e9f51f7a0283c6e494 Mon Sep 17 00:00:00 2001
From: Vincent Sanders <vincent.sanders@collabora.co.uk>
Date: Wed, 30 Jan 2013 12:45:18 +0000
Subject: [PATCH 048/423] bcm2835: add v4l2 camera device

- Supports raw YUV capture, preview, JPEG and H264.
- Uses videobuf2 for data transfer, using dma_buf.
- Uses 3.6.10 timestamping
- Camera power based on use
- Uses immutable input mode on video encoder

Signed-off-by: Daniel Stone <daniels@collabora.com>
Signed-off-by: Luke Diamand <luked@broadcom.com>

V4L2: Fixes from 6by9

V4L2: Fix EV values. Add manual shutter speed control

V4L2 EV values should be in units of 1/1000. Corrected.
Add support for V4L2_CID_EXPOSURE_ABSOLUTE which should
give manual shutter control. Requires manual exposure mode
to be selected first.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Correct JPEG Q-factor range

Should be 1-100, not 0-100

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix issue of driver jamming if STREAMON failed.

Fix issue where the driver was left in a partially enabled
state if STREAMON failed, and would then reject many IOCTLs
as it thought it was streaming.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix ISO controls.

Driver was passing the index to the GPU, and not the desired
ISO value.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add flicker avoidance controls

Add support for V4L2_CID_POWER_LINE_FREQUENCY to set flicker
avoidance frequencies.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add support for frame rate control.

Add support for frame rate (or time per frame as V4L2
inverts it) control via s_parm.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Improve G_FBUF handling so we pass conformance

Return some sane numbers for get framebuffer so that
we pass conformance.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix information advertised through g_vidfmt

Width and height were being stored based on incorrect
values.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add support for inline H264 headers

Add support for V4L2_CID_MPEG_VIDEO_REPEAT_SEQ_HEADER
to control H264 inline headers.
Requires firmware fix to work correctly, otherwise format
has to be set to H264 before this parameter is set.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix JPEG timestamp issue

JPEG images were coming through from the GPU with timestamp
of 0. Detect this and give current system time instead
of some invalid value.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix issue when switching down JPEG resolution.

JPEG buffer size calculation is based on input resolution.
Input resolution was being configured after output port
format. Caused failures if switching from one JPEG resolution
to a smaller one.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Enable MJPEG encoding

Requires GPU firmware update to support MJPEG encoder.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Correct flag settings for compressed formats

Set flags field correctly on enum_fmt_vid_cap for compressed
image formats.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: H264 profile & level ctrls, FPS control and auto exp pri

Several control handling updates.
H264 profile and level controls.
Timeperframe/FPS reworked to add V4L2_CID_EXPOSURE_AUTO_PRIORITY to
select whether AE is allowed to override the framerate specified.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Correct BGR24 to RGB24 in format table

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add additional pixel formats. Correct colourspace

Adds the other flavours of YUYV, and NV12.
Corrects the overlay advertised colourspace.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Drop logging msg from info to debug

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Initial pass at scene modes.

Only supports exposure mode and metering modes.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add manual white balance control.

Adds support for V4L2_CID_RED_BALANCE and
V4L2_CID_BLUE_BALANCE. Only has an effect if
V4L2_CID_AUTO_N_PRESET_WHITE_BALANCE has
V4L2_WHITE_BALANCE_MANUAL selected.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

config: Enable V4L / MMAL driver

V4L2: Increase the MMAL timeout to 3sec

MJPEG codec flush is now taking longer and results
in a kernel panic if the driver has stopped waiting for
the result when it finally completes.
Increase the timeout value from 1 to 3secs.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add support for setting H264_I_PERIOD

Adds support for the parameter V4L2_CID_MPEG_VIDEO_H264_I_PERIOD
to set the frequency with which I frames are produced.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Enable GPU function for removing padding from images.

GPU can now support arbitrary strides, although may require
additional processing to achieve it. Enable this feature
so that the images delivered are the size requested.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add support for V4L2_PIX_FMT_BGR32

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Set the colourspace to avoid odd YUV-RGB conversions

Removes the amiguity from the conversion routines and stops
them dropping back to the SD vs HD choice of coeffs.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Make video/still threshold a run-time param

Move the define for at what resolution the driver
switches from a video mode capture to a stills mode
capture to module parameters.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Fix incorrect pool sizing

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add option to disable enum_framesizes.

Gstreamer's handling of a driver that advertises
V4L2_FRMSIZE_TYPE_STEPWISE to define the supported
resolutions is broken. See bug
https://bugzilla.gnome.org/show_bug.cgi?id=726521

Optional parameter of gst_v4l2src_is_broken added.
If non-zero, the driver claims not to support that
ioctl, and gstreamer should be happy again (it
guesses a set of defaults for itself).

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Add support for more image formats

Adds YVU420 (YV12), YVU420SP (NV21), and BGR888.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

V4L2: Extend range for V4L2_CID_MPEG_VIDEO_H264_I_PERIOD

Request to extend the range from the fairly arbitrary
1000 frames (33 seconds at 30fps). Extend out to the
max range supported (int32 value).
Also allow 0, which is handled by the codec as only
send an I-frame on the first frame and never again.
There may be an exception if it detects a significant
scene change, but there's no easy way around that.

Signed-off-by: Dave Stevenson <dsteve@broadcom.com>

bcm2835-camera: stop_streaming now has a void return

BCM2835-V4L2: Fix compliance test failures

VIDIOC_TRY_FMT and VIDIOC_S_FMT tests were faling due
to reporting V4L2_COLORSPACE_JPEG when the colour
format wasn't V4L2_PIX_FMT_JPEG.
Now reports V4L2_COLORSPACE_SMPTE170M for YUV formats.

bcm2835 camera planar/packed stride length

Added a field to the mmal_fmt struct used to compute the bytes per line
when using a particular format. This results in the correct stride being
calculated even when the format is planar.

Signed-off-by: Garrett Wilson <g@floft.net>

bcm2835: camera: check for scene not being found

static analysis by cppcheck detected some potential NULL pointer
dereference issues:

[drivers/media/platform/bcm2835/controls.c:854]: (error) Possible null
  pointer dereference: scene
  (and lines 858, 859 too)

it is possible that scene is not found because of an invalue ctrl->val
and is therefore NULL and hence causing a null pointer dereference.

Signed-off-by: Colin Ian King <colin.king@canonical.com>

bcm2835: memcpy port data to m rather than rmsg

static analysis by cppcheck detected a memcpy to rmsg which is
not actually initialized at that point.  The memcpy should be copying
to variable m instead.

Signed-off-by: Colin Ian King <colin.king@canonical.com>

BCM2835-V4L2: Return buffers to videobuf2 on shutdown

https://github.com/raspberrypi/linux/issues/817
Fixes the kernel warning from videobuf2 as buffers
are now returned as they are being flushed on
stop_streaming.

squash: Fixup bcm2835-camera for changes in kernel 4.4 api
---
 Documentation/video4linux/bcm2835-v4l2.txt       |   60 +
 drivers/media/platform/Kconfig                   |    2 +
 drivers/media/platform/Makefile                  |    2 +
 drivers/media/platform/bcm2835/Kconfig           |   25 +
 drivers/media/platform/bcm2835/Makefile          |    5 +
 drivers/media/platform/bcm2835/bcm2835-camera.c  | 1844 +++++++++++++++++++++
 drivers/media/platform/bcm2835/bcm2835-camera.h  |  126 ++
 drivers/media/platform/bcm2835/controls.c        | 1324 +++++++++++++++
 drivers/media/platform/bcm2835/mmal-common.h     |   53 +
 drivers/media/platform/bcm2835/mmal-encodings.h  |  127 ++
 drivers/media/platform/bcm2835/mmal-msg-common.h |   50 +
 drivers/media/platform/bcm2835/mmal-msg-format.h |   81 +
 drivers/media/platform/bcm2835/mmal-msg-port.h   |  107 ++
 drivers/media/platform/bcm2835/mmal-msg.h        |  404 +++++
 drivers/media/platform/bcm2835/mmal-parameters.h |  656 ++++++++
 drivers/media/platform/bcm2835/mmal-vchiq.c      | 1916 ++++++++++++++++++++++
 drivers/media/platform/bcm2835/mmal-vchiq.h      |  178 ++
 17 files changed, 6960 insertions(+)
 create mode 100644 Documentation/video4linux/bcm2835-v4l2.txt
 create mode 100644 drivers/media/platform/bcm2835/Kconfig
 create mode 100644 drivers/media/platform/bcm2835/Makefile
 create mode 100644 drivers/media/platform/bcm2835/bcm2835-camera.c
 create mode 100644 drivers/media/platform/bcm2835/bcm2835-camera.h
 create mode 100644 drivers/media/platform/bcm2835/controls.c
 create mode 100644 drivers/media/platform/bcm2835/mmal-common.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-encodings.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-msg-common.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-msg-format.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-msg-port.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-msg.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-parameters.h
 create mode 100644 drivers/media/platform/bcm2835/mmal-vchiq.c
 create mode 100644 drivers/media/platform/bcm2835/mmal-vchiq.h

--- /dev/null
+++ b/Documentation/video4linux/bcm2835-v4l2.txt
@@ -0,0 +1,60 @@
+
+BCM2835 (aka Raspberry Pi) V4L2 driver
+======================================
+
+1. Copyright
+============
+
+Copyright © 2013 Raspberry Pi (Trading) Ltd.
+
+2. License
+==========
+
+This program is free software; you can redistribute it and/or modify
+it under the terms of the GNU General Public License as published by
+the Free Software Foundation; either version 2 of the License, or
+(at your option) any later version.
+
+This program is distributed in the hope that it will be useful,
+but WITHOUT ANY WARRANTY; without even the implied warranty of
+MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+GNU General Public License for more details.
+
+You should have received a copy of the GNU General Public License
+along with this program; if not, write to the Free Software
+Foundation, Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+
+3. Quick Start
+==============
+
+You need a version 1.0 or later of v4l2-ctl, available from:
+	git://git.linuxtv.org/v4l-utils.git
+
+$ sudo modprobe bcm2835-v4l2
+
+Turn on the overlay:
+
+$ v4l2-ctl --overlay=1
+
+Turn off the overlay:
+
+$ v4l2-ctl --overlay=0
+
+Set the capture format for video:
+
+$ v4l2-ctl  --set-fmt-video=width=1920,height=1088,pixelformat=4
+
+(Note: 1088 not 1080).
+
+Capture:
+
+$ v4l2-ctl --stream-mmap=3 --stream-count=100 --stream-to=somefile.h264
+
+Stills capture:
+
+$ v4l2-ctl  --set-fmt-video=width=2592,height=1944,pixelformat=3
+$ v4l2-ctl --stream-mmap=3 --stream-count=1 --stream-to=somefile.jpg
+
+List of available formats:
+
+$ v4l2-ctl --list-formats
--- a/drivers/media/platform/Kconfig
+++ b/drivers/media/platform/Kconfig
@@ -11,6 +11,8 @@ menuconfig V4L_PLATFORM_DRIVERS
 
 if V4L_PLATFORM_DRIVERS
 
+source "drivers/media/platform/bcm2835/Kconfig"
+
 source "drivers/media/platform/marvell-ccic/Kconfig"
 
 config VIDEO_VIA_CAMERA
--- a/drivers/media/platform/Makefile
+++ b/drivers/media/platform/Makefile
@@ -2,6 +2,8 @@
 # Makefile for the video capture/playback device drivers.
 #
 
+obj-$(CONFIG_VIDEO_BCM2835)		+= bcm2835/
+
 obj-$(CONFIG_VIDEO_TIMBERDALE)	+= timblogiw.o
 obj-$(CONFIG_VIDEO_M32R_AR_M64278) += arv.o
 
--- /dev/null
+++ b/drivers/media/platform/bcm2835/Kconfig
@@ -0,0 +1,25 @@
+# Broadcom VideoCore IV v4l2 camera support
+
+config VIDEO_BCM2835
+	bool "Broadcom BCM2835 camera interface driver"
+	depends on VIDEO_V4L2 && (ARCH_BCM2708 || ARCH_BCM2709 || ARCH_BCM2835)
+	---help---
+	  Say Y here to enable camera host interface devices for
+	  Broadcom BCM2835 SoC. This operates over the VCHIQ interface
+	  to a service running on VideoCore.
+
+
+if VIDEO_BCM2835
+
+config VIDEO_BCM2835_MMAL
+	tristate "Broadcom BM2835 MMAL camera interface driver"
+	depends on BCM2708_VCHIQ
+	select VIDEOBUF2_VMALLOC
+	---help---
+	  This is a V4L2 driver for the Broadcom BCM2835 MMAL camera host interface
+
+	  To compile this driver as a module, choose M here: the
+	  module will be called bcm2835-v4l2.o
+
+
+endif # VIDEO_BM2835
--- /dev/null
+++ b/drivers/media/platform/bcm2835/Makefile
@@ -0,0 +1,5 @@
+bcm2835-v4l2-objs := bcm2835-camera.o controls.o mmal-vchiq.o
+
+obj-$(CONFIG_VIDEO_BCM2835_MMAL) += bcm2835-v4l2.o
+
+ccflags-$(CONFIG_VIDEO_BCM2835) += -Idrivers/misc/vc04_services -Idrivers/misc/vc04_services/interface/vcos/linuxkernel -D__VCCOREVER__=0x04000000
--- /dev/null
+++ b/drivers/media/platform/bcm2835/bcm2835-camera.c
@@ -0,0 +1,1844 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+#include <linux/errno.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/slab.h>
+#include <media/videobuf2-vmalloc.h>
+#include <media/videobuf2-dma-contig.h>
+#include <media/v4l2-device.h>
+#include <media/v4l2-ioctl.h>
+#include <media/v4l2-ctrls.h>
+#include <media/v4l2-fh.h>
+#include <media/v4l2-event.h>
+#include <media/v4l2-common.h>
+#include <linux/delay.h>
+
+#include "mmal-common.h"
+#include "mmal-encodings.h"
+#include "mmal-vchiq.h"
+#include "mmal-msg.h"
+#include "mmal-parameters.h"
+#include "bcm2835-camera.h"
+
+#define BM2835_MMAL_VERSION "0.0.2"
+#define BM2835_MMAL_MODULE_NAME "bcm2835-v4l2"
+#define MIN_WIDTH 16
+#define MIN_HEIGHT 16
+#define MAX_WIDTH 2592
+#define MAX_HEIGHT 1944
+#define MIN_BUFFER_SIZE (80*1024)
+
+#define MAX_VIDEO_MODE_WIDTH 1280
+#define MAX_VIDEO_MODE_HEIGHT 720
+
+MODULE_DESCRIPTION("Broadcom 2835 MMAL video capture");
+MODULE_AUTHOR("Vincent Sanders");
+MODULE_LICENSE("GPL");
+MODULE_VERSION(BM2835_MMAL_VERSION);
+
+int bcm2835_v4l2_debug;
+module_param_named(debug, bcm2835_v4l2_debug, int, 0644);
+MODULE_PARM_DESC(bcm2835_v4l2_debug, "Debug level 0-2");
+
+int max_video_width = MAX_VIDEO_MODE_WIDTH;
+int max_video_height = MAX_VIDEO_MODE_HEIGHT;
+module_param(max_video_width, int, S_IRUSR | S_IWUSR | S_IRGRP | S_IROTH);
+MODULE_PARM_DESC(max_video_width, "Threshold for video mode");
+module_param(max_video_height, int, S_IRUSR | S_IWUSR | S_IRGRP | S_IROTH);
+MODULE_PARM_DESC(max_video_height, "Threshold for video mode");
+
+/* Gstreamer bug https://bugzilla.gnome.org/show_bug.cgi?id=726521
+ * v4l2src does bad (and actually wrong) things when the vidioc_enum_framesizes
+ * function says type V4L2_FRMSIZE_TYPE_STEPWISE, which we do by default.
+ * It's happier if we just don't say anything at all, when it then
+ * sets up a load of defaults that it thinks might work.
+ * If gst_v4l2src_is_broken is non-zero, then we remove the function from
+ * our function table list (actually switch to an alternate set, but same
+ * result).
+ */
+int gst_v4l2src_is_broken = 0;
+module_param(gst_v4l2src_is_broken, int, S_IRUSR | S_IWUSR | S_IRGRP | S_IROTH);
+MODULE_PARM_DESC(gst_v4l2src_is_broken, "If non-zero, enable workaround for Gstreamer");
+
+static struct bm2835_mmal_dev *gdev;	/* global device data */
+
+#define FPS_MIN 1
+#define FPS_MAX 90
+
+/* timeperframe: min/max and default */
+static const struct v4l2_fract
+	tpf_min     = {.numerator = 1,		.denominator = FPS_MAX},
+	tpf_max     = {.numerator = 1,	        .denominator = FPS_MIN},
+	tpf_default = {.numerator = 1000,	.denominator = 30000};
+
+/* video formats */
+static struct mmal_fmt formats[] = {
+	{
+	 .name = "4:2:0, planar, YUV",
+	 .fourcc = V4L2_PIX_FMT_YUV420,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_I420,
+	 .depth = 12,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 1,
+	 },
+	{
+	 .name = "4:2:2, packed, YUYV",
+	 .fourcc = V4L2_PIX_FMT_YUYV,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_YUYV,
+	 .depth = 16,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 2,
+	 },
+	{
+	 .name = "RGB24 (LE)",
+	 .fourcc = V4L2_PIX_FMT_RGB24,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_BGR24,
+	 .depth = 24,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 3,
+	 },
+	{
+	 .name = "JPEG",
+	 .fourcc = V4L2_PIX_FMT_JPEG,
+	 .flags = V4L2_FMT_FLAG_COMPRESSED,
+	 .mmal = MMAL_ENCODING_JPEG,
+	 .depth = 8,
+	 .mmal_component = MMAL_COMPONENT_IMAGE_ENCODE,
+	 .ybbp = 0,
+	 },
+	{
+	 .name = "H264",
+	 .fourcc = V4L2_PIX_FMT_H264,
+	 .flags = V4L2_FMT_FLAG_COMPRESSED,
+	 .mmal = MMAL_ENCODING_H264,
+	 .depth = 8,
+	 .mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
+	 .ybbp = 0,
+	 },
+	{
+	 .name = "MJPEG",
+	 .fourcc = V4L2_PIX_FMT_MJPEG,
+	 .flags = V4L2_FMT_FLAG_COMPRESSED,
+	 .mmal = MMAL_ENCODING_MJPEG,
+	 .depth = 8,
+	 .mmal_component = MMAL_COMPONENT_VIDEO_ENCODE,
+	 .ybbp = 0,
+	 },
+	{
+	 .name = "4:2:2, packed, YVYU",
+	 .fourcc = V4L2_PIX_FMT_YVYU,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_YVYU,
+	 .depth = 16,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 2,
+	 },
+	{
+	 .name = "4:2:2, packed, VYUY",
+	 .fourcc = V4L2_PIX_FMT_VYUY,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_VYUY,
+	 .depth = 16,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 2,
+	 },
+	{
+	 .name = "4:2:2, packed, UYVY",
+	 .fourcc = V4L2_PIX_FMT_UYVY,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_UYVY,
+	 .depth = 16,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 2,
+	 },
+	{
+	 .name = "4:2:0, planar, NV12",
+	 .fourcc = V4L2_PIX_FMT_NV12,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_NV12,
+	 .depth = 12,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 1,
+	 },
+	{
+	 .name = "RGB24 (BE)",
+	 .fourcc = V4L2_PIX_FMT_BGR24,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_RGB24,
+	 .depth = 24,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 3,
+	 },
+	{
+	 .name = "4:2:0, planar, YVU",
+	 .fourcc = V4L2_PIX_FMT_YVU420,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_YV12,
+	 .depth = 12,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 1,
+	 },
+	{
+	 .name = "4:2:0, planar, NV21",
+	 .fourcc = V4L2_PIX_FMT_NV21,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_NV21,
+	 .depth = 12,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 1,
+	 },
+	{
+	 .name = "RGB32 (BE)",
+	 .fourcc = V4L2_PIX_FMT_BGR32,
+	 .flags = 0,
+	 .mmal = MMAL_ENCODING_BGRA,
+	 .depth = 32,
+	 .mmal_component = MMAL_COMPONENT_CAMERA,
+	 .ybbp = 4,
+	 },
+};
+
+static struct mmal_fmt *get_format(struct v4l2_format *f)
+{
+	struct mmal_fmt *fmt;
+	unsigned int k;
+
+	for (k = 0; k < ARRAY_SIZE(formats); k++) {
+		fmt = &formats[k];
+		if (fmt->fourcc == f->fmt.pix.pixelformat)
+			break;
+	}
+
+	if (k == ARRAY_SIZE(formats))
+		return NULL;
+
+	return &formats[k];
+}
+
+/* ------------------------------------------------------------------
+	Videobuf queue operations
+   ------------------------------------------------------------------*/
+
+static int queue_setup(struct vb2_queue *vq, const void *parg,
+		       unsigned int *nbuffers, unsigned int *nplanes,
+		       unsigned int sizes[], void *alloc_ctxs[])
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vq);
+	unsigned long size;
+
+	/* refuse queue setup if port is not configured */
+	if (dev->capture.port == NULL) {
+		v4l2_err(&dev->v4l2_dev,
+			 "%s: capture port not configured\n", __func__);
+		return -EINVAL;
+	}
+
+	size = dev->capture.port->current_buffer.size;
+	if (size == 0) {
+		v4l2_err(&dev->v4l2_dev,
+			 "%s: capture port buffer size is zero\n", __func__);
+		return -EINVAL;
+	}
+
+	if (*nbuffers < (dev->capture.port->current_buffer.num + 2))
+		*nbuffers = (dev->capture.port->current_buffer.num + 2);
+
+	*nplanes = 1;
+
+	sizes[0] = size;
+
+	/*
+	 * videobuf2-vmalloc allocator is context-less so no need to set
+	 * alloc_ctxs array.
+	 */
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "%s: dev:%p\n",
+		 __func__, dev);
+
+	return 0;
+}
+
+static int buffer_prepare(struct vb2_buffer *vb)
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vb->vb2_queue);
+	unsigned long size;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "%s: dev:%p\n",
+		 __func__, dev);
+
+	BUG_ON(dev->capture.port == NULL);
+	BUG_ON(dev->capture.fmt == NULL);
+
+	size = dev->capture.stride * dev->capture.height;
+	if (vb2_plane_size(vb, 0) < size) {
+		v4l2_err(&dev->v4l2_dev,
+			 "%s data will not fit into plane (%lu < %lu)\n",
+			 __func__, vb2_plane_size(vb, 0), size);
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static inline bool is_capturing(struct bm2835_mmal_dev *dev)
+{
+	return dev->capture.camera_port ==
+	    &dev->
+	    component[MMAL_COMPONENT_CAMERA]->output[MMAL_CAMERA_PORT_CAPTURE];
+}
+
+static void buffer_cb(struct vchiq_mmal_instance *instance,
+		      struct vchiq_mmal_port *port,
+		      int status,
+		      struct mmal_buffer *buf,
+		      unsigned long length, u32 mmal_flags, s64 dts, s64 pts)
+{
+	struct bm2835_mmal_dev *dev = port->cb_ctx;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "%s: status:%d, buf:%p, length:%lu, flags %u, pts %lld\n",
+		 __func__, status, buf, length, mmal_flags, pts);
+
+	if (status != 0) {
+		/* error in transfer */
+		if (buf != NULL) {
+			/* there was a buffer with the error so return it */
+			vb2_buffer_done(&buf->vb.vb2_buf, VB2_BUF_STATE_ERROR);
+		}
+		return;
+	} else if (length == 0) {
+		/* stream ended */
+		if (buf != NULL) {
+			/* this should only ever happen if the port is
+			 * disabled and there are buffers still queued
+			 */
+			vb2_buffer_done(&buf->vb.vb2_buf, VB2_BUF_STATE_ERROR);
+			pr_debug("Empty buffer");
+		} else if (dev->capture.frame_count) {
+			/* grab another frame */
+			if (is_capturing(dev)) {
+				pr_debug("Grab another frame");
+				vchiq_mmal_port_parameter_set(
+					instance,
+					dev->capture.
+					camera_port,
+					MMAL_PARAMETER_CAPTURE,
+					&dev->capture.
+					frame_count,
+					sizeof(dev->capture.frame_count));
+			}
+		} else {
+			/* signal frame completion */
+			complete(&dev->capture.frame_cmplt);
+		}
+	} else {
+		if (dev->capture.frame_count) {
+			if (dev->capture.vc_start_timestamp != -1 &&
+			    pts != 0) {
+				s64 runtime_us = pts -
+				    dev->capture.vc_start_timestamp;
+				u32 div = 0;
+				u32 rem = 0;
+
+				div =
+				    div_u64_rem(runtime_us, USEC_PER_SEC, &rem);
+				buf->vb.timestamp.tv_sec =
+				    dev->capture.kernel_start_ts.tv_sec - 1 +
+				    div;
+				buf->vb.timestamp.tv_usec =
+				    dev->capture.kernel_start_ts.tv_usec + rem;
+
+				if (buf->vb.timestamp.tv_usec >=
+				    USEC_PER_SEC) {
+					buf->vb.timestamp.tv_sec++;
+					buf->vb.timestamp.tv_usec -=
+					    USEC_PER_SEC;
+				}
+				v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+					 "Convert start time %d.%06d and %llu "
+					 "with offset %llu to %d.%06d\n",
+					 (int)dev->capture.kernel_start_ts.
+					 tv_sec,
+					 (int)dev->capture.kernel_start_ts.
+					 tv_usec,
+					 dev->capture.vc_start_timestamp, pts,
+					 (int)buf->vb.timestamp.tv_sec,
+					 (int)buf->vb.timestamp.
+					 tv_usec);
+			} else {
+				v4l2_get_timestamp(&buf->vb.timestamp);
+			}
+
+			vb2_set_plane_payload(&buf->vb.vb2_buf, 0, length);
+			vb2_buffer_done(&buf->vb.vb2_buf, VB2_BUF_STATE_DONE);
+
+			if (mmal_flags & MMAL_BUFFER_HEADER_FLAG_EOS &&
+			    is_capturing(dev)) {
+				v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+					 "Grab another frame as buffer has EOS");
+				vchiq_mmal_port_parameter_set(
+					instance,
+					dev->capture.
+					camera_port,
+					MMAL_PARAMETER_CAPTURE,
+					&dev->capture.
+					frame_count,
+					sizeof(dev->capture.frame_count));
+			}
+		} else {
+			/* signal frame completion */
+			vb2_buffer_done(&buf->vb.vb2_buf, VB2_BUF_STATE_ERROR);
+			complete(&dev->capture.frame_cmplt);
+		}
+	}
+}
+
+static int enable_camera(struct bm2835_mmal_dev *dev)
+{
+	int ret;
+	if (!dev->camera_use_count) {
+		ret = vchiq_mmal_component_enable(
+				dev->instance,
+				dev->component[MMAL_COMPONENT_CAMERA]);
+		if (ret < 0) {
+			v4l2_err(&dev->v4l2_dev,
+				 "Failed enabling camera, ret %d\n", ret);
+			return -EINVAL;
+		}
+	}
+	dev->camera_use_count++;
+	v4l2_dbg(1, bcm2835_v4l2_debug,
+		 &dev->v4l2_dev, "enabled camera (refcount %d)\n",
+			dev->camera_use_count);
+	return 0;
+}
+
+static int disable_camera(struct bm2835_mmal_dev *dev)
+{
+	int ret;
+	if (!dev->camera_use_count) {
+		v4l2_err(&dev->v4l2_dev,
+			 "Disabled the camera when already disabled\n");
+		return -EINVAL;
+	}
+	dev->camera_use_count--;
+	if (!dev->camera_use_count) {
+		unsigned int i = 0xFFFFFFFF;
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "Disabling camera\n");
+		ret =
+		    vchiq_mmal_component_disable(
+				dev->instance,
+				dev->component[MMAL_COMPONENT_CAMERA]);
+		if (ret < 0) {
+			v4l2_err(&dev->v4l2_dev,
+				 "Failed disabling camera, ret %d\n", ret);
+			return -EINVAL;
+		}
+		vchiq_mmal_port_parameter_set(
+			dev->instance,
+			&dev->component[MMAL_COMPONENT_CAMERA]->control,
+			MMAL_PARAMETER_CAMERA_NUM, &i,
+			sizeof(i));
+	}
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "Camera refcount now %d\n", dev->camera_use_count);
+	return 0;
+}
+
+static void buffer_queue(struct vb2_buffer *vb)
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vb->vb2_queue);
+	struct vb2_v4l2_buffer *vb2 = to_vb2_v4l2_buffer(vb);
+	struct mmal_buffer *buf = container_of(vb2, struct mmal_buffer, vb);
+	int ret;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "%s: dev:%p buf:%p\n", __func__, dev, buf);
+
+	buf->buffer = vb2_plane_vaddr(&buf->vb.vb2_buf, 0);
+	buf->buffer_size = vb2_plane_size(&buf->vb.vb2_buf, 0);
+
+	ret = vchiq_mmal_submit_buffer(dev->instance, dev->capture.port, buf);
+	if (ret < 0)
+		v4l2_err(&dev->v4l2_dev, "%s: error submitting buffer\n",
+			 __func__);
+}
+
+static int start_streaming(struct vb2_queue *vq, unsigned int count)
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vq);
+	int ret;
+	int parameter_size;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "%s: dev:%p\n",
+		 __func__, dev);
+
+	/* ensure a format has actually been set */
+	if (dev->capture.port == NULL)
+		return -EINVAL;
+
+	if (enable_camera(dev) < 0) {
+		v4l2_err(&dev->v4l2_dev, "Failed to enable camera\n");
+		return -EINVAL;
+	}
+
+	/*init_completion(&dev->capture.frame_cmplt); */
+
+	/* enable frame capture */
+	dev->capture.frame_count = 1;
+
+	/* if the preview is not already running, wait for a few frames for AGC
+	 * to settle down.
+	 */
+	if (!dev->component[MMAL_COMPONENT_PREVIEW]->enabled)
+		msleep(300);
+
+	/* enable the connection from camera to encoder (if applicable) */
+	if (dev->capture.camera_port != dev->capture.port
+	    && dev->capture.camera_port) {
+		ret = vchiq_mmal_port_enable(dev->instance,
+					     dev->capture.camera_port, NULL);
+		if (ret) {
+			v4l2_err(&dev->v4l2_dev,
+				 "Failed to enable encode tunnel - error %d\n",
+				 ret);
+			return -1;
+		}
+	}
+
+	/* Get VC timestamp at this point in time */
+	parameter_size = sizeof(dev->capture.vc_start_timestamp);
+	if (vchiq_mmal_port_parameter_get(dev->instance,
+					  dev->capture.camera_port,
+					  MMAL_PARAMETER_SYSTEM_TIME,
+					  &dev->capture.vc_start_timestamp,
+					  &parameter_size)) {
+		v4l2_err(&dev->v4l2_dev,
+			 "Failed to get VC start time - update your VC f/w\n");
+
+		/* Flag to indicate just to rely on kernel timestamps */
+		dev->capture.vc_start_timestamp = -1;
+	} else
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "Start time %lld size %d\n",
+			 dev->capture.vc_start_timestamp, parameter_size);
+
+	v4l2_get_timestamp(&dev->capture.kernel_start_ts);
+
+	/* enable the camera port */
+	dev->capture.port->cb_ctx = dev;
+	ret =
+	    vchiq_mmal_port_enable(dev->instance, dev->capture.port, buffer_cb);
+	if (ret) {
+		v4l2_err(&dev->v4l2_dev,
+			"Failed to enable capture port - error %d. "
+			"Disabling camera port again\n", ret);
+
+		vchiq_mmal_port_disable(dev->instance,
+					dev->capture.camera_port);
+		if (disable_camera(dev) < 0) {
+			v4l2_err(&dev->v4l2_dev, "Failed to disable camera\n");
+			return -EINVAL;
+		}
+		return -1;
+	}
+
+	/* capture the first frame */
+	vchiq_mmal_port_parameter_set(dev->instance,
+				      dev->capture.camera_port,
+				      MMAL_PARAMETER_CAPTURE,
+				      &dev->capture.frame_count,
+				      sizeof(dev->capture.frame_count));
+	return 0;
+}
+
+/* abort streaming and wait for last buffer */
+static void stop_streaming(struct vb2_queue *vq)
+{
+	int ret;
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vq);
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "%s: dev:%p\n",
+		 __func__, dev);
+
+	init_completion(&dev->capture.frame_cmplt);
+	dev->capture.frame_count = 0;
+
+	/* ensure a format has actually been set */
+	if (dev->capture.port == NULL) {
+		v4l2_err(&dev->v4l2_dev,
+			 "no capture port - stream not started?\n");
+		return;
+	}
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "stopping capturing\n");
+
+	/* stop capturing frames */
+	vchiq_mmal_port_parameter_set(dev->instance,
+				      dev->capture.camera_port,
+				      MMAL_PARAMETER_CAPTURE,
+				      &dev->capture.frame_count,
+				      sizeof(dev->capture.frame_count));
+
+	/* wait for last frame to complete */
+	ret = wait_for_completion_timeout(&dev->capture.frame_cmplt, HZ);
+	if (ret <= 0)
+		v4l2_err(&dev->v4l2_dev,
+			 "error %d waiting for frame completion\n", ret);
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "disabling connection\n");
+
+	/* disable the connection from camera to encoder */
+	ret = vchiq_mmal_port_disable(dev->instance, dev->capture.camera_port);
+	if (!ret && dev->capture.camera_port != dev->capture.port) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "disabling port\n");
+		ret = vchiq_mmal_port_disable(dev->instance, dev->capture.port);
+	} else if (dev->capture.camera_port != dev->capture.port) {
+		v4l2_err(&dev->v4l2_dev, "port_disable failed, error %d\n",
+			 ret);
+	}
+
+	if (disable_camera(dev) < 0)
+		v4l2_err(&dev->v4l2_dev, "Failed to disable camera\n");
+}
+
+static void bm2835_mmal_lock(struct vb2_queue *vq)
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vq);
+	mutex_lock(&dev->mutex);
+}
+
+static void bm2835_mmal_unlock(struct vb2_queue *vq)
+{
+	struct bm2835_mmal_dev *dev = vb2_get_drv_priv(vq);
+	mutex_unlock(&dev->mutex);
+}
+
+static struct vb2_ops bm2835_mmal_video_qops = {
+	.queue_setup = queue_setup,
+	.buf_prepare = buffer_prepare,
+	.buf_queue = buffer_queue,
+	.start_streaming = start_streaming,
+	.stop_streaming = stop_streaming,
+	.wait_prepare = bm2835_mmal_unlock,
+	.wait_finish = bm2835_mmal_lock,
+};
+
+/* ------------------------------------------------------------------
+	IOCTL operations
+   ------------------------------------------------------------------*/
+
+/* overlay ioctl */
+static int vidioc_enum_fmt_vid_overlay(struct file *file, void *priv,
+				       struct v4l2_fmtdesc *f)
+{
+	struct mmal_fmt *fmt;
+
+	if (f->index >= ARRAY_SIZE(formats))
+		return -EINVAL;
+
+	fmt = &formats[f->index];
+
+	strlcpy(f->description, fmt->name, sizeof(f->description));
+	f->pixelformat = fmt->fourcc;
+	f->flags = fmt->flags;
+
+	return 0;
+}
+
+static int vidioc_g_fmt_vid_overlay(struct file *file, void *priv,
+				    struct v4l2_format *f)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+
+	f->fmt.win = dev->overlay;
+
+	return 0;
+}
+
+static int vidioc_try_fmt_vid_overlay(struct file *file, void *priv,
+				      struct v4l2_format *f)
+{
+	/* Only support one format so get the current one. */
+	vidioc_g_fmt_vid_overlay(file, priv, f);
+
+	/* todo: allow the size and/or offset to be changed. */
+	return 0;
+}
+
+static int vidioc_s_fmt_vid_overlay(struct file *file, void *priv,
+				    struct v4l2_format *f)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+
+	vidioc_try_fmt_vid_overlay(file, priv, f);
+
+	dev->overlay = f->fmt.win;
+
+	/* todo: program the preview port parameters */
+	return 0;
+}
+
+static int vidioc_overlay(struct file *file, void *f, unsigned int on)
+{
+	int ret;
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	struct vchiq_mmal_port *src;
+	struct vchiq_mmal_port *dst;
+	struct mmal_parameter_displayregion prev_config = {
+		.set = MMAL_DISPLAY_SET_LAYER | MMAL_DISPLAY_SET_ALPHA |
+		    MMAL_DISPLAY_SET_DEST_RECT | MMAL_DISPLAY_SET_FULLSCREEN,
+		.layer = PREVIEW_LAYER,
+		.alpha = 255,
+		.fullscreen = 0,
+		.dest_rect = {
+			      .x = dev->overlay.w.left,
+			      .y = dev->overlay.w.top,
+			      .width = dev->overlay.w.width,
+			      .height = dev->overlay.w.height,
+			      },
+	};
+
+	if ((on && dev->component[MMAL_COMPONENT_PREVIEW]->enabled) ||
+	    (!on && !dev->component[MMAL_COMPONENT_PREVIEW]->enabled))
+		return 0;	/* already in requested state */
+
+	src =
+	    &dev->component[MMAL_COMPONENT_CAMERA]->
+	    output[MMAL_CAMERA_PORT_PREVIEW];
+
+	if (!on) {
+		/* disconnect preview ports and disable component */
+		ret = vchiq_mmal_port_disable(dev->instance, src);
+		if (!ret)
+			ret =
+			    vchiq_mmal_port_connect_tunnel(dev->instance, src,
+							   NULL);
+		if (ret >= 0)
+			ret = vchiq_mmal_component_disable(
+					dev->instance,
+					dev->component[MMAL_COMPONENT_PREVIEW]);
+
+		disable_camera(dev);
+		return ret;
+	}
+
+	/* set preview port format and connect it to output */
+	dst = &dev->component[MMAL_COMPONENT_PREVIEW]->input[0];
+
+	ret = vchiq_mmal_port_set_format(dev->instance, src);
+	if (ret < 0)
+		goto error;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, dst,
+					    MMAL_PARAMETER_DISPLAYREGION,
+					    &prev_config, sizeof(prev_config));
+	if (ret < 0)
+		goto error;
+
+	if (enable_camera(dev) < 0)
+		goto error;
+
+	ret = vchiq_mmal_component_enable(
+			dev->instance,
+			dev->component[MMAL_COMPONENT_PREVIEW]);
+	if (ret < 0)
+		goto error;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev, "connecting %p to %p\n",
+		 src, dst);
+	ret = vchiq_mmal_port_connect_tunnel(dev->instance, src, dst);
+	if (!ret)
+		ret = vchiq_mmal_port_enable(dev->instance, src, NULL);
+error:
+	return ret;
+}
+
+static int vidioc_g_fbuf(struct file *file, void *fh,
+			 struct v4l2_framebuffer *a)
+{
+	/* The video overlay must stay within the framebuffer and can't be
+	   positioned independently. */
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	struct vchiq_mmal_port *preview_port =
+		    &dev->component[MMAL_COMPONENT_CAMERA]->
+		    output[MMAL_CAMERA_PORT_PREVIEW];
+	a->flags = V4L2_FBUF_FLAG_OVERLAY;
+	a->fmt.width = preview_port->es.video.width;
+	a->fmt.height = preview_port->es.video.height;
+	a->fmt.pixelformat = V4L2_PIX_FMT_YUV420;
+	a->fmt.bytesperline = preview_port->es.video.width;
+	a->fmt.sizeimage = (preview_port->es.video.width *
+			       preview_port->es.video.height * 3)>>1;
+	a->fmt.colorspace = V4L2_COLORSPACE_SMPTE170M;
+
+	return 0;
+}
+
+/* input ioctls */
+static int vidioc_enum_input(struct file *file, void *priv,
+			     struct v4l2_input *inp)
+{
+	/* only a single camera input */
+	if (inp->index != 0)
+		return -EINVAL;
+
+	inp->type = V4L2_INPUT_TYPE_CAMERA;
+	sprintf(inp->name, "Camera %u", inp->index);
+	return 0;
+}
+
+static int vidioc_g_input(struct file *file, void *priv, unsigned int *i)
+{
+	*i = 0;
+	return 0;
+}
+
+static int vidioc_s_input(struct file *file, void *priv, unsigned int i)
+{
+	if (i != 0)
+		return -EINVAL;
+
+	return 0;
+}
+
+/* capture ioctls */
+static int vidioc_querycap(struct file *file, void *priv,
+			   struct v4l2_capability *cap)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	u32 major;
+	u32 minor;
+
+	vchiq_mmal_version(dev->instance, &major, &minor);
+
+	strcpy(cap->driver, "bm2835 mmal");
+	snprintf(cap->card, sizeof(cap->card), "mmal service %d.%d",
+		 major, minor);
+
+	snprintf(cap->bus_info, sizeof(cap->bus_info),
+		 "platform:%s", dev->v4l2_dev.name);
+	cap->device_caps = V4L2_CAP_VIDEO_CAPTURE | V4L2_CAP_VIDEO_OVERLAY |
+	    V4L2_CAP_STREAMING | V4L2_CAP_READWRITE;
+	cap->capabilities = cap->device_caps | V4L2_CAP_DEVICE_CAPS;
+
+	return 0;
+}
+
+static int vidioc_enum_fmt_vid_cap(struct file *file, void *priv,
+				   struct v4l2_fmtdesc *f)
+{
+	struct mmal_fmt *fmt;
+
+	if (f->index >= ARRAY_SIZE(formats))
+		return -EINVAL;
+
+	fmt = &formats[f->index];
+
+	strlcpy(f->description, fmt->name, sizeof(f->description));
+	f->pixelformat = fmt->fourcc;
+	f->flags = fmt->flags;
+
+	return 0;
+}
+
+static int vidioc_g_fmt_vid_cap(struct file *file, void *priv,
+				struct v4l2_format *f)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+
+	f->fmt.pix.width = dev->capture.width;
+	f->fmt.pix.height = dev->capture.height;
+	f->fmt.pix.field = V4L2_FIELD_NONE;
+	f->fmt.pix.pixelformat = dev->capture.fmt->fourcc;
+	f->fmt.pix.bytesperline = dev->capture.stride;
+	f->fmt.pix.sizeimage = dev->capture.buffersize;
+
+	if (dev->capture.fmt->fourcc == V4L2_PIX_FMT_RGB24)
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_SRGB;
+	else if (dev->capture.fmt->fourcc == V4L2_PIX_FMT_JPEG)
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_JPEG;
+	else
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_SMPTE170M;
+	f->fmt.pix.priv = 0;
+
+	v4l2_dump_pix_format(1, bcm2835_v4l2_debug, &dev->v4l2_dev, &f->fmt.pix,
+			     __func__);
+	return 0;
+}
+
+static int vidioc_try_fmt_vid_cap(struct file *file, void *priv,
+				  struct v4l2_format *f)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	struct mmal_fmt *mfmt;
+
+	mfmt = get_format(f);
+	if (!mfmt) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "Fourcc format (0x%08x) unknown.\n",
+			 f->fmt.pix.pixelformat);
+		f->fmt.pix.pixelformat = formats[0].fourcc;
+		mfmt = get_format(f);
+	}
+
+	f->fmt.pix.field = V4L2_FIELD_NONE;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		"Clipping/aligning %dx%d format %08X\n",
+		f->fmt.pix.width, f->fmt.pix.height, f->fmt.pix.pixelformat);
+
+	v4l_bound_align_image(&f->fmt.pix.width, MIN_WIDTH, MAX_WIDTH, 1,
+			      &f->fmt.pix.height, MIN_HEIGHT, MAX_HEIGHT, 1, 0);
+	f->fmt.pix.bytesperline = f->fmt.pix.width * mfmt->ybbp;
+
+	/* Image buffer has to be padded to allow for alignment, even though
+	 * we then remove that padding before delivering the buffer.
+	 */
+	f->fmt.pix.sizeimage = ((f->fmt.pix.height+15)&~15) *
+			(((f->fmt.pix.width+31)&~31) * mfmt->depth) >> 3;
+
+	if ((mfmt->flags & V4L2_FMT_FLAG_COMPRESSED) &&
+	    f->fmt.pix.sizeimage < MIN_BUFFER_SIZE)
+		f->fmt.pix.sizeimage = MIN_BUFFER_SIZE;
+
+	if (f->fmt.pix.pixelformat == V4L2_PIX_FMT_RGB24)
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_SRGB;
+	else if (f->fmt.pix.pixelformat == V4L2_PIX_FMT_JPEG)
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_JPEG;
+	else
+		f->fmt.pix.colorspace = V4L2_COLORSPACE_SMPTE170M;
+	f->fmt.pix.priv = 0;
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		"Now %dx%d format %08X\n",
+		f->fmt.pix.width, f->fmt.pix.height, f->fmt.pix.pixelformat);
+
+	v4l2_dump_pix_format(1, bcm2835_v4l2_debug, &dev->v4l2_dev, &f->fmt.pix,
+			     __func__);
+	return 0;
+}
+
+static int mmal_setup_components(struct bm2835_mmal_dev *dev,
+				 struct v4l2_format *f)
+{
+	int ret;
+	struct vchiq_mmal_port *port = NULL, *camera_port = NULL;
+	struct vchiq_mmal_component *encode_component = NULL;
+	struct mmal_fmt *mfmt = get_format(f);
+
+	BUG_ON(!mfmt);
+
+	if (dev->capture.encode_component) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "vid_cap - disconnect previous tunnel\n");
+
+		/* Disconnect any previous connection */
+		vchiq_mmal_port_connect_tunnel(dev->instance,
+					       dev->capture.camera_port, NULL);
+		dev->capture.camera_port = NULL;
+		ret = vchiq_mmal_component_disable(dev->instance,
+						   dev->capture.
+						   encode_component);
+		if (ret)
+			v4l2_err(&dev->v4l2_dev,
+				 "Failed to disable encode component %d\n",
+				 ret);
+
+		dev->capture.encode_component = NULL;
+	}
+	/* format dependant port setup */
+	switch (mfmt->mmal_component) {
+	case MMAL_COMPONENT_CAMERA:
+		/* Make a further decision on port based on resolution */
+		if (f->fmt.pix.width <= max_video_width
+		    && f->fmt.pix.height <= max_video_height)
+			camera_port = port =
+			    &dev->component[MMAL_COMPONENT_CAMERA]->
+			    output[MMAL_CAMERA_PORT_VIDEO];
+		else
+			camera_port = port =
+			    &dev->component[MMAL_COMPONENT_CAMERA]->
+			    output[MMAL_CAMERA_PORT_CAPTURE];
+		break;
+	case MMAL_COMPONENT_IMAGE_ENCODE:
+		encode_component = dev->component[MMAL_COMPONENT_IMAGE_ENCODE];
+		port = &dev->component[MMAL_COMPONENT_IMAGE_ENCODE]->output[0];
+		camera_port =
+		    &dev->component[MMAL_COMPONENT_CAMERA]->
+		    output[MMAL_CAMERA_PORT_CAPTURE];
+		break;
+	case MMAL_COMPONENT_VIDEO_ENCODE:
+		encode_component = dev->component[MMAL_COMPONENT_VIDEO_ENCODE];
+		port = &dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0];
+		camera_port =
+		    &dev->component[MMAL_COMPONENT_CAMERA]->
+		    output[MMAL_CAMERA_PORT_VIDEO];
+		break;
+	default:
+		break;
+	}
+
+	if (!port)
+		return -EINVAL;
+
+	if (encode_component)
+		camera_port->format.encoding = MMAL_ENCODING_OPAQUE;
+	else
+		camera_port->format.encoding = mfmt->mmal;
+
+	camera_port->format.encoding_variant = 0;
+	camera_port->es.video.width = f->fmt.pix.width;
+	camera_port->es.video.height = f->fmt.pix.height;
+	camera_port->es.video.crop.x = 0;
+	camera_port->es.video.crop.y = 0;
+	camera_port->es.video.crop.width = f->fmt.pix.width;
+	camera_port->es.video.crop.height = f->fmt.pix.height;
+	camera_port->es.video.frame_rate.num = 0;
+	camera_port->es.video.frame_rate.den = 1;
+	camera_port->es.video.color_space = MMAL_COLOR_SPACE_JPEG_JFIF;
+
+	ret = vchiq_mmal_port_set_format(dev->instance, camera_port);
+
+	if (!ret
+	    && camera_port ==
+	    &dev->component[MMAL_COMPONENT_CAMERA]->
+	    output[MMAL_CAMERA_PORT_VIDEO]) {
+		bool overlay_enabled =
+		    !!dev->component[MMAL_COMPONENT_PREVIEW]->enabled;
+		struct vchiq_mmal_port *preview_port =
+		    &dev->component[MMAL_COMPONENT_CAMERA]->
+		    output[MMAL_CAMERA_PORT_PREVIEW];
+		/* Preview and encode ports need to match on resolution */
+		if (overlay_enabled) {
+			/* Need to disable the overlay before we can update
+			 * the resolution
+			 */
+			ret =
+			    vchiq_mmal_port_disable(dev->instance,
+						    preview_port);
+			if (!ret)
+				ret =
+				    vchiq_mmal_port_connect_tunnel(
+						dev->instance,
+						preview_port,
+						NULL);
+		}
+		preview_port->es.video.width = f->fmt.pix.width;
+		preview_port->es.video.height = f->fmt.pix.height;
+		preview_port->es.video.crop.x = 0;
+		preview_port->es.video.crop.y = 0;
+		preview_port->es.video.crop.width = f->fmt.pix.width;
+		preview_port->es.video.crop.height = f->fmt.pix.height;
+		preview_port->es.video.frame_rate.num =
+					  dev->capture.timeperframe.denominator;
+		preview_port->es.video.frame_rate.den =
+					  dev->capture.timeperframe.numerator;
+		ret = vchiq_mmal_port_set_format(dev->instance, preview_port);
+		if (overlay_enabled) {
+			ret = vchiq_mmal_port_connect_tunnel(
+				dev->instance,
+				preview_port,
+				&dev->component[MMAL_COMPONENT_PREVIEW]->input[0]);
+			if (!ret)
+				ret = vchiq_mmal_port_enable(dev->instance,
+							     preview_port,
+							     NULL);
+		}
+	}
+
+	if (ret) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "%s failed to set format %dx%d %08X\n", __func__,
+			 f->fmt.pix.width, f->fmt.pix.height,
+			 f->fmt.pix.pixelformat);
+		/* ensure capture is not going to be tried */
+		dev->capture.port = NULL;
+	} else {
+		if (encode_component) {
+			v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+				 "vid_cap - set up encode comp\n");
+
+			/* configure buffering */
+			camera_port->current_buffer.size =
+			    camera_port->recommended_buffer.size;
+			camera_port->current_buffer.num =
+			    camera_port->recommended_buffer.num;
+
+			ret =
+			    vchiq_mmal_port_connect_tunnel(
+					dev->instance,
+					camera_port,
+					&encode_component->input[0]);
+			if (ret) {
+				v4l2_dbg(1, bcm2835_v4l2_debug,
+					 &dev->v4l2_dev,
+					 "%s failed to create connection\n",
+					 __func__);
+				/* ensure capture is not going to be tried */
+				dev->capture.port = NULL;
+			} else {
+				port->es.video.width = f->fmt.pix.width;
+				port->es.video.height = f->fmt.pix.height;
+				port->es.video.crop.x = 0;
+				port->es.video.crop.y = 0;
+				port->es.video.crop.width = f->fmt.pix.width;
+				port->es.video.crop.height = f->fmt.pix.height;
+				port->es.video.frame_rate.num =
+					  dev->capture.timeperframe.denominator;
+				port->es.video.frame_rate.den =
+					  dev->capture.timeperframe.numerator;
+
+				port->format.encoding = mfmt->mmal;
+				port->format.encoding_variant = 0;
+				/* Set any encoding specific parameters */
+				switch (mfmt->mmal_component) {
+				case MMAL_COMPONENT_VIDEO_ENCODE:
+					port->format.bitrate =
+					    dev->capture.encode_bitrate;
+					break;
+				case MMAL_COMPONENT_IMAGE_ENCODE:
+					/* Could set EXIF parameters here */
+					break;
+				default:
+					break;
+				}
+				ret = vchiq_mmal_port_set_format(dev->instance,
+								 port);
+				if (ret)
+					v4l2_dbg(1, bcm2835_v4l2_debug,
+						 &dev->v4l2_dev,
+						 "%s failed to set format %dx%d fmt %08X\n",
+						 __func__,
+						 f->fmt.pix.width,
+						 f->fmt.pix.height,
+						 f->fmt.pix.pixelformat
+						 );
+			}
+
+			if (!ret) {
+				ret = vchiq_mmal_component_enable(
+						dev->instance,
+						encode_component);
+				if (ret) {
+					v4l2_dbg(1, bcm2835_v4l2_debug,
+					   &dev->v4l2_dev,
+					   "%s Failed to enable encode components\n",
+					   __func__);
+				}
+			}
+			if (!ret) {
+				/* configure buffering */
+				port->current_buffer.num = 1;
+				port->current_buffer.size =
+				    f->fmt.pix.sizeimage;
+				if (port->format.encoding ==
+				    MMAL_ENCODING_JPEG) {
+					v4l2_dbg(1, bcm2835_v4l2_debug,
+					    &dev->v4l2_dev,
+					    "JPG - buf size now %d was %d\n",
+					    f->fmt.pix.sizeimage,
+					    port->current_buffer.size);
+					port->current_buffer.size =
+					    (f->fmt.pix.sizeimage <
+					     (100 << 10))
+					    ? (100 << 10) : f->fmt.pix.
+					    sizeimage;
+				}
+				v4l2_dbg(1, bcm2835_v4l2_debug,
+					 &dev->v4l2_dev,
+					 "vid_cap - cur_buf.size set to %d\n",
+					 f->fmt.pix.sizeimage);
+				port->current_buffer.alignment = 0;
+			}
+		} else {
+			/* configure buffering */
+			camera_port->current_buffer.num = 1;
+			camera_port->current_buffer.size = f->fmt.pix.sizeimage;
+			camera_port->current_buffer.alignment = 0;
+		}
+
+		if (!ret) {
+			dev->capture.fmt = mfmt;
+			dev->capture.stride = f->fmt.pix.bytesperline;
+			dev->capture.width = camera_port->es.video.crop.width;
+			dev->capture.height = camera_port->es.video.crop.height;
+			dev->capture.buffersize = port->current_buffer.size;
+
+			/* select port for capture */
+			dev->capture.port = port;
+			dev->capture.camera_port = camera_port;
+			dev->capture.encode_component = encode_component;
+			v4l2_dbg(1, bcm2835_v4l2_debug,
+				 &dev->v4l2_dev,
+				"Set dev->capture.fmt %08X, %dx%d, stride %d, size %d",
+				port->format.encoding,
+				dev->capture.width, dev->capture.height,
+				dev->capture.stride, dev->capture.buffersize);
+		}
+	}
+
+	/* todo: Need to convert the vchiq/mmal error into a v4l2 error. */
+	return ret;
+}
+
+static int vidioc_s_fmt_vid_cap(struct file *file, void *priv,
+				struct v4l2_format *f)
+{
+	int ret;
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	struct mmal_fmt *mfmt;
+
+	/* try the format to set valid parameters */
+	ret = vidioc_try_fmt_vid_cap(file, priv, f);
+	if (ret) {
+		v4l2_err(&dev->v4l2_dev,
+			 "vid_cap - vidioc_try_fmt_vid_cap failed\n");
+		return ret;
+	}
+
+	/* if a capture is running refuse to set format */
+	if (vb2_is_busy(&dev->capture.vb_vidq)) {
+		v4l2_info(&dev->v4l2_dev, "%s device busy\n", __func__);
+		return -EBUSY;
+	}
+
+	/* If the format is unsupported v4l2 says we should switch to
+	 * a supported one and not return an error. */
+	mfmt = get_format(f);
+	if (!mfmt) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "Fourcc format (0x%08x) unknown.\n",
+			 f->fmt.pix.pixelformat);
+		f->fmt.pix.pixelformat = formats[0].fourcc;
+		mfmt = get_format(f);
+	}
+
+	ret = mmal_setup_components(dev, f);
+	if (ret != 0) {
+		v4l2_err(&dev->v4l2_dev,
+			 "%s: failed to setup mmal components: %d\n",
+			 __func__, ret);
+		ret = -EINVAL;
+	}
+
+	return ret;
+}
+
+int vidioc_enum_framesizes(struct file *file, void *fh,
+			   struct v4l2_frmsizeenum *fsize)
+{
+	static const struct v4l2_frmsize_stepwise sizes = {
+		MIN_WIDTH, MAX_WIDTH, 2,
+		MIN_HEIGHT, MAX_HEIGHT, 2
+	};
+	int i;
+
+	if (fsize->index)
+		return -EINVAL;
+	for (i = 0; i < ARRAY_SIZE(formats); i++)
+		if (formats[i].fourcc == fsize->pixel_format)
+			break;
+	if (i == ARRAY_SIZE(formats))
+		return -EINVAL;
+	fsize->type = V4L2_FRMSIZE_TYPE_STEPWISE;
+	fsize->stepwise = sizes;
+	return 0;
+}
+
+/* timeperframe is arbitrary and continous */
+static int vidioc_enum_frameintervals(struct file *file, void *priv,
+					     struct v4l2_frmivalenum *fival)
+{
+	int i;
+
+	if (fival->index)
+		return -EINVAL;
+
+	for (i = 0; i < ARRAY_SIZE(formats); i++)
+		if (formats[i].fourcc == fival->pixel_format)
+			break;
+	if (i == ARRAY_SIZE(formats))
+		return -EINVAL;
+
+	/* regarding width & height - we support any within range */
+	if (fival->width < MIN_WIDTH || fival->width > MAX_WIDTH ||
+	    fival->height < MIN_HEIGHT || fival->height > MAX_HEIGHT)
+		return -EINVAL;
+
+	fival->type = V4L2_FRMIVAL_TYPE_CONTINUOUS;
+
+	/* fill in stepwise (step=1.0 is requred by V4L2 spec) */
+	fival->stepwise.min  = tpf_min;
+	fival->stepwise.max  = tpf_max;
+	fival->stepwise.step = (struct v4l2_fract) {1, 1};
+
+	return 0;
+}
+
+static int vidioc_g_parm(struct file *file, void *priv,
+			  struct v4l2_streamparm *parm)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+
+	if (parm->type != V4L2_BUF_TYPE_VIDEO_CAPTURE)
+		return -EINVAL;
+
+	parm->parm.capture.capability   = V4L2_CAP_TIMEPERFRAME;
+	parm->parm.capture.timeperframe = dev->capture.timeperframe;
+	parm->parm.capture.readbuffers  = 1;
+	return 0;
+}
+
+#define FRACT_CMP(a, OP, b)	\
+	((u64)(a).numerator * (b).denominator  OP  \
+	 (u64)(b).numerator * (a).denominator)
+
+static int vidioc_s_parm(struct file *file, void *priv,
+			  struct v4l2_streamparm *parm)
+{
+	struct bm2835_mmal_dev *dev = video_drvdata(file);
+	struct v4l2_fract tpf;
+	struct mmal_parameter_rational fps_param;
+
+	if (parm->type != V4L2_BUF_TYPE_VIDEO_CAPTURE)
+		return -EINVAL;
+
+	tpf = parm->parm.capture.timeperframe;
+
+	/* tpf: {*, 0} resets timing; clip to [min, max]*/
+	tpf = tpf.denominator ? tpf : tpf_default;
+	tpf = FRACT_CMP(tpf, <, tpf_min) ? tpf_min : tpf;
+	tpf = FRACT_CMP(tpf, >, tpf_max) ? tpf_max : tpf;
+
+	dev->capture.timeperframe = tpf;
+	parm->parm.capture.timeperframe = tpf;
+	parm->parm.capture.readbuffers  = 1;
+
+	fps_param.num = 0;	/* Select variable fps, and then use
+				 * FPS_RANGE to select the actual limits.
+				 */
+	fps_param.den = 1;
+	set_framerate_params(dev);
+
+	return 0;
+}
+
+static const struct v4l2_ioctl_ops camera0_ioctl_ops = {
+	/* overlay */
+	.vidioc_enum_fmt_vid_overlay = vidioc_enum_fmt_vid_overlay,
+	.vidioc_g_fmt_vid_overlay = vidioc_g_fmt_vid_overlay,
+	.vidioc_try_fmt_vid_overlay = vidioc_try_fmt_vid_overlay,
+	.vidioc_s_fmt_vid_overlay = vidioc_s_fmt_vid_overlay,
+	.vidioc_overlay = vidioc_overlay,
+	.vidioc_g_fbuf = vidioc_g_fbuf,
+
+	/* inputs */
+	.vidioc_enum_input = vidioc_enum_input,
+	.vidioc_g_input = vidioc_g_input,
+	.vidioc_s_input = vidioc_s_input,
+
+	/* capture */
+	.vidioc_querycap = vidioc_querycap,
+	.vidioc_enum_fmt_vid_cap = vidioc_enum_fmt_vid_cap,
+	.vidioc_g_fmt_vid_cap = vidioc_g_fmt_vid_cap,
+	.vidioc_try_fmt_vid_cap = vidioc_try_fmt_vid_cap,
+	.vidioc_s_fmt_vid_cap = vidioc_s_fmt_vid_cap,
+
+	/* buffer management */
+	.vidioc_reqbufs = vb2_ioctl_reqbufs,
+	.vidioc_create_bufs = vb2_ioctl_create_bufs,
+	.vidioc_prepare_buf = vb2_ioctl_prepare_buf,
+	.vidioc_querybuf = vb2_ioctl_querybuf,
+	.vidioc_qbuf = vb2_ioctl_qbuf,
+	.vidioc_dqbuf = vb2_ioctl_dqbuf,
+	.vidioc_enum_framesizes = vidioc_enum_framesizes,
+	.vidioc_enum_frameintervals = vidioc_enum_frameintervals,
+	.vidioc_g_parm        = vidioc_g_parm,
+	.vidioc_s_parm        = vidioc_s_parm,
+	.vidioc_streamon = vb2_ioctl_streamon,
+	.vidioc_streamoff = vb2_ioctl_streamoff,
+
+	.vidioc_log_status = v4l2_ctrl_log_status,
+	.vidioc_subscribe_event = v4l2_ctrl_subscribe_event,
+	.vidioc_unsubscribe_event = v4l2_event_unsubscribe,
+};
+
+static const struct v4l2_ioctl_ops camera0_ioctl_ops_gstreamer = {
+	/* overlay */
+	.vidioc_enum_fmt_vid_overlay = vidioc_enum_fmt_vid_overlay,
+	.vidioc_g_fmt_vid_overlay = vidioc_g_fmt_vid_overlay,
+	.vidioc_try_fmt_vid_overlay = vidioc_try_fmt_vid_overlay,
+	.vidioc_s_fmt_vid_overlay = vidioc_s_fmt_vid_overlay,
+	.vidioc_overlay = vidioc_overlay,
+	.vidioc_g_fbuf = vidioc_g_fbuf,
+
+	/* inputs */
+	.vidioc_enum_input = vidioc_enum_input,
+	.vidioc_g_input = vidioc_g_input,
+	.vidioc_s_input = vidioc_s_input,
+
+	/* capture */
+	.vidioc_querycap = vidioc_querycap,
+	.vidioc_enum_fmt_vid_cap = vidioc_enum_fmt_vid_cap,
+	.vidioc_g_fmt_vid_cap = vidioc_g_fmt_vid_cap,
+	.vidioc_try_fmt_vid_cap = vidioc_try_fmt_vid_cap,
+	.vidioc_s_fmt_vid_cap = vidioc_s_fmt_vid_cap,
+
+	/* buffer management */
+	.vidioc_reqbufs = vb2_ioctl_reqbufs,
+	.vidioc_create_bufs = vb2_ioctl_create_bufs,
+	.vidioc_prepare_buf = vb2_ioctl_prepare_buf,
+	.vidioc_querybuf = vb2_ioctl_querybuf,
+	.vidioc_qbuf = vb2_ioctl_qbuf,
+	.vidioc_dqbuf = vb2_ioctl_dqbuf,
+	/* Remove this function ptr to fix gstreamer bug
+	.vidioc_enum_framesizes = vidioc_enum_framesizes, */
+	.vidioc_enum_frameintervals = vidioc_enum_frameintervals,
+	.vidioc_g_parm        = vidioc_g_parm,
+	.vidioc_s_parm        = vidioc_s_parm,
+	.vidioc_streamon = vb2_ioctl_streamon,
+	.vidioc_streamoff = vb2_ioctl_streamoff,
+
+	.vidioc_log_status = v4l2_ctrl_log_status,
+	.vidioc_subscribe_event = v4l2_ctrl_subscribe_event,
+	.vidioc_unsubscribe_event = v4l2_event_unsubscribe,
+};
+
+/* ------------------------------------------------------------------
+	Driver init/finalise
+   ------------------------------------------------------------------*/
+
+static const struct v4l2_file_operations camera0_fops = {
+	.owner = THIS_MODULE,
+	.open = v4l2_fh_open,
+	.release = vb2_fop_release,
+	.read = vb2_fop_read,
+	.poll = vb2_fop_poll,
+	.unlocked_ioctl = video_ioctl2,	/* V4L2 ioctl handler */
+	.mmap = vb2_fop_mmap,
+};
+
+static struct video_device vdev_template = {
+	.name = "camera0",
+	.fops = &camera0_fops,
+	.ioctl_ops = &camera0_ioctl_ops,
+	.release = video_device_release_empty,
+};
+
+static int set_camera_parameters(struct vchiq_mmal_instance *instance,
+				 struct vchiq_mmal_component *camera)
+{
+	int ret;
+	struct mmal_parameter_camera_config cam_config = {
+		.max_stills_w = MAX_WIDTH,
+		.max_stills_h = MAX_HEIGHT,
+		.stills_yuv422 = 1,
+		.one_shot_stills = 1,
+		.max_preview_video_w = (max_video_width > 1920) ?
+						max_video_width : 1920,
+		.max_preview_video_h = (max_video_height > 1088) ?
+						max_video_height : 1088,
+		.num_preview_video_frames = 3,
+		.stills_capture_circular_buffer_height = 0,
+		.fast_preview_resume = 0,
+		.use_stc_timestamp = MMAL_PARAM_TIMESTAMP_MODE_RAW_STC
+	};
+
+	ret = vchiq_mmal_port_parameter_set(instance, &camera->control,
+					    MMAL_PARAMETER_CAMERA_CONFIG,
+					    &cam_config, sizeof(cam_config));
+	return ret;
+}
+
+/* MMAL instance and component init */
+static int __init mmal_init(struct bm2835_mmal_dev *dev)
+{
+	int ret;
+	struct mmal_es_format *format;
+	u32 bool_true = 1;
+
+	ret = vchiq_mmal_init(&dev->instance);
+	if (ret < 0)
+		return ret;
+
+	/* get the camera component ready */
+	ret = vchiq_mmal_component_init(dev->instance, "ril.camera",
+					&dev->component[MMAL_COMPONENT_CAMERA]);
+	if (ret < 0)
+		goto unreg_mmal;
+
+	if (dev->component[MMAL_COMPONENT_CAMERA]->outputs <
+	    MMAL_CAMERA_PORT_COUNT) {
+		ret = -EINVAL;
+		goto unreg_camera;
+	}
+
+	ret = set_camera_parameters(dev->instance,
+				    dev->component[MMAL_COMPONENT_CAMERA]);
+	if (ret < 0)
+		goto unreg_camera;
+
+	format =
+	    &dev->component[MMAL_COMPONENT_CAMERA]->
+	    output[MMAL_CAMERA_PORT_PREVIEW].format;
+
+	format->encoding = MMAL_ENCODING_OPAQUE;
+	format->encoding_variant = MMAL_ENCODING_I420;
+
+	format->es->video.width = 1024;
+	format->es->video.height = 768;
+	format->es->video.crop.x = 0;
+	format->es->video.crop.y = 0;
+	format->es->video.crop.width = 1024;
+	format->es->video.crop.height = 768;
+	format->es->video.frame_rate.num = 0; /* Rely on fps_range */
+	format->es->video.frame_rate.den = 1;
+
+	format =
+	    &dev->component[MMAL_COMPONENT_CAMERA]->
+	    output[MMAL_CAMERA_PORT_VIDEO].format;
+
+	format->encoding = MMAL_ENCODING_OPAQUE;
+	format->encoding_variant = MMAL_ENCODING_I420;
+
+	format->es->video.width = 1024;
+	format->es->video.height = 768;
+	format->es->video.crop.x = 0;
+	format->es->video.crop.y = 0;
+	format->es->video.crop.width = 1024;
+	format->es->video.crop.height = 768;
+	format->es->video.frame_rate.num = 0; /* Rely on fps_range */
+	format->es->video.frame_rate.den = 1;
+
+	vchiq_mmal_port_parameter_set(dev->instance,
+		&dev->component[MMAL_COMPONENT_CAMERA]->
+				output[MMAL_CAMERA_PORT_VIDEO],
+		MMAL_PARAMETER_NO_IMAGE_PADDING,
+		&bool_true, sizeof(bool_true));
+
+	format =
+	    &dev->component[MMAL_COMPONENT_CAMERA]->
+	    output[MMAL_CAMERA_PORT_CAPTURE].format;
+
+	format->encoding = MMAL_ENCODING_OPAQUE;
+
+	format->es->video.width = 2592;
+	format->es->video.height = 1944;
+	format->es->video.crop.x = 0;
+	format->es->video.crop.y = 0;
+	format->es->video.crop.width = 2592;
+	format->es->video.crop.height = 1944;
+	format->es->video.frame_rate.num = 0; /* Rely on fps_range */
+	format->es->video.frame_rate.den = 1;
+
+	dev->capture.width = format->es->video.width;
+	dev->capture.height = format->es->video.height;
+	dev->capture.fmt = &formats[0];
+	dev->capture.encode_component = NULL;
+	dev->capture.timeperframe = tpf_default;
+	dev->capture.enc_profile = V4L2_MPEG_VIDEO_H264_PROFILE_HIGH;
+	dev->capture.enc_level = V4L2_MPEG_VIDEO_H264_LEVEL_4_0;
+
+	vchiq_mmal_port_parameter_set(dev->instance,
+		&dev->component[MMAL_COMPONENT_CAMERA]->
+			output[MMAL_CAMERA_PORT_CAPTURE],
+		MMAL_PARAMETER_NO_IMAGE_PADDING,
+		&bool_true, sizeof(bool_true));
+
+	/* get the preview component ready */
+	ret = vchiq_mmal_component_init(
+			dev->instance, "ril.video_render",
+			&dev->component[MMAL_COMPONENT_PREVIEW]);
+	if (ret < 0)
+		goto unreg_camera;
+
+	if (dev->component[MMAL_COMPONENT_PREVIEW]->inputs < 1) {
+		ret = -EINVAL;
+		pr_debug("too few input ports %d needed %d\n",
+			 dev->component[MMAL_COMPONENT_PREVIEW]->inputs, 1);
+		goto unreg_preview;
+	}
+
+	/* get the image encoder component ready */
+	ret = vchiq_mmal_component_init(
+		dev->instance, "ril.image_encode",
+		&dev->component[MMAL_COMPONENT_IMAGE_ENCODE]);
+	if (ret < 0)
+		goto unreg_preview;
+
+	if (dev->component[MMAL_COMPONENT_IMAGE_ENCODE]->inputs < 1) {
+		ret = -EINVAL;
+		v4l2_err(&dev->v4l2_dev, "too few input ports %d needed %d\n",
+			 dev->component[MMAL_COMPONENT_IMAGE_ENCODE]->inputs,
+			 1);
+		goto unreg_image_encoder;
+	}
+
+	/* get the video encoder component ready */
+	ret = vchiq_mmal_component_init(dev->instance, "ril.video_encode",
+					&dev->
+					component[MMAL_COMPONENT_VIDEO_ENCODE]);
+	if (ret < 0)
+		goto unreg_image_encoder;
+
+	if (dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->inputs < 1) {
+		ret = -EINVAL;
+		v4l2_err(&dev->v4l2_dev, "too few input ports %d needed %d\n",
+			 dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->inputs,
+			 1);
+		goto unreg_vid_encoder;
+	}
+
+	{
+		struct vchiq_mmal_port *encoder_port =
+			&dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0];
+		encoder_port->format.encoding = MMAL_ENCODING_H264;
+		ret = vchiq_mmal_port_set_format(dev->instance,
+			encoder_port);
+	}
+
+	{
+		unsigned int enable = 1;
+		vchiq_mmal_port_parameter_set(
+			dev->instance,
+			&dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->control,
+			MMAL_PARAMETER_VIDEO_IMMUTABLE_INPUT,
+			&enable, sizeof(enable));
+
+		vchiq_mmal_port_parameter_set(dev->instance,
+			&dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->control,
+			MMAL_PARAMETER_MINIMISE_FRAGMENTATION,
+			&enable,
+			sizeof(enable));
+	}
+	ret = bm2835_mmal_set_all_camera_controls(dev);
+	if (ret < 0)
+		goto unreg_vid_encoder;
+
+	return 0;
+
+unreg_vid_encoder:
+	pr_err("Cleanup: Destroy video encoder\n");
+	vchiq_mmal_component_finalise(
+		dev->instance,
+		dev->component[MMAL_COMPONENT_VIDEO_ENCODE]);
+
+unreg_image_encoder:
+	pr_err("Cleanup: Destroy image encoder\n");
+	vchiq_mmal_component_finalise(
+		dev->instance,
+		dev->component[MMAL_COMPONENT_IMAGE_ENCODE]);
+
+unreg_preview:
+	pr_err("Cleanup: Destroy video render\n");
+	vchiq_mmal_component_finalise(dev->instance,
+				      dev->component[MMAL_COMPONENT_PREVIEW]);
+
+unreg_camera:
+	pr_err("Cleanup: Destroy camera\n");
+	vchiq_mmal_component_finalise(dev->instance,
+				      dev->component[MMAL_COMPONENT_CAMERA]);
+
+unreg_mmal:
+	vchiq_mmal_finalise(dev->instance);
+	return ret;
+}
+
+static int __init bm2835_mmal_init_device(struct bm2835_mmal_dev *dev,
+					  struct video_device *vfd)
+{
+	int ret;
+
+	*vfd = vdev_template;
+	if (gst_v4l2src_is_broken) {
+		v4l2_info(&dev->v4l2_dev,
+		  "Work-around for gstreamer issue is active.\n");
+		vfd->ioctl_ops = &camera0_ioctl_ops_gstreamer;
+	}
+
+	vfd->v4l2_dev = &dev->v4l2_dev;
+
+	vfd->lock = &dev->mutex;
+
+	vfd->queue = &dev->capture.vb_vidq;
+
+	/* video device needs to be able to access instance data */
+	video_set_drvdata(vfd, dev);
+
+	ret = video_register_device(vfd, VFL_TYPE_GRABBER, -1);
+	if (ret < 0)
+		return ret;
+
+	v4l2_info(vfd->v4l2_dev,
+		"V4L2 device registered as %s - stills mode > %dx%d\n",
+		video_device_node_name(vfd), max_video_width, max_video_height);
+
+	return 0;
+}
+
+static struct v4l2_format default_v4l2_format = {
+	.fmt.pix.pixelformat = V4L2_PIX_FMT_JPEG,
+	.fmt.pix.width = 1024,
+	.fmt.pix.bytesperline = 1024,
+	.fmt.pix.height = 768,
+	.fmt.pix.sizeimage = 1024*768,
+};
+
+static int __init bm2835_mmal_init(void)
+{
+	int ret;
+	struct bm2835_mmal_dev *dev;
+	struct vb2_queue *q;
+
+	dev = kzalloc(sizeof(*gdev), GFP_KERNEL);
+	if (!dev)
+		return -ENOMEM;
+
+	/* setup device defaults */
+	dev->overlay.w.left = 150;
+	dev->overlay.w.top = 50;
+	dev->overlay.w.width = 1024;
+	dev->overlay.w.height = 768;
+	dev->overlay.clipcount = 0;
+	dev->overlay.field = V4L2_FIELD_NONE;
+
+	dev->capture.fmt = &formats[3]; /* JPEG */
+
+	/* v4l device registration */
+	snprintf(dev->v4l2_dev.name, sizeof(dev->v4l2_dev.name),
+		 "%s", BM2835_MMAL_MODULE_NAME);
+	ret = v4l2_device_register(NULL, &dev->v4l2_dev);
+	if (ret)
+		goto free_dev;
+
+	/* setup v4l controls */
+	ret = bm2835_mmal_init_controls(dev, &dev->ctrl_handler);
+	if (ret < 0)
+		goto unreg_dev;
+	dev->v4l2_dev.ctrl_handler = &dev->ctrl_handler;
+
+	/* mmal init */
+	ret = mmal_init(dev);
+	if (ret < 0)
+		goto unreg_dev;
+
+	/* initialize queue */
+	q = &dev->capture.vb_vidq;
+	memset(q, 0, sizeof(*q));
+	q->type = V4L2_BUF_TYPE_VIDEO_CAPTURE;
+	q->io_modes = VB2_MMAP | VB2_USERPTR | VB2_READ;
+	q->drv_priv = dev;
+	q->buf_struct_size = sizeof(struct mmal_buffer);
+	q->ops = &bm2835_mmal_video_qops;
+	q->mem_ops = &vb2_vmalloc_memops;
+	q->timestamp_flags = V4L2_BUF_FLAG_TIMESTAMP_MONOTONIC;
+	ret = vb2_queue_init(q);
+	if (ret < 0)
+		goto unreg_dev;
+
+	/* v4l2 core mutex used to protect all fops and v4l2 ioctls. */
+	mutex_init(&dev->mutex);
+
+	/* initialise video devices */
+	ret = bm2835_mmal_init_device(dev, &dev->vdev);
+	if (ret < 0)
+		goto unreg_dev;
+
+	/* Really want to call vidioc_s_fmt_vid_cap with the default
+	 * format, but currently the APIs don't join up.
+	 */
+	ret = mmal_setup_components(dev, &default_v4l2_format);
+	if (ret < 0) {
+		v4l2_err(&dev->v4l2_dev,
+			 "%s: could not setup components\n", __func__);
+		goto unreg_dev;
+	}
+
+	v4l2_info(&dev->v4l2_dev,
+		  "Broadcom 2835 MMAL video capture ver %s loaded.\n",
+		  BM2835_MMAL_VERSION);
+
+	gdev = dev;
+	return 0;
+
+unreg_dev:
+	v4l2_ctrl_handler_free(&dev->ctrl_handler);
+	v4l2_device_unregister(&dev->v4l2_dev);
+
+free_dev:
+	kfree(dev);
+
+	v4l2_err(&dev->v4l2_dev,
+		 "%s: error %d while loading driver\n",
+		 BM2835_MMAL_MODULE_NAME, ret);
+
+	return ret;
+}
+
+static void __exit bm2835_mmal_exit(void)
+{
+	if (!gdev)
+		return;
+
+	v4l2_info(&gdev->v4l2_dev, "unregistering %s\n",
+		  video_device_node_name(&gdev->vdev));
+
+	video_unregister_device(&gdev->vdev);
+
+	if (gdev->capture.encode_component) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &gdev->v4l2_dev,
+			 "mmal_exit - disconnect tunnel\n");
+		vchiq_mmal_port_connect_tunnel(gdev->instance,
+					       gdev->capture.camera_port, NULL);
+		vchiq_mmal_component_disable(gdev->instance,
+					     gdev->capture.encode_component);
+	}
+	vchiq_mmal_component_disable(gdev->instance,
+				     gdev->component[MMAL_COMPONENT_CAMERA]);
+
+	vchiq_mmal_component_finalise(gdev->instance,
+				      gdev->
+				      component[MMAL_COMPONENT_VIDEO_ENCODE]);
+
+	vchiq_mmal_component_finalise(gdev->instance,
+				      gdev->
+				      component[MMAL_COMPONENT_IMAGE_ENCODE]);
+
+	vchiq_mmal_component_finalise(gdev->instance,
+				      gdev->component[MMAL_COMPONENT_PREVIEW]);
+
+	vchiq_mmal_component_finalise(gdev->instance,
+				      gdev->component[MMAL_COMPONENT_CAMERA]);
+
+	vchiq_mmal_finalise(gdev->instance);
+
+	v4l2_ctrl_handler_free(&gdev->ctrl_handler);
+
+	v4l2_device_unregister(&gdev->v4l2_dev);
+
+	kfree(gdev);
+}
+
+module_init(bm2835_mmal_init);
+module_exit(bm2835_mmal_exit);
--- /dev/null
+++ b/drivers/media/platform/bcm2835/bcm2835-camera.h
@@ -0,0 +1,126 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ *
+ * core driver device
+ */
+
+#define V4L2_CTRL_COUNT 28 /* number of v4l controls */
+
+enum {
+	MMAL_COMPONENT_CAMERA = 0,
+	MMAL_COMPONENT_PREVIEW,
+	MMAL_COMPONENT_IMAGE_ENCODE,
+	MMAL_COMPONENT_VIDEO_ENCODE,
+	MMAL_COMPONENT_COUNT
+};
+
+enum {
+	MMAL_CAMERA_PORT_PREVIEW = 0,
+	MMAL_CAMERA_PORT_VIDEO,
+	MMAL_CAMERA_PORT_CAPTURE,
+	MMAL_CAMERA_PORT_COUNT
+};
+
+#define PREVIEW_LAYER      2
+
+extern int bcm2835_v4l2_debug;
+
+struct bm2835_mmal_dev {
+	/* v4l2 devices */
+	struct v4l2_device     v4l2_dev;
+	struct video_device    vdev;
+	struct mutex           mutex;
+
+	/* controls */
+	struct v4l2_ctrl_handler  ctrl_handler;
+	struct v4l2_ctrl          *ctrls[V4L2_CTRL_COUNT];
+	enum v4l2_scene_mode	  scene_mode;
+	struct mmal_colourfx      colourfx;
+	int                       hflip;
+	int                       vflip;
+	int			  red_gain;
+	int			  blue_gain;
+	enum mmal_parameter_exposuremode exposure_mode_user;
+	enum v4l2_exposure_auto_type exposure_mode_v4l2_user;
+	/* active exposure mode may differ if selected via a scene mode */
+	enum mmal_parameter_exposuremode exposure_mode_active;
+	enum mmal_parameter_exposuremeteringmode metering_mode;
+	unsigned int		  manual_shutter_speed;
+	bool			  exp_auto_priority;
+
+	/* allocated mmal instance and components */
+	struct vchiq_mmal_instance   *instance;
+	struct vchiq_mmal_component  *component[MMAL_COMPONENT_COUNT];
+	int camera_use_count;
+
+	struct v4l2_window overlay;
+
+	struct {
+		unsigned int     width;  /* width */
+		unsigned int     height;  /* height */
+		unsigned int     stride;  /* stride */
+		unsigned int     buffersize; /* buffer size with padding */
+		struct mmal_fmt  *fmt;
+		struct v4l2_fract timeperframe;
+
+		/* H264 encode bitrate */
+		int         encode_bitrate;
+		/* H264 bitrate mode. CBR/VBR */
+		int         encode_bitrate_mode;
+		/* H264 profile */
+		enum v4l2_mpeg_video_h264_profile enc_profile;
+		/* H264 level */
+		enum v4l2_mpeg_video_h264_level enc_level;
+		/* JPEG Q-factor */
+		int         q_factor;
+
+		struct vb2_queue	vb_vidq;
+
+		/* VC start timestamp for streaming */
+		s64         vc_start_timestamp;
+		/* Kernel start timestamp for streaming */
+		struct timeval kernel_start_ts;
+
+		struct vchiq_mmal_port  *port; /* port being used for capture */
+		/* camera port being used for capture */
+		struct vchiq_mmal_port  *camera_port;
+		/* component being used for encode */
+		struct vchiq_mmal_component *encode_component;
+		/* number of frames remaining which driver should capture */
+		unsigned int  frame_count;
+		/* last frame completion */
+		struct completion  frame_cmplt;
+
+	} capture;
+
+};
+
+int bm2835_mmal_init_controls(
+			struct bm2835_mmal_dev *dev,
+			struct v4l2_ctrl_handler *hdl);
+
+int bm2835_mmal_set_all_camera_controls(struct bm2835_mmal_dev *dev);
+int set_framerate_params(struct bm2835_mmal_dev *dev);
+
+/* Debug helpers */
+
+#define v4l2_dump_pix_format(level, debug, dev, pix_fmt, desc)	\
+{	\
+	v4l2_dbg(level, debug, dev,	\
+"%s: w %u h %u field %u pfmt 0x%x bpl %u sz_img %u colorspace 0x%x priv %u\n", \
+		desc == NULL ? "" : desc,	\
+		(pix_fmt)->width, (pix_fmt)->height, (pix_fmt)->field,	\
+		(pix_fmt)->pixelformat, (pix_fmt)->bytesperline,	\
+		(pix_fmt)->sizeimage, (pix_fmt)->colorspace, (pix_fmt)->priv); \
+}
--- /dev/null
+++ b/drivers/media/platform/bcm2835/controls.c
@@ -0,0 +1,1324 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+#include <linux/errno.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/slab.h>
+#include <media/videobuf2-vmalloc.h>
+#include <media/v4l2-device.h>
+#include <media/v4l2-ioctl.h>
+#include <media/v4l2-ctrls.h>
+#include <media/v4l2-fh.h>
+#include <media/v4l2-event.h>
+#include <media/v4l2-common.h>
+
+#include "mmal-common.h"
+#include "mmal-vchiq.h"
+#include "mmal-parameters.h"
+#include "bcm2835-camera.h"
+
+/* The supported V4L2_CID_AUTO_EXPOSURE_BIAS values are from -4.0 to +4.0.
+ * MMAL values are in 1/6th increments so the MMAL range is -24 to +24.
+ * V4L2 docs say value "is expressed in terms of EV, drivers should interpret
+ * the values as 0.001 EV units, where the value 1000 stands for +1 EV."
+ * V4L2 is limited to a max of 32 values in a menu, so count in 1/3rds from
+ * -4 to +4
+ */
+static const s64 ev_bias_qmenu[] = {
+	-4000, -3667, -3333,
+	-3000, -2667, -2333,
+	-2000, -1667, -1333,
+	-1000,  -667,  -333,
+	    0,   333,   667,
+	 1000,  1333,  1667,
+	 2000,  2333,  2667,
+	 3000,  3333,  3667,
+	 4000
+};
+
+/* Supported ISO values
+ * ISOO = auto ISO
+ */
+static const s64 iso_qmenu[] = {
+	0, 100, 200, 400, 800,
+};
+
+static const s64 mains_freq_qmenu[] = {
+	V4L2_CID_POWER_LINE_FREQUENCY_DISABLED,
+	V4L2_CID_POWER_LINE_FREQUENCY_50HZ,
+	V4L2_CID_POWER_LINE_FREQUENCY_60HZ,
+	V4L2_CID_POWER_LINE_FREQUENCY_AUTO
+};
+
+/* Supported video encode modes */
+static const s64 bitrate_mode_qmenu[] = {
+	(s64)V4L2_MPEG_VIDEO_BITRATE_MODE_VBR,
+	(s64)V4L2_MPEG_VIDEO_BITRATE_MODE_CBR,
+};
+
+enum bm2835_mmal_ctrl_type {
+	MMAL_CONTROL_TYPE_STD,
+	MMAL_CONTROL_TYPE_STD_MENU,
+	MMAL_CONTROL_TYPE_INT_MENU,
+	MMAL_CONTROL_TYPE_CLUSTER, /* special cluster entry */
+};
+
+struct bm2835_mmal_v4l2_ctrl;
+
+typedef	int(bm2835_mmal_v4l2_ctrl_cb)(
+				struct bm2835_mmal_dev *dev,
+				struct v4l2_ctrl *ctrl,
+				const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl);
+
+struct bm2835_mmal_v4l2_ctrl {
+	u32 id; /* v4l2 control identifier */
+	enum bm2835_mmal_ctrl_type type;
+	/* control minimum value or
+	 * mask for MMAL_CONTROL_TYPE_STD_MENU */
+	s32 min;
+	s32 max; /* maximum value of control */
+	s32 def;  /* default value of control */
+	s32 step; /* step size of the control */
+	const s64 *imenu; /* integer menu array */
+	u32 mmal_id; /* mmal parameter id */
+	bm2835_mmal_v4l2_ctrl_cb *setter;
+	bool ignore_errors;
+};
+
+struct v4l2_to_mmal_effects_setting {
+	u32 v4l2_effect;
+	u32 mmal_effect;
+	s32 col_fx_enable;
+	s32 col_fx_fixed_cbcr;
+	u32 u;
+	u32 v;
+	u32 num_effect_params;
+	u32 effect_params[MMAL_MAX_IMAGEFX_PARAMETERS];
+};
+
+static const struct v4l2_to_mmal_effects_setting
+	v4l2_to_mmal_effects_values[] = {
+	{  V4L2_COLORFX_NONE,         MMAL_PARAM_IMAGEFX_NONE,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_BW,           MMAL_PARAM_IMAGEFX_NONE,
+		1,   0,    128,  128, 0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SEPIA,        MMAL_PARAM_IMAGEFX_NONE,
+		1,   0,    87,   151, 0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_NEGATIVE,     MMAL_PARAM_IMAGEFX_NEGATIVE,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_EMBOSS,       MMAL_PARAM_IMAGEFX_EMBOSS,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SKETCH,       MMAL_PARAM_IMAGEFX_SKETCH,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SKY_BLUE,     MMAL_PARAM_IMAGEFX_PASTEL,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_GRASS_GREEN,  MMAL_PARAM_IMAGEFX_WATERCOLOUR,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SKIN_WHITEN,  MMAL_PARAM_IMAGEFX_WASHEDOUT,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_VIVID,        MMAL_PARAM_IMAGEFX_SATURATION,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_AQUA,         MMAL_PARAM_IMAGEFX_NONE,
+		1,   0,    171,  121, 0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_ART_FREEZE,   MMAL_PARAM_IMAGEFX_HATCH,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SILHOUETTE,   MMAL_PARAM_IMAGEFX_FILM,
+		0,   0,    0,    0,   0, {0, 0, 0, 0, 0} },
+	{  V4L2_COLORFX_SOLARIZATION, MMAL_PARAM_IMAGEFX_SOLARIZE,
+		0,   0,    0,    0,   5, {1, 128, 160, 160, 48} },
+	{  V4L2_COLORFX_ANTIQUE,      MMAL_PARAM_IMAGEFX_COLOURBALANCE,
+		0,   0,    0,    0,   3, {108, 274, 238, 0, 0} },
+	{  V4L2_COLORFX_SET_CBCR,     MMAL_PARAM_IMAGEFX_NONE,
+		1,   1,    0,    0,   0, {0, 0, 0, 0, 0} }
+};
+
+struct v4l2_mmal_scene_config {
+	enum v4l2_scene_mode			v4l2_scene;
+	enum mmal_parameter_exposuremode	exposure_mode;
+	enum mmal_parameter_exposuremeteringmode metering_mode;
+};
+
+static const struct v4l2_mmal_scene_config scene_configs[] = {
+	/* V4L2_SCENE_MODE_NONE automatically added */
+	{
+		V4L2_SCENE_MODE_NIGHT,
+		MMAL_PARAM_EXPOSUREMODE_NIGHT,
+		MMAL_PARAM_EXPOSUREMETERINGMODE_AVERAGE
+	},
+	{
+		V4L2_SCENE_MODE_SPORTS,
+		MMAL_PARAM_EXPOSUREMODE_SPORTS,
+		MMAL_PARAM_EXPOSUREMETERINGMODE_AVERAGE
+	},
+};
+
+/* control handlers*/
+
+static int ctrl_set_rational(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	struct mmal_parameter_rational rational_value;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	rational_value.num = ctrl->val;
+	rational_value.den = 100;
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &rational_value,
+					     sizeof(rational_value));
+}
+
+static int ctrl_set_value(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	u32_value = ctrl->val;
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_value_menu(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *control;
+
+	if (ctrl->val > mmal_ctrl->max || ctrl->val < mmal_ctrl->min)
+		return 1;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	u32_value = mmal_ctrl->imenu[ctrl->val];
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_value_ev(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	s32 s32_value;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	s32_value = (ctrl->val-12)*2;	/* Convert from index to 1/6ths */
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &s32_value, sizeof(s32_value));
+}
+
+static int ctrl_set_rotate(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret;
+	u32 u32_value;
+	struct vchiq_mmal_component *camera;
+
+	camera = dev->component[MMAL_COMPONENT_CAMERA];
+
+	u32_value = ((ctrl->val % 360) / 90) * 90;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[0],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+	if (ret < 0)
+		return ret;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[1],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+	if (ret < 0)
+		return ret;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[2],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+
+	return ret;
+}
+
+static int ctrl_set_flip(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret;
+	u32 u32_value;
+	struct vchiq_mmal_component *camera;
+
+	if (ctrl->id == V4L2_CID_HFLIP)
+		dev->hflip = ctrl->val;
+	else
+		dev->vflip = ctrl->val;
+
+	camera = dev->component[MMAL_COMPONENT_CAMERA];
+
+	if (dev->hflip && dev->vflip)
+		u32_value = MMAL_PARAM_MIRROR_BOTH;
+	else if (dev->hflip)
+		u32_value = MMAL_PARAM_MIRROR_HORIZONTAL;
+	else if (dev->vflip)
+		u32_value = MMAL_PARAM_MIRROR_VERTICAL;
+	else
+		u32_value = MMAL_PARAM_MIRROR_NONE;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[0],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+	if (ret < 0)
+		return ret;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[1],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+	if (ret < 0)
+		return ret;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, &camera->output[2],
+					    mmal_ctrl->mmal_id,
+					    &u32_value, sizeof(u32_value));
+
+	return ret;
+
+}
+
+static int ctrl_set_exposure(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	enum mmal_parameter_exposuremode exp_mode = dev->exposure_mode_user;
+	u32 shutter_speed = 0;
+	struct vchiq_mmal_port *control;
+	int ret = 0;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	if (mmal_ctrl->mmal_id == MMAL_PARAMETER_SHUTTER_SPEED)	{
+		/* V4L2 is in 100usec increments.
+		 * MMAL is 1usec.
+		 */
+		dev->manual_shutter_speed = ctrl->val * 100;
+	} else if (mmal_ctrl->mmal_id == MMAL_PARAMETER_EXPOSURE_MODE) {
+		switch (ctrl->val) {
+		case V4L2_EXPOSURE_AUTO:
+			exp_mode = MMAL_PARAM_EXPOSUREMODE_AUTO;
+			break;
+
+		case V4L2_EXPOSURE_MANUAL:
+			exp_mode = MMAL_PARAM_EXPOSUREMODE_OFF;
+			break;
+		}
+		dev->exposure_mode_user = exp_mode;
+		dev->exposure_mode_v4l2_user = ctrl->val;
+	} else if (mmal_ctrl->id == V4L2_CID_EXPOSURE_AUTO_PRIORITY) {
+		dev->exp_auto_priority = ctrl->val;
+	}
+
+	if (dev->scene_mode == V4L2_SCENE_MODE_NONE) {
+		if (exp_mode == MMAL_PARAM_EXPOSUREMODE_OFF)
+			shutter_speed = dev->manual_shutter_speed;
+
+		ret = vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_SHUTTER_SPEED,
+					&shutter_speed,
+					sizeof(shutter_speed));
+		ret += vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_EXPOSURE_MODE,
+					&exp_mode,
+					sizeof(u32));
+		dev->exposure_mode_active = exp_mode;
+	}
+	/* exposure_dynamic_framerate (V4L2_CID_EXPOSURE_AUTO_PRIORITY) should
+	 * always apply irrespective of scene mode.
+	 */
+	ret += set_framerate_params(dev);
+
+	return ret;
+}
+
+static int ctrl_set_metering_mode(struct bm2835_mmal_dev *dev,
+			   struct v4l2_ctrl *ctrl,
+			   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	switch (ctrl->val) {
+	case V4L2_EXPOSURE_METERING_AVERAGE:
+		dev->metering_mode = MMAL_PARAM_EXPOSUREMETERINGMODE_AVERAGE;
+		break;
+
+	case V4L2_EXPOSURE_METERING_CENTER_WEIGHTED:
+		dev->metering_mode = MMAL_PARAM_EXPOSUREMETERINGMODE_BACKLIT;
+		break;
+
+	case V4L2_EXPOSURE_METERING_SPOT:
+		dev->metering_mode = MMAL_PARAM_EXPOSUREMETERINGMODE_SPOT;
+		break;
+
+	/* todo matrix weighting not added to Linux API till 3.9
+	case V4L2_EXPOSURE_METERING_MATRIX:
+		dev->metering_mode = MMAL_PARAM_EXPOSUREMETERINGMODE_MATRIX;
+		break;
+	*/
+
+	}
+
+	if (dev->scene_mode == V4L2_SCENE_MODE_NONE) {
+		struct vchiq_mmal_port *control;
+		u32 u32_value = dev->metering_mode;
+
+		control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+		return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+	} else
+		return 0;
+}
+
+static int ctrl_set_flicker_avoidance(struct bm2835_mmal_dev *dev,
+			   struct v4l2_ctrl *ctrl,
+			   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	switch (ctrl->val) {
+	case V4L2_CID_POWER_LINE_FREQUENCY_DISABLED:
+		u32_value = MMAL_PARAM_FLICKERAVOID_OFF;
+		break;
+	case V4L2_CID_POWER_LINE_FREQUENCY_50HZ:
+		u32_value = MMAL_PARAM_FLICKERAVOID_50HZ;
+		break;
+	case V4L2_CID_POWER_LINE_FREQUENCY_60HZ:
+		u32_value = MMAL_PARAM_FLICKERAVOID_60HZ;
+		break;
+	case V4L2_CID_POWER_LINE_FREQUENCY_AUTO:
+		u32_value = MMAL_PARAM_FLICKERAVOID_AUTO;
+		break;
+	}
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_awb_mode(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	switch (ctrl->val) {
+	case V4L2_WHITE_BALANCE_MANUAL:
+		u32_value = MMAL_PARAM_AWBMODE_OFF;
+		break;
+
+	case V4L2_WHITE_BALANCE_AUTO:
+		u32_value = MMAL_PARAM_AWBMODE_AUTO;
+		break;
+
+	case V4L2_WHITE_BALANCE_INCANDESCENT:
+		u32_value = MMAL_PARAM_AWBMODE_INCANDESCENT;
+		break;
+
+	case V4L2_WHITE_BALANCE_FLUORESCENT:
+		u32_value = MMAL_PARAM_AWBMODE_FLUORESCENT;
+		break;
+
+	case V4L2_WHITE_BALANCE_FLUORESCENT_H:
+		u32_value = MMAL_PARAM_AWBMODE_TUNGSTEN;
+		break;
+
+	case V4L2_WHITE_BALANCE_HORIZON:
+		u32_value = MMAL_PARAM_AWBMODE_HORIZON;
+		break;
+
+	case V4L2_WHITE_BALANCE_DAYLIGHT:
+		u32_value = MMAL_PARAM_AWBMODE_SUNLIGHT;
+		break;
+
+	case V4L2_WHITE_BALANCE_FLASH:
+		u32_value = MMAL_PARAM_AWBMODE_FLASH;
+		break;
+
+	case V4L2_WHITE_BALANCE_CLOUDY:
+		u32_value = MMAL_PARAM_AWBMODE_CLOUDY;
+		break;
+
+	case V4L2_WHITE_BALANCE_SHADE:
+		u32_value = MMAL_PARAM_AWBMODE_SHADE;
+		break;
+
+	}
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_awb_gains(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	struct vchiq_mmal_port *control;
+	struct mmal_parameter_awbgains gains;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	if (ctrl->id == V4L2_CID_RED_BALANCE)
+		dev->red_gain = ctrl->val;
+	else if (ctrl->id == V4L2_CID_BLUE_BALANCE)
+		dev->blue_gain = ctrl->val;
+
+	gains.r_gain.num = dev->red_gain;
+	gains.b_gain.num = dev->blue_gain;
+	gains.r_gain.den = gains.b_gain.den = 1000;
+
+	return vchiq_mmal_port_parameter_set(dev->instance, control,
+					     mmal_ctrl->mmal_id,
+					     &gains, sizeof(gains));
+}
+
+static int ctrl_set_image_effect(struct bm2835_mmal_dev *dev,
+		   struct v4l2_ctrl *ctrl,
+		   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret = -EINVAL;
+	int i, j;
+	struct vchiq_mmal_port *control;
+	struct mmal_parameter_imagefx_parameters imagefx;
+
+	for (i = 0; i < ARRAY_SIZE(v4l2_to_mmal_effects_values); i++) {
+		if (ctrl->val == v4l2_to_mmal_effects_values[i].v4l2_effect) {
+
+			imagefx.effect =
+				v4l2_to_mmal_effects_values[i].mmal_effect;
+			imagefx.num_effect_params =
+				v4l2_to_mmal_effects_values[i].num_effect_params;
+
+			if (imagefx.num_effect_params > MMAL_MAX_IMAGEFX_PARAMETERS)
+				imagefx.num_effect_params = MMAL_MAX_IMAGEFX_PARAMETERS;
+
+			for (j = 0; j < imagefx.num_effect_params; j++)
+				imagefx.effect_parameter[j] =
+					v4l2_to_mmal_effects_values[i].effect_params[j];
+
+			dev->colourfx.enable =
+				v4l2_to_mmal_effects_values[i].col_fx_enable;
+			if (!v4l2_to_mmal_effects_values[i].col_fx_fixed_cbcr) {
+				dev->colourfx.u =
+					v4l2_to_mmal_effects_values[i].u;
+				dev->colourfx.v =
+					v4l2_to_mmal_effects_values[i].v;
+			}
+
+			control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+			ret = vchiq_mmal_port_parameter_set(
+					dev->instance, control,
+					MMAL_PARAMETER_IMAGE_EFFECT_PARAMETERS,
+					&imagefx, sizeof(imagefx));
+			if (ret)
+				goto exit;
+
+			ret = vchiq_mmal_port_parameter_set(
+					dev->instance, control,
+					MMAL_PARAMETER_COLOUR_EFFECT,
+					&dev->colourfx, sizeof(dev->colourfx));
+		}
+	}
+
+exit:
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "mmal_ctrl:%p ctrl id:0x%x ctrl val:%d imagefx:0x%x color_effect:%s u:%d v:%d ret %d(%d)\n",
+				mmal_ctrl, ctrl->id, ctrl->val, imagefx.effect,
+				dev->colourfx.enable ? "true" : "false",
+				dev->colourfx.u, dev->colourfx.v,
+				ret, (ret == 0 ? 0 : -EINVAL));
+	return (ret == 0 ? 0 : EINVAL);
+}
+
+static int ctrl_set_colfx(struct bm2835_mmal_dev *dev,
+		   struct v4l2_ctrl *ctrl,
+		   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret = -EINVAL;
+	struct vchiq_mmal_port *control;
+
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	dev->colourfx.enable = (ctrl->val & 0xff00) >> 8;
+	dev->colourfx.enable = ctrl->val & 0xff;
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, control,
+					MMAL_PARAMETER_COLOUR_EFFECT,
+					&dev->colourfx, sizeof(dev->colourfx));
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "%s: After: mmal_ctrl:%p ctrl id:0x%x ctrl val:%d ret %d(%d)\n",
+			__func__, mmal_ctrl, ctrl->id, ctrl->val, ret,
+			(ret == 0 ? 0 : -EINVAL));
+	return (ret == 0 ? 0 : EINVAL);
+}
+
+static int ctrl_set_bitrate(struct bm2835_mmal_dev *dev,
+		   struct v4l2_ctrl *ctrl,
+		   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret;
+	struct vchiq_mmal_port *encoder_out;
+
+	dev->capture.encode_bitrate = ctrl->val;
+
+	encoder_out = &dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0];
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance, encoder_out,
+					    mmal_ctrl->mmal_id,
+					    &ctrl->val, sizeof(ctrl->val));
+	ret = 0;
+	return ret;
+}
+
+static int ctrl_set_bitrate_mode(struct bm2835_mmal_dev *dev,
+		   struct v4l2_ctrl *ctrl,
+		   const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 bitrate_mode;
+	struct vchiq_mmal_port *encoder_out;
+
+	encoder_out = &dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0];
+
+	dev->capture.encode_bitrate_mode = ctrl->val;
+	switch (ctrl->val) {
+	default:
+	case V4L2_MPEG_VIDEO_BITRATE_MODE_VBR:
+		bitrate_mode = MMAL_VIDEO_RATECONTROL_VARIABLE;
+		break;
+	case V4L2_MPEG_VIDEO_BITRATE_MODE_CBR:
+		bitrate_mode = MMAL_VIDEO_RATECONTROL_CONSTANT;
+		break;
+	}
+
+	vchiq_mmal_port_parameter_set(dev->instance, encoder_out,
+					     mmal_ctrl->mmal_id,
+					     &bitrate_mode,
+					     sizeof(bitrate_mode));
+	return 0;
+}
+
+static int ctrl_set_image_encode_output(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *jpeg_out;
+
+	jpeg_out = &dev->component[MMAL_COMPONENT_IMAGE_ENCODE]->output[0];
+
+	u32_value = ctrl->val;
+
+	return vchiq_mmal_port_parameter_set(dev->instance, jpeg_out,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_video_encode_param_output(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	u32 u32_value;
+	struct vchiq_mmal_port *vid_enc_ctl;
+
+	vid_enc_ctl = &dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0];
+
+	u32_value = ctrl->val;
+
+	return vchiq_mmal_port_parameter_set(dev->instance, vid_enc_ctl,
+					     mmal_ctrl->mmal_id,
+					     &u32_value, sizeof(u32_value));
+}
+
+static int ctrl_set_video_encode_profile_level(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	struct mmal_parameter_video_profile param;
+	int ret = 0;
+
+	if (ctrl->id == V4L2_CID_MPEG_VIDEO_H264_PROFILE) {
+		switch (ctrl->val) {
+		case V4L2_MPEG_VIDEO_H264_PROFILE_BASELINE:
+		case V4L2_MPEG_VIDEO_H264_PROFILE_CONSTRAINED_BASELINE:
+		case V4L2_MPEG_VIDEO_H264_PROFILE_MAIN:
+		case V4L2_MPEG_VIDEO_H264_PROFILE_HIGH:
+			dev->capture.enc_profile = ctrl->val;
+			break;
+		default:
+			ret = -EINVAL;
+			break;
+		}
+	} else if (ctrl->id == V4L2_CID_MPEG_VIDEO_H264_LEVEL) {
+		switch (ctrl->val) {
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_0:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1B:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_1:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_2:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_3:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_0:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_1:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_2:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_0:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_1:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_2:
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_0:
+			dev->capture.enc_level = ctrl->val;
+			break;
+		default:
+			ret = -EINVAL;
+			break;
+		}
+	}
+
+	if (!ret) {
+		switch (dev->capture.enc_profile) {
+		case V4L2_MPEG_VIDEO_H264_PROFILE_BASELINE:
+			param.profile = MMAL_VIDEO_PROFILE_H264_BASELINE;
+			break;
+		case V4L2_MPEG_VIDEO_H264_PROFILE_CONSTRAINED_BASELINE:
+			param.profile =
+				MMAL_VIDEO_PROFILE_H264_CONSTRAINED_BASELINE;
+			break;
+		case V4L2_MPEG_VIDEO_H264_PROFILE_MAIN:
+			param.profile = MMAL_VIDEO_PROFILE_H264_MAIN;
+			break;
+		case V4L2_MPEG_VIDEO_H264_PROFILE_HIGH:
+			param.profile = MMAL_VIDEO_PROFILE_H264_HIGH;
+			break;
+		default:
+			/* Should never get here */
+			break;
+		}
+
+		switch (dev->capture.enc_level) {
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_0:
+			param.level = MMAL_VIDEO_LEVEL_H264_1;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1B:
+			param.level = MMAL_VIDEO_LEVEL_H264_1b;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_1:
+			param.level = MMAL_VIDEO_LEVEL_H264_11;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_2:
+			param.level = MMAL_VIDEO_LEVEL_H264_12;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_1_3:
+			param.level = MMAL_VIDEO_LEVEL_H264_13;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_0:
+			param.level = MMAL_VIDEO_LEVEL_H264_2;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_1:
+			param.level = MMAL_VIDEO_LEVEL_H264_21;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_2_2:
+			param.level = MMAL_VIDEO_LEVEL_H264_22;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_0:
+			param.level = MMAL_VIDEO_LEVEL_H264_3;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_1:
+			param.level = MMAL_VIDEO_LEVEL_H264_31;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_3_2:
+			param.level = MMAL_VIDEO_LEVEL_H264_32;
+			break;
+		case V4L2_MPEG_VIDEO_H264_LEVEL_4_0:
+			param.level = MMAL_VIDEO_LEVEL_H264_4;
+			break;
+		default:
+			/* Should never get here */
+			break;
+		}
+
+		ret = vchiq_mmal_port_parameter_set(dev->instance,
+			&dev->component[MMAL_COMPONENT_VIDEO_ENCODE]->output[0],
+			mmal_ctrl->mmal_id,
+			&param, sizeof(param));
+	}
+	return ret;
+}
+
+static int ctrl_set_scene_mode(struct bm2835_mmal_dev *dev,
+		      struct v4l2_ctrl *ctrl,
+		      const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl)
+{
+	int ret = 0;
+	int shutter_speed;
+	struct vchiq_mmal_port *control;
+
+	v4l2_dbg(0, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		"scene mode selected %d, was %d\n", ctrl->val,
+		dev->scene_mode);
+	control = &dev->component[MMAL_COMPONENT_CAMERA]->control;
+
+	if (ctrl->val == dev->scene_mode)
+		return 0;
+
+	if (ctrl->val == V4L2_SCENE_MODE_NONE) {
+		/* Restore all user selections */
+		dev->scene_mode = V4L2_SCENE_MODE_NONE;
+
+		if (dev->exposure_mode_user == MMAL_PARAM_EXPOSUREMODE_OFF)
+			shutter_speed = dev->manual_shutter_speed;
+		else
+			shutter_speed = 0;
+
+		v4l2_dbg(0, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			"%s: scene mode none: shut_speed %d, exp_mode %d, metering %d\n",
+			__func__, shutter_speed, dev->exposure_mode_user,
+			dev->metering_mode);
+		ret = vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_SHUTTER_SPEED,
+					&shutter_speed,
+					sizeof(shutter_speed));
+		ret += vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_EXPOSURE_MODE,
+					&dev->exposure_mode_user,
+					sizeof(u32));
+		dev->exposure_mode_active = dev->exposure_mode_user;
+		ret += vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_EXP_METERING_MODE,
+					&dev->metering_mode,
+					sizeof(u32));
+		ret += set_framerate_params(dev);
+	} else {
+		/* Set up scene mode */
+		int i;
+		const struct v4l2_mmal_scene_config *scene = NULL;
+		int shutter_speed;
+		enum mmal_parameter_exposuremode exposure_mode;
+		enum mmal_parameter_exposuremeteringmode metering_mode;
+
+		for (i = 0; i < ARRAY_SIZE(scene_configs); i++) {
+			if (scene_configs[i].v4l2_scene ==
+				ctrl->val) {
+				scene = &scene_configs[i];
+				break;
+			}
+		}
+		if (!scene)
+			return -EINVAL;
+		if (i >= ARRAY_SIZE(scene_configs))
+			return -EINVAL;
+
+		/* Set all the values */
+		dev->scene_mode = ctrl->val;
+
+		if (scene->exposure_mode == MMAL_PARAM_EXPOSUREMODE_OFF)
+			shutter_speed = dev->manual_shutter_speed;
+		else
+			shutter_speed = 0;
+		exposure_mode = scene->exposure_mode;
+		metering_mode = scene->metering_mode;
+
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			"%s: scene mode none: shut_speed %d, exp_mode %d, metering %d\n",
+			__func__, shutter_speed, exposure_mode, metering_mode);
+
+		ret = vchiq_mmal_port_parameter_set(dev->instance, control,
+					MMAL_PARAMETER_SHUTTER_SPEED,
+					&shutter_speed,
+					sizeof(shutter_speed));
+		ret += vchiq_mmal_port_parameter_set(dev->instance,
+					control,
+					MMAL_PARAMETER_EXPOSURE_MODE,
+					&exposure_mode,
+					sizeof(u32));
+		dev->exposure_mode_active = exposure_mode;
+		ret += vchiq_mmal_port_parameter_set(dev->instance, control,
+					MMAL_PARAMETER_EXPOSURE_MODE,
+					&exposure_mode,
+					sizeof(u32));
+		ret += vchiq_mmal_port_parameter_set(dev->instance, control,
+					MMAL_PARAMETER_EXP_METERING_MODE,
+					&metering_mode,
+					sizeof(u32));
+		ret += set_framerate_params(dev);
+	}
+	if (ret) {
+		v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			"%s: Setting scene to %d, ret=%d\n",
+			__func__, ctrl->val, ret);
+		ret = -EINVAL;
+	}
+	return 0;
+}
+
+static int bm2835_mmal_s_ctrl(struct v4l2_ctrl *ctrl)
+{
+	struct bm2835_mmal_dev *dev =
+		container_of(ctrl->handler, struct bm2835_mmal_dev,
+			     ctrl_handler);
+	const struct bm2835_mmal_v4l2_ctrl *mmal_ctrl = ctrl->priv;
+	int ret;
+
+	if ((mmal_ctrl == NULL) ||
+	    (mmal_ctrl->id != ctrl->id) ||
+	    (mmal_ctrl->setter == NULL)) {
+		pr_warn("mmal_ctrl:%p ctrl id:%d\n", mmal_ctrl, ctrl->id);
+		return -EINVAL;
+	}
+
+	ret = mmal_ctrl->setter(dev, ctrl, mmal_ctrl);
+	if (ret)
+		pr_warn("ctrl id:%d/MMAL param %08X- returned ret %d\n",
+				ctrl->id, mmal_ctrl->mmal_id, ret);
+	if (mmal_ctrl->ignore_errors)
+		ret = 0;
+	return ret;
+}
+
+static const struct v4l2_ctrl_ops bm2835_mmal_ctrl_ops = {
+	.s_ctrl = bm2835_mmal_s_ctrl,
+};
+
+
+
+static const struct bm2835_mmal_v4l2_ctrl v4l2_ctrls[V4L2_CTRL_COUNT] = {
+	{
+		V4L2_CID_SATURATION, MMAL_CONTROL_TYPE_STD,
+		-100, 100, 0, 1, NULL,
+		MMAL_PARAMETER_SATURATION,
+		&ctrl_set_rational,
+		false
+	},
+	{
+		V4L2_CID_SHARPNESS, MMAL_CONTROL_TYPE_STD,
+		-100, 100, 0, 1, NULL,
+		MMAL_PARAMETER_SHARPNESS,
+		&ctrl_set_rational,
+		false
+	},
+	{
+		V4L2_CID_CONTRAST, MMAL_CONTROL_TYPE_STD,
+		-100, 100, 0, 1, NULL,
+		MMAL_PARAMETER_CONTRAST,
+		&ctrl_set_rational,
+		false
+	},
+	{
+		V4L2_CID_BRIGHTNESS, MMAL_CONTROL_TYPE_STD,
+		0, 100, 50, 1, NULL,
+		MMAL_PARAMETER_BRIGHTNESS,
+		&ctrl_set_rational,
+		false
+	},
+	{
+		V4L2_CID_ISO_SENSITIVITY, MMAL_CONTROL_TYPE_INT_MENU,
+		0, ARRAY_SIZE(iso_qmenu) - 1, 0, 1, iso_qmenu,
+		MMAL_PARAMETER_ISO,
+		&ctrl_set_value_menu,
+		false
+	},
+	{
+		V4L2_CID_IMAGE_STABILIZATION, MMAL_CONTROL_TYPE_STD,
+		0, 1, 0, 1, NULL,
+		MMAL_PARAMETER_VIDEO_STABILISATION,
+		&ctrl_set_value,
+		false
+	},
+/*	{
+		0, MMAL_CONTROL_TYPE_CLUSTER, 3, 1, 0, NULL, 0, NULL
+	}, */
+	{
+		V4L2_CID_EXPOSURE_AUTO, MMAL_CONTROL_TYPE_STD_MENU,
+		~0x03, 3, V4L2_EXPOSURE_AUTO, 0, NULL,
+		MMAL_PARAMETER_EXPOSURE_MODE,
+		&ctrl_set_exposure,
+		false
+	},
+/* todo this needs mixing in with set exposure
+	{
+	       V4L2_CID_SCENE_MODE, MMAL_CONTROL_TYPE_STD_MENU,
+	},
+ */
+	{
+		V4L2_CID_EXPOSURE_ABSOLUTE, MMAL_CONTROL_TYPE_STD,
+		/* Units of 100usecs */
+		1, 1*1000*10, 100*10, 1, NULL,
+		MMAL_PARAMETER_SHUTTER_SPEED,
+		&ctrl_set_exposure,
+		false
+	},
+	{
+		V4L2_CID_AUTO_EXPOSURE_BIAS, MMAL_CONTROL_TYPE_INT_MENU,
+		0, ARRAY_SIZE(ev_bias_qmenu) - 1,
+		(ARRAY_SIZE(ev_bias_qmenu)+1)/2 - 1, 0, ev_bias_qmenu,
+		MMAL_PARAMETER_EXPOSURE_COMP,
+		&ctrl_set_value_ev,
+		false
+	},
+	{
+		V4L2_CID_EXPOSURE_AUTO_PRIORITY, MMAL_CONTROL_TYPE_STD,
+		0, 1,
+		0, 1, NULL,
+		0,	/* Dummy MMAL ID as it gets mapped into FPS range*/
+		&ctrl_set_exposure,
+		false
+	},
+	{
+		V4L2_CID_EXPOSURE_METERING,
+		MMAL_CONTROL_TYPE_STD_MENU,
+		~0x7, 2, V4L2_EXPOSURE_METERING_AVERAGE, 0, NULL,
+		MMAL_PARAMETER_EXP_METERING_MODE,
+		&ctrl_set_metering_mode,
+		false
+	},
+	{
+		V4L2_CID_AUTO_N_PRESET_WHITE_BALANCE,
+		MMAL_CONTROL_TYPE_STD_MENU,
+		~0x3ff, 9, V4L2_WHITE_BALANCE_AUTO, 0, NULL,
+		MMAL_PARAMETER_AWB_MODE,
+		&ctrl_set_awb_mode,
+		false
+	},
+	{
+		V4L2_CID_RED_BALANCE, MMAL_CONTROL_TYPE_STD,
+		1, 7999, 1000, 1, NULL,
+		MMAL_PARAMETER_CUSTOM_AWB_GAINS,
+		&ctrl_set_awb_gains,
+		false
+	},
+	{
+		V4L2_CID_BLUE_BALANCE, MMAL_CONTROL_TYPE_STD,
+		1, 7999, 1000, 1, NULL,
+		MMAL_PARAMETER_CUSTOM_AWB_GAINS,
+		&ctrl_set_awb_gains,
+		false
+	},
+	{
+		V4L2_CID_COLORFX, MMAL_CONTROL_TYPE_STD_MENU,
+		0, 15, V4L2_COLORFX_NONE, 0, NULL,
+		MMAL_PARAMETER_IMAGE_EFFECT,
+		&ctrl_set_image_effect,
+		false
+	},
+	{
+		V4L2_CID_COLORFX_CBCR, MMAL_CONTROL_TYPE_STD,
+		0, 0xffff, 0x8080, 1, NULL,
+		MMAL_PARAMETER_COLOUR_EFFECT,
+		&ctrl_set_colfx,
+		false
+	},
+	{
+		V4L2_CID_ROTATE, MMAL_CONTROL_TYPE_STD,
+		0, 360, 0, 90, NULL,
+		MMAL_PARAMETER_ROTATION,
+		&ctrl_set_rotate,
+		false
+	},
+	{
+		V4L2_CID_HFLIP, MMAL_CONTROL_TYPE_STD,
+		0, 1, 0, 1, NULL,
+		MMAL_PARAMETER_MIRROR,
+		&ctrl_set_flip,
+		false
+	},
+	{
+		V4L2_CID_VFLIP, MMAL_CONTROL_TYPE_STD,
+		0, 1, 0, 1, NULL,
+		MMAL_PARAMETER_MIRROR,
+		&ctrl_set_flip,
+		false
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_BITRATE_MODE, MMAL_CONTROL_TYPE_STD_MENU,
+		0, ARRAY_SIZE(bitrate_mode_qmenu) - 1,
+		0, 0, bitrate_mode_qmenu,
+		MMAL_PARAMETER_RATECONTROL,
+		&ctrl_set_bitrate_mode,
+		false
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_BITRATE, MMAL_CONTROL_TYPE_STD,
+		25*1000, 25*1000*1000, 10*1000*1000, 25*1000, NULL,
+		MMAL_PARAMETER_VIDEO_BIT_RATE,
+		&ctrl_set_bitrate,
+		false
+	},
+	{
+		V4L2_CID_JPEG_COMPRESSION_QUALITY, MMAL_CONTROL_TYPE_STD,
+		1, 100,
+		30, 1, NULL,
+		MMAL_PARAMETER_JPEG_Q_FACTOR,
+		&ctrl_set_image_encode_output,
+		false
+	},
+	{
+		V4L2_CID_POWER_LINE_FREQUENCY, MMAL_CONTROL_TYPE_STD_MENU,
+		0, ARRAY_SIZE(mains_freq_qmenu) - 1,
+		1, 1, NULL,
+		MMAL_PARAMETER_FLICKER_AVOID,
+		&ctrl_set_flicker_avoidance,
+		false
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_REPEAT_SEQ_HEADER, MMAL_CONTROL_TYPE_STD,
+		0, 1,
+		0, 1, NULL,
+		MMAL_PARAMETER_VIDEO_ENCODE_INLINE_HEADER,
+		&ctrl_set_video_encode_param_output,
+		true	/* Errors ignored as requires latest firmware to work */
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_H264_PROFILE,
+		MMAL_CONTROL_TYPE_STD_MENU,
+		~((1<<V4L2_MPEG_VIDEO_H264_PROFILE_BASELINE) |
+			(1<<V4L2_MPEG_VIDEO_H264_PROFILE_CONSTRAINED_BASELINE) |
+			(1<<V4L2_MPEG_VIDEO_H264_PROFILE_MAIN) |
+			(1<<V4L2_MPEG_VIDEO_H264_PROFILE_HIGH)),
+		V4L2_MPEG_VIDEO_H264_PROFILE_HIGH,
+		V4L2_MPEG_VIDEO_H264_PROFILE_HIGH, 1, NULL,
+		MMAL_PARAMETER_PROFILE,
+		&ctrl_set_video_encode_profile_level,
+		false
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_H264_LEVEL, MMAL_CONTROL_TYPE_STD_MENU,
+		~((1<<V4L2_MPEG_VIDEO_H264_LEVEL_1_0) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_1B) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_1_1) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_1_2) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_1_3) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_2_0) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_2_1) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_2_2) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_3_0) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_3_1) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_3_2) |
+			(1<<V4L2_MPEG_VIDEO_H264_LEVEL_4_0)),
+		V4L2_MPEG_VIDEO_H264_LEVEL_4_0,
+		V4L2_MPEG_VIDEO_H264_LEVEL_4_0, 1, NULL,
+		MMAL_PARAMETER_PROFILE,
+		&ctrl_set_video_encode_profile_level,
+		false
+	},
+	{
+		V4L2_CID_SCENE_MODE, MMAL_CONTROL_TYPE_STD_MENU,
+		-1,	/* Min is computed at runtime */
+		V4L2_SCENE_MODE_TEXT,
+		V4L2_SCENE_MODE_NONE, 1, NULL,
+		MMAL_PARAMETER_PROFILE,
+		&ctrl_set_scene_mode,
+		false
+	},
+	{
+		V4L2_CID_MPEG_VIDEO_H264_I_PERIOD, MMAL_CONTROL_TYPE_STD,
+		0, 0x7FFFFFFF, 60, 1, NULL,
+		MMAL_PARAMETER_INTRAPERIOD,
+		&ctrl_set_video_encode_param_output,
+		false
+	},
+};
+
+int bm2835_mmal_set_all_camera_controls(struct bm2835_mmal_dev *dev)
+{
+	int c;
+	int ret = 0;
+
+	for (c = 0; c < V4L2_CTRL_COUNT; c++) {
+		if ((dev->ctrls[c]) && (v4l2_ctrls[c].setter)) {
+			ret = v4l2_ctrls[c].setter(dev, dev->ctrls[c],
+						   &v4l2_ctrls[c]);
+			if (!v4l2_ctrls[c].ignore_errors && ret) {
+				v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+					"Failed when setting default values for ctrl %d\n",
+					c);
+				break;
+			}
+		}
+	}
+	return ret;
+}
+
+int set_framerate_params(struct bm2835_mmal_dev *dev)
+{
+	struct mmal_parameter_fps_range fps_range;
+	int ret;
+
+	if ((dev->exposure_mode_active != MMAL_PARAM_EXPOSUREMODE_OFF) &&
+	     (dev->exp_auto_priority)) {
+		/* Variable FPS. Define min FPS as 1fps.
+		 * Max as max defined FPS.
+		 */
+		fps_range.fps_low.num = 1;
+		fps_range.fps_low.den = 1;
+		fps_range.fps_high.num = dev->capture.timeperframe.denominator;
+		fps_range.fps_high.den = dev->capture.timeperframe.numerator;
+	} else {
+		/* Fixed FPS - set min and max to be the same */
+		fps_range.fps_low.num = fps_range.fps_high.num =
+			dev->capture.timeperframe.denominator;
+		fps_range.fps_low.den = fps_range.fps_high.den =
+			dev->capture.timeperframe.numerator;
+	}
+
+	v4l2_dbg(1, bcm2835_v4l2_debug, &dev->v4l2_dev,
+			 "Set fps range to %d/%d to %d/%d\n",
+			 fps_range.fps_low.num,
+			 fps_range.fps_low.den,
+			 fps_range.fps_high.num,
+			 fps_range.fps_high.den
+		 );
+
+	ret = vchiq_mmal_port_parameter_set(dev->instance,
+				      &dev->component[MMAL_COMPONENT_CAMERA]->
+					output[MMAL_CAMERA_PORT_PREVIEW],
+				      MMAL_PARAMETER_FPS_RANGE,
+				      &fps_range, sizeof(fps_range));
+	ret += vchiq_mmal_port_parameter_set(dev->instance,
+				      &dev->component[MMAL_COMPONENT_CAMERA]->
+					output[MMAL_CAMERA_PORT_VIDEO],
+				      MMAL_PARAMETER_FPS_RANGE,
+				      &fps_range, sizeof(fps_range));
+	ret += vchiq_mmal_port_parameter_set(dev->instance,
+				      &dev->component[MMAL_COMPONENT_CAMERA]->
+					output[MMAL_CAMERA_PORT_CAPTURE],
+				      MMAL_PARAMETER_FPS_RANGE,
+				      &fps_range, sizeof(fps_range));
+	if (ret)
+		v4l2_dbg(0, bcm2835_v4l2_debug, &dev->v4l2_dev,
+		 "Failed to set fps ret %d\n",
+		 ret);
+
+	return ret;
+
+}
+
+int bm2835_mmal_init_controls(struct bm2835_mmal_dev *dev,
+			      struct v4l2_ctrl_handler *hdl)
+{
+	int c;
+	const struct bm2835_mmal_v4l2_ctrl *ctrl;
+
+	v4l2_ctrl_handler_init(hdl, V4L2_CTRL_COUNT);
+
+	for (c = 0; c < V4L2_CTRL_COUNT; c++) {
+		ctrl = &v4l2_ctrls[c];
+
+		switch (ctrl->type) {
+		case MMAL_CONTROL_TYPE_STD:
+			dev->ctrls[c] = v4l2_ctrl_new_std(hdl,
+				&bm2835_mmal_ctrl_ops, ctrl->id,
+				ctrl->min, ctrl->max, ctrl->step, ctrl->def);
+			break;
+
+		case MMAL_CONTROL_TYPE_STD_MENU:
+		{
+			int mask = ctrl->min;
+
+			if (ctrl->id == V4L2_CID_SCENE_MODE) {
+				/* Special handling to work out the mask
+				 * value based on the scene_configs array
+				 * at runtime. Reduces the chance of
+				 * mismatches.
+				 */
+				int i;
+				mask = 1<<V4L2_SCENE_MODE_NONE;
+				for (i = 0;
+				     i < ARRAY_SIZE(scene_configs);
+				     i++) {
+					mask |= 1<<scene_configs[i].v4l2_scene;
+				}
+				mask = ~mask;
+			}
+
+			dev->ctrls[c] = v4l2_ctrl_new_std_menu(hdl,
+			&bm2835_mmal_ctrl_ops, ctrl->id,
+			ctrl->max, mask, ctrl->def);
+			break;
+		}
+
+		case MMAL_CONTROL_TYPE_INT_MENU:
+			dev->ctrls[c] = v4l2_ctrl_new_int_menu(hdl,
+				&bm2835_mmal_ctrl_ops, ctrl->id,
+				ctrl->max, ctrl->def, ctrl->imenu);
+			break;
+
+		case MMAL_CONTROL_TYPE_CLUSTER:
+			/* skip this entry when constructing controls */
+			continue;
+		}
+
+		if (hdl->error)
+			break;
+
+		dev->ctrls[c]->priv = (void *)ctrl;
+	}
+
+	if (hdl->error) {
+		pr_err("error adding control %d/%d id 0x%x\n", c,
+			 V4L2_CTRL_COUNT, ctrl->id);
+		return hdl->error;
+	}
+
+	for (c = 0; c < V4L2_CTRL_COUNT; c++) {
+		ctrl = &v4l2_ctrls[c];
+
+		switch (ctrl->type) {
+		case MMAL_CONTROL_TYPE_CLUSTER:
+			v4l2_ctrl_auto_cluster(ctrl->min,
+					       &dev->ctrls[c+1],
+					       ctrl->max,
+					       ctrl->def);
+			break;
+
+		case MMAL_CONTROL_TYPE_STD:
+		case MMAL_CONTROL_TYPE_STD_MENU:
+		case MMAL_CONTROL_TYPE_INT_MENU:
+			break;
+		}
+
+	}
+
+	return 0;
+}
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-common.h
@@ -0,0 +1,53 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ *
+ * MMAL structures
+ *
+ */
+
+#define MMAL_FOURCC(a, b, c, d) ((a) | (b << 8) | (c << 16) | (d << 24))
+#define MMAL_MAGIC MMAL_FOURCC('m', 'm', 'a', 'l')
+
+/** Special value signalling that time is not known */
+#define MMAL_TIME_UNKNOWN (1LL<<63)
+
+/* mapping between v4l and mmal video modes */
+struct mmal_fmt {
+	char  *name;
+	u32   fourcc;          /* v4l2 format id */
+	int   flags;           /* v4l2 flags field */
+	u32   mmal;
+	int   depth;
+	u32   mmal_component;  /* MMAL component index to be used to encode */
+	u32   ybbp;            /* depth of first Y plane for planar formats */
+};
+
+/* buffer for one video frame */
+struct mmal_buffer {
+	/* v4l buffer data -- must be first */
+	struct vb2_v4l2_buffer	vb;
+
+	/* list of buffers available */
+	struct list_head	list;
+
+	void *buffer; /* buffer pointer */
+	unsigned long buffer_size; /* size of allocated buffer */
+};
+
+/* */
+struct mmal_colourfx {
+	s32 enable;
+	u32 u;
+	u32 v;
+};
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-encodings.h
@@ -0,0 +1,127 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+#ifndef MMAL_ENCODINGS_H
+#define MMAL_ENCODINGS_H
+
+#define MMAL_ENCODING_H264             MMAL_FOURCC('H', '2', '6', '4')
+#define MMAL_ENCODING_H263             MMAL_FOURCC('H', '2', '6', '3')
+#define MMAL_ENCODING_MP4V             MMAL_FOURCC('M', 'P', '4', 'V')
+#define MMAL_ENCODING_MP2V             MMAL_FOURCC('M', 'P', '2', 'V')
+#define MMAL_ENCODING_MP1V             MMAL_FOURCC('M', 'P', '1', 'V')
+#define MMAL_ENCODING_WMV3             MMAL_FOURCC('W', 'M', 'V', '3')
+#define MMAL_ENCODING_WMV2             MMAL_FOURCC('W', 'M', 'V', '2')
+#define MMAL_ENCODING_WMV1             MMAL_FOURCC('W', 'M', 'V', '1')
+#define MMAL_ENCODING_WVC1             MMAL_FOURCC('W', 'V', 'C', '1')
+#define MMAL_ENCODING_VP8              MMAL_FOURCC('V', 'P', '8', ' ')
+#define MMAL_ENCODING_VP7              MMAL_FOURCC('V', 'P', '7', ' ')
+#define MMAL_ENCODING_VP6              MMAL_FOURCC('V', 'P', '6', ' ')
+#define MMAL_ENCODING_THEORA           MMAL_FOURCC('T', 'H', 'E', 'O')
+#define MMAL_ENCODING_SPARK            MMAL_FOURCC('S', 'P', 'R', 'K')
+#define MMAL_ENCODING_MJPEG            MMAL_FOURCC('M', 'J', 'P', 'G')
+
+#define MMAL_ENCODING_JPEG             MMAL_FOURCC('J', 'P', 'E', 'G')
+#define MMAL_ENCODING_GIF              MMAL_FOURCC('G', 'I', 'F', ' ')
+#define MMAL_ENCODING_PNG              MMAL_FOURCC('P', 'N', 'G', ' ')
+#define MMAL_ENCODING_PPM              MMAL_FOURCC('P', 'P', 'M', ' ')
+#define MMAL_ENCODING_TGA              MMAL_FOURCC('T', 'G', 'A', ' ')
+#define MMAL_ENCODING_BMP              MMAL_FOURCC('B', 'M', 'P', ' ')
+
+#define MMAL_ENCODING_I420             MMAL_FOURCC('I', '4', '2', '0')
+#define MMAL_ENCODING_I420_SLICE       MMAL_FOURCC('S', '4', '2', '0')
+#define MMAL_ENCODING_YV12             MMAL_FOURCC('Y', 'V', '1', '2')
+#define MMAL_ENCODING_I422             MMAL_FOURCC('I', '4', '2', '2')
+#define MMAL_ENCODING_I422_SLICE       MMAL_FOURCC('S', '4', '2', '2')
+#define MMAL_ENCODING_YUYV             MMAL_FOURCC('Y', 'U', 'Y', 'V')
+#define MMAL_ENCODING_YVYU             MMAL_FOURCC('Y', 'V', 'Y', 'U')
+#define MMAL_ENCODING_UYVY             MMAL_FOURCC('U', 'Y', 'V', 'Y')
+#define MMAL_ENCODING_VYUY             MMAL_FOURCC('V', 'Y', 'U', 'Y')
+#define MMAL_ENCODING_NV12             MMAL_FOURCC('N', 'V', '1', '2')
+#define MMAL_ENCODING_NV21             MMAL_FOURCC('N', 'V', '2', '1')
+#define MMAL_ENCODING_ARGB             MMAL_FOURCC('A', 'R', 'G', 'B')
+#define MMAL_ENCODING_RGBA             MMAL_FOURCC('R', 'G', 'B', 'A')
+#define MMAL_ENCODING_ABGR             MMAL_FOURCC('A', 'B', 'G', 'R')
+#define MMAL_ENCODING_BGRA             MMAL_FOURCC('B', 'G', 'R', 'A')
+#define MMAL_ENCODING_RGB16            MMAL_FOURCC('R', 'G', 'B', '2')
+#define MMAL_ENCODING_RGB24            MMAL_FOURCC('R', 'G', 'B', '3')
+#define MMAL_ENCODING_RGB32            MMAL_FOURCC('R', 'G', 'B', '4')
+#define MMAL_ENCODING_BGR16            MMAL_FOURCC('B', 'G', 'R', '2')
+#define MMAL_ENCODING_BGR24            MMAL_FOURCC('B', 'G', 'R', '3')
+#define MMAL_ENCODING_BGR32            MMAL_FOURCC('B', 'G', 'R', '4')
+
+/** SAND Video (YUVUV128) format, native format understood by VideoCore.
+ * This format is *not* opaque - if requested you will receive full frames
+ * of YUV_UV video.
+ */
+#define MMAL_ENCODING_YUVUV128         MMAL_FOURCC('S', 'A', 'N', 'D')
+
+/** VideoCore opaque image format, image handles are returned to
+ * the host but not the actual image data.
+ */
+#define MMAL_ENCODING_OPAQUE           MMAL_FOURCC('O', 'P', 'Q', 'V')
+
+/** An EGL image handle
+ */
+#define MMAL_ENCODING_EGL_IMAGE        MMAL_FOURCC('E', 'G', 'L', 'I')
+
+/* }@ */
+
+/** \name Pre-defined audio encodings */
+/* @{ */
+#define MMAL_ENCODING_PCM_UNSIGNED_BE  MMAL_FOURCC('P', 'C', 'M', 'U')
+#define MMAL_ENCODING_PCM_UNSIGNED_LE  MMAL_FOURCC('p', 'c', 'm', 'u')
+#define MMAL_ENCODING_PCM_SIGNED_BE    MMAL_FOURCC('P', 'C', 'M', 'S')
+#define MMAL_ENCODING_PCM_SIGNED_LE    MMAL_FOURCC('p', 'c', 'm', 's')
+#define MMAL_ENCODING_PCM_FLOAT_BE     MMAL_FOURCC('P', 'C', 'M', 'F')
+#define MMAL_ENCODING_PCM_FLOAT_LE     MMAL_FOURCC('p', 'c', 'm', 'f')
+
+/* Pre-defined H264 encoding variants */
+
+/** ISO 14496-10 Annex B byte stream format */
+#define MMAL_ENCODING_VARIANT_H264_DEFAULT   0
+/** ISO 14496-15 AVC stream format */
+#define MMAL_ENCODING_VARIANT_H264_AVC1      MMAL_FOURCC('A', 'V', 'C', '1')
+/** Implicitly delineated NAL units without emulation prevention */
+#define MMAL_ENCODING_VARIANT_H264_RAW       MMAL_FOURCC('R', 'A', 'W', ' ')
+
+
+/** \defgroup MmalColorSpace List of pre-defined video color spaces
+ * This defines a list of common color spaces. This list isn't exhaustive and
+ * is only provided as a convenience to avoid clients having to use FourCC
+ * codes directly. However components are allowed to define and use their own
+ * FourCC codes.
+ */
+/* @{ */
+
+/** Unknown color space */
+#define MMAL_COLOR_SPACE_UNKNOWN       0
+/** ITU-R BT.601-5 [SDTV] */
+#define MMAL_COLOR_SPACE_ITUR_BT601    MMAL_FOURCC('Y', '6', '0', '1')
+/** ITU-R BT.709-3 [HDTV] */
+#define MMAL_COLOR_SPACE_ITUR_BT709    MMAL_FOURCC('Y', '7', '0', '9')
+/** JPEG JFIF */
+#define MMAL_COLOR_SPACE_JPEG_JFIF     MMAL_FOURCC('Y', 'J', 'F', 'I')
+/** Title 47 Code of Federal Regulations (2003) 73.682 (a) (20) */
+#define MMAL_COLOR_SPACE_FCC           MMAL_FOURCC('Y', 'F', 'C', 'C')
+/** Society of Motion Picture and Television Engineers 240M (1999) */
+#define MMAL_COLOR_SPACE_SMPTE240M     MMAL_FOURCC('Y', '2', '4', '0')
+/** ITU-R BT.470-2 System M */
+#define MMAL_COLOR_SPACE_BT470_2_M     MMAL_FOURCC('Y', '_', '_', 'M')
+/** ITU-R BT.470-2 System BG */
+#define MMAL_COLOR_SPACE_BT470_2_BG    MMAL_FOURCC('Y', '_', 'B', 'G')
+/** JPEG JFIF, but with 16..255 luma */
+#define MMAL_COLOR_SPACE_JFIF_Y16_255  MMAL_FOURCC('Y', 'Y', '1', '6')
+/* @} MmalColorSpace List */
+
+#endif /* MMAL_ENCODINGS_H */
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-msg-common.h
@@ -0,0 +1,50 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+#ifndef MMAL_MSG_COMMON_H
+#define MMAL_MSG_COMMON_H
+
+enum mmal_msg_status {
+	MMAL_MSG_STATUS_SUCCESS = 0, /**< Success */
+	MMAL_MSG_STATUS_ENOMEM,      /**< Out of memory */
+	MMAL_MSG_STATUS_ENOSPC,      /**< Out of resources other than memory */
+	MMAL_MSG_STATUS_EINVAL,      /**< Argument is invalid */
+	MMAL_MSG_STATUS_ENOSYS,      /**< Function not implemented */
+	MMAL_MSG_STATUS_ENOENT,      /**< No such file or directory */
+	MMAL_MSG_STATUS_ENXIO,       /**< No such device or address */
+	MMAL_MSG_STATUS_EIO,         /**< I/O error */
+	MMAL_MSG_STATUS_ESPIPE,      /**< Illegal seek */
+	MMAL_MSG_STATUS_ECORRUPT,    /**< Data is corrupt \attention */
+	MMAL_MSG_STATUS_ENOTREADY,   /**< Component is not ready */
+	MMAL_MSG_STATUS_ECONFIG,     /**< Component is not configured */
+	MMAL_MSG_STATUS_EISCONN,     /**< Port is already connected */
+	MMAL_MSG_STATUS_ENOTCONN,    /**< Port is disconnected */
+	MMAL_MSG_STATUS_EAGAIN,      /**< Resource temporarily unavailable. */
+	MMAL_MSG_STATUS_EFAULT,      /**< Bad address */
+};
+
+struct mmal_rect {
+	s32 x;      /**< x coordinate (from left) */
+	s32 y;      /**< y coordinate (from top) */
+	s32 width;  /**< width */
+	s32 height; /**< height */
+};
+
+struct mmal_rational {
+	s32 num;    /**< Numerator */
+	s32 den;    /**< Denominator */
+};
+
+#endif /* MMAL_MSG_COMMON_H */
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-msg-format.h
@@ -0,0 +1,81 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+#ifndef MMAL_MSG_FORMAT_H
+#define MMAL_MSG_FORMAT_H
+
+#include "mmal-msg-common.h"
+
+/* MMAL_ES_FORMAT_T */
+
+
+struct mmal_audio_format {
+	u32 channels;           /**< Number of audio channels */
+	u32 sample_rate;        /**< Sample rate */
+
+	u32 bits_per_sample;    /**< Bits per sample */
+	u32 block_align;        /**< Size of a block of data */
+};
+
+struct mmal_video_format {
+	u32 width;        /**< Width of frame in pixels */
+	u32 height;       /**< Height of frame in rows of pixels */
+	struct mmal_rect crop;         /**< Visible region of the frame */
+	struct mmal_rational frame_rate;   /**< Frame rate */
+	struct mmal_rational par;          /**< Pixel aspect ratio */
+
+	/* FourCC specifying the color space of the video stream. See the
+	 * \ref MmalColorSpace "pre-defined color spaces" for some examples.
+	 */
+	u32 color_space;
+};
+
+struct mmal_subpicture_format {
+	u32 x_offset;
+	u32 y_offset;
+};
+
+union mmal_es_specific_format {
+	struct mmal_audio_format audio;
+	struct mmal_video_format video;
+	struct mmal_subpicture_format subpicture;
+};
+
+/** Definition of an elementary stream format (MMAL_ES_FORMAT_T) */
+struct mmal_es_format {
+	u32 type;      /* enum mmal_es_type */
+
+	u32 encoding;  /* FourCC specifying encoding of the elementary stream.*/
+	u32 encoding_variant; /* FourCC specifying the specific
+			       * encoding variant of the elementary
+			       * stream.
+			       */
+
+	union mmal_es_specific_format *es; /* TODO: pointers in
+					    * message serialisation?!?
+					    */
+					    /* Type specific
+					     * information for the
+					     * elementary stream
+					     */
+
+	u32 bitrate;        /**< Bitrate in bits per second */
+	u32 flags; /**< Flags describing properties of the elementary stream. */
+
+	u32 extradata_size;       /**< Size of the codec specific data */
+	u8  *extradata;           /**< Codec specific data */
+};
+
+#endif /* MMAL_MSG_FORMAT_H */
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-msg-port.h
@@ -0,0 +1,107 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+/* MMAL_PORT_TYPE_T */
+enum mmal_port_type {
+	MMAL_PORT_TYPE_UNKNOWN = 0,  /**< Unknown port type */
+	MMAL_PORT_TYPE_CONTROL,      /**< Control port */
+	MMAL_PORT_TYPE_INPUT,        /**< Input port */
+	MMAL_PORT_TYPE_OUTPUT,       /**< Output port */
+	MMAL_PORT_TYPE_CLOCK,        /**< Clock port */
+};
+
+/** The port is pass-through and doesn't need buffer headers allocated */
+#define MMAL_PORT_CAPABILITY_PASSTHROUGH                       0x01
+/** The port wants to allocate the buffer payloads.
+ * This signals a preference that payload allocation should be done
+ * on this port for efficiency reasons. */
+#define MMAL_PORT_CAPABILITY_ALLOCATION                        0x02
+/** The port supports format change events.
+ * This applies to input ports and is used to let the client know
+ * whether the port supports being reconfigured via a format
+ * change event (i.e. without having to disable the port). */
+#define MMAL_PORT_CAPABILITY_SUPPORTS_EVENT_FORMAT_CHANGE      0x04
+
+/* mmal port structure (MMAL_PORT_T)
+ *
+ * most elements are informational only, the pointer values for
+ * interogation messages are generally provided as additional
+ * strucures within the message. When used to set values only teh
+ * buffer_num, buffer_size and userdata parameters are writable.
+ */
+struct mmal_port {
+	void *priv; /* Private member used by the framework */
+	const char *name; /* Port name. Used for debugging purposes (RO) */
+
+	u32 type;      /* Type of the port (RO) enum mmal_port_type */
+	u16 index;     /* Index of the port in its type list (RO) */
+	u16 index_all; /* Index of the port in the list of all ports (RO) */
+
+	u32 is_enabled; /* Indicates whether the port is enabled or not (RO) */
+	struct mmal_es_format *format; /* Format of the elementary stream */
+
+	u32 buffer_num_min; /* Minimum number of buffers the port
+			     *   requires (RO).  This is set by the
+			     *   component.
+			     */
+
+	u32 buffer_size_min; /* Minimum size of buffers the port
+			      * requires (RO).  This is set by the
+			      * component.
+			      */
+
+	u32 buffer_alignment_min; /* Minimum alignment requirement for
+				   * the buffers (RO).  A value of
+				   * zero means no special alignment
+				   * requirements.  This is set by the
+				   * component.
+				   */
+
+	u32 buffer_num_recommended;  /* Number of buffers the port
+				      * recommends for optimal
+				      * performance (RO).  A value of
+				      * zero means no special
+				      * recommendation.  This is set
+				      * by the component.
+				      */
+
+	u32 buffer_size_recommended; /* Size of buffers the port
+				      * recommends for optimal
+				      * performance (RO).  A value of
+				      * zero means no special
+				      * recommendation.  This is set
+				      * by the component.
+				      */
+
+	u32 buffer_num; /* Actual number of buffers the port will use.
+			 * This is set by the client.
+			 */
+
+	u32 buffer_size; /* Actual maximum size of the buffers that
+			  * will be sent to the port. This is set by
+			  * the client.
+			  */
+
+	void *component; /* Component this port belongs to (Read Only) */
+
+	void *userdata; /* Field reserved for use by the client */
+
+	u32 capabilities; /* Flags describing the capabilities of a
+			   * port (RO).  Bitwise combination of \ref
+			   * portcapabilities "Port capabilities"
+			   * values.
+			   */
+
+};
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-msg.h
@@ -0,0 +1,404 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+/* all the data structures which serialise the MMAL protocol. note
+ * these are directly mapped onto the recived message data.
+ *
+ * BEWARE: They seem to *assume* pointers are u32 and that there is no
+ * structure padding!
+ *
+ * NOTE: this implementation uses kernel types to ensure sizes. Rather
+ * than assigning values to enums to force their size the
+ * implementation uses fixed size types and not the enums (though the
+ * comments have the actual enum type
+ */
+
+#define VC_MMAL_VER 15
+#define VC_MMAL_MIN_VER 10
+#define VC_MMAL_SERVER_NAME  MAKE_FOURCC("mmal")
+
+/* max total message size is 512 bytes */
+#define MMAL_MSG_MAX_SIZE 512
+/* with six 32bit header elements max payload is therefore 488 bytes */
+#define MMAL_MSG_MAX_PAYLOAD 488
+
+#include "mmal-msg-common.h"
+#include "mmal-msg-format.h"
+#include "mmal-msg-port.h"
+
+enum mmal_msg_type {
+	MMAL_MSG_TYPE_QUIT = 1,
+	MMAL_MSG_TYPE_SERVICE_CLOSED,
+	MMAL_MSG_TYPE_GET_VERSION,
+	MMAL_MSG_TYPE_COMPONENT_CREATE,
+	MMAL_MSG_TYPE_COMPONENT_DESTROY, /* 5 */
+	MMAL_MSG_TYPE_COMPONENT_ENABLE,
+	MMAL_MSG_TYPE_COMPONENT_DISABLE,
+	MMAL_MSG_TYPE_PORT_INFO_GET,
+	MMAL_MSG_TYPE_PORT_INFO_SET,
+	MMAL_MSG_TYPE_PORT_ACTION, /* 10 */
+	MMAL_MSG_TYPE_BUFFER_FROM_HOST,
+	MMAL_MSG_TYPE_BUFFER_TO_HOST,
+	MMAL_MSG_TYPE_GET_STATS,
+	MMAL_MSG_TYPE_PORT_PARAMETER_SET,
+	MMAL_MSG_TYPE_PORT_PARAMETER_GET, /* 15 */
+	MMAL_MSG_TYPE_EVENT_TO_HOST,
+	MMAL_MSG_TYPE_GET_CORE_STATS_FOR_PORT,
+	MMAL_MSG_TYPE_OPAQUE_ALLOCATOR,
+	MMAL_MSG_TYPE_CONSUME_MEM,
+	MMAL_MSG_TYPE_LMK, /* 20 */
+	MMAL_MSG_TYPE_OPAQUE_ALLOCATOR_DESC,
+	MMAL_MSG_TYPE_DRM_GET_LHS32,
+	MMAL_MSG_TYPE_DRM_GET_TIME,
+	MMAL_MSG_TYPE_BUFFER_FROM_HOST_ZEROLEN,
+	MMAL_MSG_TYPE_PORT_FLUSH, /* 25 */
+	MMAL_MSG_TYPE_HOST_LOG,
+	MMAL_MSG_TYPE_MSG_LAST
+};
+
+/* port action request messages differ depending on the action type */
+enum mmal_msg_port_action_type {
+	MMAL_MSG_PORT_ACTION_TYPE_UNKNOWN = 0,      /* Unkown action */
+	MMAL_MSG_PORT_ACTION_TYPE_ENABLE,           /* Enable a port */
+	MMAL_MSG_PORT_ACTION_TYPE_DISABLE,          /* Disable a port */
+	MMAL_MSG_PORT_ACTION_TYPE_FLUSH,            /* Flush a port */
+	MMAL_MSG_PORT_ACTION_TYPE_CONNECT,          /* Connect ports */
+	MMAL_MSG_PORT_ACTION_TYPE_DISCONNECT,       /* Disconnect ports */
+	MMAL_MSG_PORT_ACTION_TYPE_SET_REQUIREMENTS, /* Set buffer requirements*/
+};
+
+struct mmal_msg_header {
+	u32 magic;
+	u32 type; /** enum mmal_msg_type */
+
+	/* Opaque handle to the control service */
+	struct mmal_control_service *control_service;
+
+	struct mmal_msg_context *context; /** a u32 per message context */
+	u32 status; /** The status of the vchiq operation */
+	u32 padding;
+};
+
+/* Send from VC to host to report version */
+struct mmal_msg_version {
+	u32 flags;
+	u32 major;
+	u32 minor;
+	u32 minimum;
+};
+
+/* request to VC to create component */
+struct mmal_msg_component_create {
+	void *client_component; /* component context */
+	char name[128];
+	u32 pid;                /* For debug */
+};
+
+/* reply from VC to component creation request */
+struct mmal_msg_component_create_reply {
+	u32 status; /** enum mmal_msg_status - how does this differ to
+		     * the one in the header?
+		     */
+	u32 component_handle; /* VideoCore handle for component */
+	u32 input_num;        /* Number of input ports */
+	u32 output_num;       /* Number of output ports */
+	u32 clock_num;        /* Number of clock ports */
+};
+
+/* request to VC to destroy a component */
+struct mmal_msg_component_destroy {
+	u32 component_handle;
+};
+
+struct mmal_msg_component_destroy_reply {
+	u32 status; /** The component destruction status */
+};
+
+
+/* request and reply to VC to enable a component */
+struct mmal_msg_component_enable {
+	u32 component_handle;
+};
+
+struct mmal_msg_component_enable_reply {
+	u32 status; /** The component enable status */
+};
+
+
+/* request and reply to VC to disable a component */
+struct mmal_msg_component_disable {
+	u32 component_handle;
+};
+
+struct mmal_msg_component_disable_reply {
+	u32 status; /** The component disable status */
+};
+
+/* request to VC to get port information */
+struct mmal_msg_port_info_get {
+	u32 component_handle;  /* component handle port is associated with */
+	u32 port_type;         /* enum mmal_msg_port_type */
+	u32 index;             /* port index to query */
+};
+
+/* reply from VC to get port info request */
+struct mmal_msg_port_info_get_reply {
+	u32 status; /** enum mmal_msg_status */
+	u32 component_handle;  /* component handle port is associated with */
+	u32 port_type;         /* enum mmal_msg_port_type */
+	u32 port_index;        /* port indexed in query */
+	s32 found;             /* unused */
+	u32 port_handle;               /**< Handle to use for this port */
+	struct mmal_port port;
+	struct mmal_es_format format; /* elementry stream format */
+	union mmal_es_specific_format es; /* es type specific data */
+	u8 extradata[MMAL_FORMAT_EXTRADATA_MAX_SIZE]; /* es extra data */
+};
+
+/* request to VC to set port information */
+struct mmal_msg_port_info_set {
+	u32 component_handle;
+	u32 port_type;         /* enum mmal_msg_port_type */
+	u32 port_index;           /* port indexed in query */
+	struct mmal_port port;
+	struct mmal_es_format format;
+	union mmal_es_specific_format es;
+	u8 extradata[MMAL_FORMAT_EXTRADATA_MAX_SIZE];
+};
+
+/* reply from VC to port info set request */
+struct mmal_msg_port_info_set_reply {
+	u32 status;
+	u32 component_handle;  /* component handle port is associated with */
+	u32 port_type;         /* enum mmal_msg_port_type */
+	u32 index;             /* port indexed in query */
+	s32 found;             /* unused */
+	u32 port_handle;               /**< Handle to use for this port */
+	struct mmal_port port;
+	struct mmal_es_format format;
+	union mmal_es_specific_format es;
+	u8 extradata[MMAL_FORMAT_EXTRADATA_MAX_SIZE];
+};
+
+
+/* port action requests that take a mmal_port as a parameter */
+struct mmal_msg_port_action_port {
+	u32 component_handle;
+	u32 port_handle;
+	u32 action; /* enum mmal_msg_port_action_type */
+	struct mmal_port port;
+};
+
+/* port action requests that take handles as a parameter */
+struct mmal_msg_port_action_handle {
+	u32 component_handle;
+	u32 port_handle;
+	u32 action; /* enum mmal_msg_port_action_type */
+	u32 connect_component_handle;
+	u32 connect_port_handle;
+};
+
+struct mmal_msg_port_action_reply {
+	u32 status; /** The port action operation status */
+};
+
+
+
+
+/* MMAL buffer transfer */
+
+/** Size of space reserved in a buffer message for short messages. */
+#define MMAL_VC_SHORT_DATA 128
+
+/** Signals that the current payload is the end of the stream of data */
+#define MMAL_BUFFER_HEADER_FLAG_EOS                    (1<<0)
+/** Signals that the start of the current payload starts a frame */
+#define MMAL_BUFFER_HEADER_FLAG_FRAME_START            (1<<1)
+/** Signals that the end of the current payload ends a frame */
+#define MMAL_BUFFER_HEADER_FLAG_FRAME_END              (1<<2)
+/** Signals that the current payload contains only complete frames (>1) */
+#define MMAL_BUFFER_HEADER_FLAG_FRAME                  \
+	(MMAL_BUFFER_HEADER_FLAG_FRAME_START|MMAL_BUFFER_HEADER_FLAG_FRAME_END)
+/** Signals that the current payload is a keyframe (i.e. self decodable) */
+#define MMAL_BUFFER_HEADER_FLAG_KEYFRAME               (1<<3)
+/** Signals a discontinuity in the stream of data (e.g. after a seek).
+ * Can be used for instance by a decoder to reset its state */
+#define MMAL_BUFFER_HEADER_FLAG_DISCONTINUITY          (1<<4)
+/** Signals a buffer containing some kind of config data for the component
+ * (e.g. codec config data) */
+#define MMAL_BUFFER_HEADER_FLAG_CONFIG                 (1<<5)
+/** Signals an encrypted payload */
+#define MMAL_BUFFER_HEADER_FLAG_ENCRYPTED              (1<<6)
+/** Signals a buffer containing side information */
+#define MMAL_BUFFER_HEADER_FLAG_CODECSIDEINFO          (1<<7)
+/** Signals a buffer which is the snapshot/postview image from a stills
+ * capture
+ */
+#define MMAL_BUFFER_HEADER_FLAGS_SNAPSHOT              (1<<8)
+/** Signals a buffer which contains data known to be corrupted */
+#define MMAL_BUFFER_HEADER_FLAG_CORRUPTED              (1<<9)
+/** Signals that a buffer failed to be transmitted */
+#define MMAL_BUFFER_HEADER_FLAG_TRANSMISSION_FAILED    (1<<10)
+
+struct mmal_driver_buffer {
+	u32 magic;
+	u32 component_handle;
+	u32 port_handle;
+	void *client_context;
+};
+
+/* buffer header */
+struct mmal_buffer_header {
+	struct mmal_buffer_header *next; /* next header */
+	void *priv; /* framework private data */
+	u32 cmd;
+	void *data;
+	u32 alloc_size;
+	u32 length;
+	u32 offset;
+	u32 flags;
+	s64 pts;
+	s64 dts;
+	void *type;
+	void *user_data;
+};
+
+struct mmal_buffer_header_type_specific {
+	union {
+		struct {
+		u32 planes;
+		u32 offset[4];
+		u32 pitch[4];
+		u32 flags;
+		} video;
+	} u;
+};
+
+struct mmal_msg_buffer_from_host {
+	/* The front 32 bytes of the buffer header are copied
+	 * back to us in the reply to allow for context. This
+	 * area is used to store two mmal_driver_buffer structures to
+	 * allow for multiple concurrent service users.
+	 */
+	/* control data */
+	struct mmal_driver_buffer drvbuf;
+
+	/* referenced control data for passthrough buffer management */
+	struct mmal_driver_buffer drvbuf_ref;
+	struct mmal_buffer_header buffer_header; /* buffer header itself */
+	struct mmal_buffer_header_type_specific buffer_header_type_specific;
+	s32 is_zero_copy;
+	s32 has_reference;
+
+	/** allows short data to be xfered in control message */
+	u32 payload_in_message;
+	u8 short_data[MMAL_VC_SHORT_DATA];
+};
+
+
+/* port parameter setting */
+
+#define MMAL_WORKER_PORT_PARAMETER_SPACE      96
+
+struct mmal_msg_port_parameter_set {
+	u32 component_handle; /* component */
+	u32 port_handle;      /* port */
+	u32 id;     /* Parameter ID  */
+	u32 size;      /* Parameter size */
+	uint32_t value[MMAL_WORKER_PORT_PARAMETER_SPACE];
+};
+
+struct mmal_msg_port_parameter_set_reply {
+	u32 status; /** enum mmal_msg_status todo: how does this
+		     * differ to the one in the header?
+		     */
+};
+
+/* port parameter getting */
+
+struct mmal_msg_port_parameter_get {
+	u32 component_handle; /* component */
+	u32 port_handle;      /* port */
+	u32 id;     /* Parameter ID  */
+	u32 size;      /* Parameter size */
+};
+
+struct mmal_msg_port_parameter_get_reply {
+	u32 status;           /* Status of mmal_port_parameter_get call */
+	u32 id;     /* Parameter ID  */
+	u32 size;      /* Parameter size */
+	uint32_t value[MMAL_WORKER_PORT_PARAMETER_SPACE];
+};
+
+/* event messages */
+#define MMAL_WORKER_EVENT_SPACE 256
+
+struct mmal_msg_event_to_host {
+	void *client_component; /* component context */
+
+	u32 port_type;
+	u32 port_num;
+
+	u32 cmd;
+	u32 length;
+	u8 data[MMAL_WORKER_EVENT_SPACE];
+	struct mmal_buffer_header *delayed_buffer;
+};
+
+/* all mmal messages are serialised through this structure */
+struct mmal_msg {
+	/* header */
+	struct mmal_msg_header h;
+	/* payload */
+	union {
+		struct mmal_msg_version version;
+
+		struct mmal_msg_component_create component_create;
+		struct mmal_msg_component_create_reply component_create_reply;
+
+		struct mmal_msg_component_destroy component_destroy;
+		struct mmal_msg_component_destroy_reply component_destroy_reply;
+
+		struct mmal_msg_component_enable component_enable;
+		struct mmal_msg_component_enable_reply component_enable_reply;
+
+		struct mmal_msg_component_disable component_disable;
+		struct mmal_msg_component_disable_reply component_disable_reply;
+
+		struct mmal_msg_port_info_get port_info_get;
+		struct mmal_msg_port_info_get_reply port_info_get_reply;
+
+		struct mmal_msg_port_info_set port_info_set;
+		struct mmal_msg_port_info_set_reply port_info_set_reply;
+
+		struct mmal_msg_port_action_port port_action_port;
+		struct mmal_msg_port_action_handle port_action_handle;
+		struct mmal_msg_port_action_reply port_action_reply;
+
+		struct mmal_msg_buffer_from_host buffer_from_host;
+
+		struct mmal_msg_port_parameter_set port_parameter_set;
+		struct mmal_msg_port_parameter_set_reply
+			port_parameter_set_reply;
+		struct mmal_msg_port_parameter_get
+			port_parameter_get;
+		struct mmal_msg_port_parameter_get_reply
+			port_parameter_get_reply;
+
+		struct mmal_msg_event_to_host event_to_host;
+
+		u8 payload[MMAL_MSG_MAX_PAYLOAD];
+	} u;
+};
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-parameters.h
@@ -0,0 +1,656 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ */
+
+/* common parameters */
+
+/** @name Parameter groups
+ * Parameters are divided into groups, and then allocated sequentially within
+ * a group using an enum.
+ * @{
+ */
+
+/** Common parameter ID group, used with many types of component. */
+#define MMAL_PARAMETER_GROUP_COMMON            (0<<16)
+/** Camera-specific parameter ID group. */
+#define MMAL_PARAMETER_GROUP_CAMERA            (1<<16)
+/** Video-specific parameter ID group. */
+#define MMAL_PARAMETER_GROUP_VIDEO             (2<<16)
+/** Audio-specific parameter ID group. */
+#define MMAL_PARAMETER_GROUP_AUDIO             (3<<16)
+/** Clock-specific parameter ID group. */
+#define MMAL_PARAMETER_GROUP_CLOCK             (4<<16)
+/** Miracast-specific parameter ID group. */
+#define MMAL_PARAMETER_GROUP_MIRACAST       (5<<16)
+
+/* Common parameters */
+enum mmal_parameter_common_type {
+	MMAL_PARAMETER_UNUSED  /**< Never a valid parameter ID */
+		= MMAL_PARAMETER_GROUP_COMMON,
+	MMAL_PARAMETER_SUPPORTED_ENCODINGS, /**< MMAL_PARAMETER_ENCODING_T */
+	MMAL_PARAMETER_URI, /**< MMAL_PARAMETER_URI_T */
+
+	/** MMAL_PARAMETER_CHANGE_EVENT_REQUEST_T */
+	MMAL_PARAMETER_CHANGE_EVENT_REQUEST,
+
+	/** MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_ZERO_COPY,
+
+	/**< MMAL_PARAMETER_BUFFER_REQUIREMENTS_T */
+	MMAL_PARAMETER_BUFFER_REQUIREMENTS,
+
+	MMAL_PARAMETER_STATISTICS, /**< MMAL_PARAMETER_STATISTICS_T */
+	MMAL_PARAMETER_CORE_STATISTICS, /**< MMAL_PARAMETER_CORE_STATISTICS_T */
+	MMAL_PARAMETER_MEM_USAGE, /**< MMAL_PARAMETER_MEM_USAGE_T */
+	MMAL_PARAMETER_BUFFER_FLAG_FILTER, /**< MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_SEEK, /**< MMAL_PARAMETER_SEEK_T */
+	MMAL_PARAMETER_POWERMON_ENABLE, /**< MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_LOGGING, /**< MMAL_PARAMETER_LOGGING_T */
+	MMAL_PARAMETER_SYSTEM_TIME, /**< MMAL_PARAMETER_UINT64_T */
+	MMAL_PARAMETER_NO_IMAGE_PADDING  /**< MMAL_PARAMETER_BOOLEAN_T */
+};
+
+/* camera parameters */
+
+enum mmal_parameter_camera_type {
+	/* 0 */
+	/** @ref MMAL_PARAMETER_THUMBNAIL_CONFIG_T */
+	MMAL_PARAMETER_THUMBNAIL_CONFIGURATION
+		= MMAL_PARAMETER_GROUP_CAMERA,
+	MMAL_PARAMETER_CAPTURE_QUALITY, /**< Unused? */
+	MMAL_PARAMETER_ROTATION, /**< @ref MMAL_PARAMETER_INT32_T */
+	MMAL_PARAMETER_EXIF_DISABLE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_EXIF, /**< @ref MMAL_PARAMETER_EXIF_T */
+	MMAL_PARAMETER_AWB_MODE, /**< @ref MMAL_PARAM_AWBMODE_T */
+	MMAL_PARAMETER_IMAGE_EFFECT, /**< @ref MMAL_PARAMETER_IMAGEFX_T */
+	MMAL_PARAMETER_COLOUR_EFFECT, /**< @ref MMAL_PARAMETER_COLOURFX_T */
+	MMAL_PARAMETER_FLICKER_AVOID, /**< @ref MMAL_PARAMETER_FLICKERAVOID_T */
+	MMAL_PARAMETER_FLASH, /**< @ref MMAL_PARAMETER_FLASH_T */
+	MMAL_PARAMETER_REDEYE, /**< @ref MMAL_PARAMETER_REDEYE_T */
+	MMAL_PARAMETER_FOCUS, /**< @ref MMAL_PARAMETER_FOCUS_T */
+	MMAL_PARAMETER_FOCAL_LENGTHS, /**< Unused? */
+	MMAL_PARAMETER_EXPOSURE_COMP, /**< @ref MMAL_PARAMETER_INT32_T */
+	MMAL_PARAMETER_ZOOM, /**< @ref MMAL_PARAMETER_SCALEFACTOR_T */
+	MMAL_PARAMETER_MIRROR, /**< @ref MMAL_PARAMETER_MIRROR_T */
+
+	/* 0x10 */
+	MMAL_PARAMETER_CAMERA_NUM, /**< @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_CAPTURE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_EXPOSURE_MODE, /**< @ref MMAL_PARAMETER_EXPOSUREMODE_T */
+	MMAL_PARAMETER_EXP_METERING_MODE, /**< @ref MMAL_PARAMETER_EXPOSUREMETERINGMODE_T */
+	MMAL_PARAMETER_FOCUS_STATUS, /**< @ref MMAL_PARAMETER_FOCUS_STATUS_T */
+	MMAL_PARAMETER_CAMERA_CONFIG, /**< @ref MMAL_PARAMETER_CAMERA_CONFIG_T */
+	MMAL_PARAMETER_CAPTURE_STATUS, /**< @ref MMAL_PARAMETER_CAPTURE_STATUS_T */
+	MMAL_PARAMETER_FACE_TRACK, /**< @ref MMAL_PARAMETER_FACE_TRACK_T */
+	MMAL_PARAMETER_DRAW_BOX_FACES_AND_FOCUS, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_JPEG_Q_FACTOR, /**< @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_FRAME_RATE, /**< @ref MMAL_PARAMETER_FRAME_RATE_T */
+	MMAL_PARAMETER_USE_STC, /**< @ref MMAL_PARAMETER_CAMERA_STC_MODE_T */
+	MMAL_PARAMETER_CAMERA_INFO, /**< @ref MMAL_PARAMETER_CAMERA_INFO_T */
+	MMAL_PARAMETER_VIDEO_STABILISATION, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_FACE_TRACK_RESULTS, /**< @ref MMAL_PARAMETER_FACE_TRACK_RESULTS_T */
+	MMAL_PARAMETER_ENABLE_RAW_CAPTURE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+
+	/* 0x20 */
+	MMAL_PARAMETER_DPF_FILE, /**< @ref MMAL_PARAMETER_URI_T */
+	MMAL_PARAMETER_ENABLE_DPF_FILE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_DPF_FAIL_IS_FATAL, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_CAPTURE_MODE, /**< @ref MMAL_PARAMETER_CAPTUREMODE_T */
+	MMAL_PARAMETER_FOCUS_REGIONS, /**< @ref MMAL_PARAMETER_FOCUS_REGIONS_T */
+	MMAL_PARAMETER_INPUT_CROP, /**< @ref MMAL_PARAMETER_INPUT_CROP_T */
+	MMAL_PARAMETER_SENSOR_INFORMATION, /**< @ref MMAL_PARAMETER_SENSOR_INFORMATION_T */
+	MMAL_PARAMETER_FLASH_SELECT, /**< @ref MMAL_PARAMETER_FLASH_SELECT_T */
+	MMAL_PARAMETER_FIELD_OF_VIEW, /**< @ref MMAL_PARAMETER_FIELD_OF_VIEW_T */
+	MMAL_PARAMETER_HIGH_DYNAMIC_RANGE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_DYNAMIC_RANGE_COMPRESSION, /**< @ref MMAL_PARAMETER_DRC_T */
+	MMAL_PARAMETER_ALGORITHM_CONTROL, /**< @ref MMAL_PARAMETER_ALGORITHM_CONTROL_T */
+	MMAL_PARAMETER_SHARPNESS, /**< @ref MMAL_PARAMETER_RATIONAL_T */
+	MMAL_PARAMETER_CONTRAST, /**< @ref MMAL_PARAMETER_RATIONAL_T */
+	MMAL_PARAMETER_BRIGHTNESS, /**< @ref MMAL_PARAMETER_RATIONAL_T */
+	MMAL_PARAMETER_SATURATION, /**< @ref MMAL_PARAMETER_RATIONAL_T */
+
+	/* 0x30 */
+	MMAL_PARAMETER_ISO, /**< @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_ANTISHAKE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+
+	/** @ref MMAL_PARAMETER_IMAGEFX_PARAMETERS_T */
+	MMAL_PARAMETER_IMAGE_EFFECT_PARAMETERS,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_CAMERA_BURST_CAPTURE,
+
+	/** @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_CAMERA_MIN_ISO,
+
+	/** @ref MMAL_PARAMETER_CAMERA_USE_CASE_T */
+	MMAL_PARAMETER_CAMERA_USE_CASE,
+
+	/**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_CAPTURE_STATS_PASS,
+
+	/** @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_CAMERA_CUSTOM_SENSOR_CONFIG,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_ENABLE_REGISTER_FILE,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_REGISTER_FAIL_IS_FATAL,
+
+	/** @ref MMAL_PARAMETER_CONFIGFILE_T */
+	MMAL_PARAMETER_CONFIGFILE_REGISTERS,
+
+	/** @ref MMAL_PARAMETER_CONFIGFILE_CHUNK_T */
+	MMAL_PARAMETER_CONFIGFILE_CHUNK_REGISTERS,
+	MMAL_PARAMETER_JPEG_ATTACH_LOG, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_ZERO_SHUTTER_LAG, /**< @ref MMAL_PARAMETER_ZEROSHUTTERLAG_T */
+	MMAL_PARAMETER_FPS_RANGE, /**< @ref MMAL_PARAMETER_FPS_RANGE_T */
+	MMAL_PARAMETER_CAPTURE_EXPOSURE_COMP, /**< @ref MMAL_PARAMETER_INT32_T */
+
+	/* 0x40 */
+	MMAL_PARAMETER_SW_SHARPEN_DISABLE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_FLASH_REQUIRED, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_SW_SATURATION_DISABLE, /**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_SHUTTER_SPEED,             /**< Takes a @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_CUSTOM_AWB_GAINS,          /**< Takes a @ref MMAL_PARAMETER_AWB_GAINS_T */
+};
+
+struct mmal_parameter_rational {
+	s32 num;    /**< Numerator */
+	s32 den;    /**< Denominator */
+};
+
+enum mmal_parameter_camera_config_timestamp_mode {
+	MMAL_PARAM_TIMESTAMP_MODE_ZERO = 0, /* Always timestamp frames as 0 */
+	MMAL_PARAM_TIMESTAMP_MODE_RAW_STC,  /* Use the raw STC value
+					     * for the frame timestamp
+					     */
+	MMAL_PARAM_TIMESTAMP_MODE_RESET_STC, /* Use the STC timestamp
+					      * but subtract the
+					      * timestamp of the first
+					      * frame sent to give a
+					      * zero based timestamp.
+					      */
+};
+
+struct mmal_parameter_fps_range {
+	/**< Low end of the permitted framerate range */
+	struct mmal_parameter_rational	fps_low;
+	/**< High end of the permitted framerate range */
+	struct mmal_parameter_rational	fps_high;
+};
+
+
+/* camera configuration parameter */
+struct mmal_parameter_camera_config {
+	/* Parameters for setting up the image pools */
+	u32 max_stills_w; /* Max size of stills capture */
+	u32 max_stills_h;
+	u32 stills_yuv422; /* Allow YUV422 stills capture */
+	u32 one_shot_stills; /* Continuous or one shot stills captures. */
+
+	u32 max_preview_video_w; /* Max size of the preview or video
+				  * capture frames
+				  */
+	u32 max_preview_video_h;
+	u32 num_preview_video_frames;
+
+	/** Sets the height of the circular buffer for stills capture. */
+	u32 stills_capture_circular_buffer_height;
+
+	/** Allows preview/encode to resume as fast as possible after the stills
+	 * input frame has been received, and then processes the still frame in
+	 * the background whilst preview/encode has resumed.
+	 * Actual mode is controlled by MMAL_PARAMETER_CAPTURE_MODE.
+	 */
+	u32 fast_preview_resume;
+
+	/** Selects algorithm for timestamping frames if
+	 * there is no clock component connected.
+	 * enum mmal_parameter_camera_config_timestamp_mode
+	 */
+	s32 use_stc_timestamp;
+};
+
+
+enum mmal_parameter_exposuremode {
+	MMAL_PARAM_EXPOSUREMODE_OFF,
+	MMAL_PARAM_EXPOSUREMODE_AUTO,
+	MMAL_PARAM_EXPOSUREMODE_NIGHT,
+	MMAL_PARAM_EXPOSUREMODE_NIGHTPREVIEW,
+	MMAL_PARAM_EXPOSUREMODE_BACKLIGHT,
+	MMAL_PARAM_EXPOSUREMODE_SPOTLIGHT,
+	MMAL_PARAM_EXPOSUREMODE_SPORTS,
+	MMAL_PARAM_EXPOSUREMODE_SNOW,
+	MMAL_PARAM_EXPOSUREMODE_BEACH,
+	MMAL_PARAM_EXPOSUREMODE_VERYLONG,
+	MMAL_PARAM_EXPOSUREMODE_FIXEDFPS,
+	MMAL_PARAM_EXPOSUREMODE_ANTISHAKE,
+	MMAL_PARAM_EXPOSUREMODE_FIREWORKS,
+};
+
+enum mmal_parameter_exposuremeteringmode {
+	MMAL_PARAM_EXPOSUREMETERINGMODE_AVERAGE,
+	MMAL_PARAM_EXPOSUREMETERINGMODE_SPOT,
+	MMAL_PARAM_EXPOSUREMETERINGMODE_BACKLIT,
+	MMAL_PARAM_EXPOSUREMETERINGMODE_MATRIX,
+};
+
+enum mmal_parameter_awbmode {
+	MMAL_PARAM_AWBMODE_OFF,
+	MMAL_PARAM_AWBMODE_AUTO,
+	MMAL_PARAM_AWBMODE_SUNLIGHT,
+	MMAL_PARAM_AWBMODE_CLOUDY,
+	MMAL_PARAM_AWBMODE_SHADE,
+	MMAL_PARAM_AWBMODE_TUNGSTEN,
+	MMAL_PARAM_AWBMODE_FLUORESCENT,
+	MMAL_PARAM_AWBMODE_INCANDESCENT,
+	MMAL_PARAM_AWBMODE_FLASH,
+	MMAL_PARAM_AWBMODE_HORIZON,
+};
+
+enum mmal_parameter_imagefx {
+	MMAL_PARAM_IMAGEFX_NONE,
+	MMAL_PARAM_IMAGEFX_NEGATIVE,
+	MMAL_PARAM_IMAGEFX_SOLARIZE,
+	MMAL_PARAM_IMAGEFX_POSTERIZE,
+	MMAL_PARAM_IMAGEFX_WHITEBOARD,
+	MMAL_PARAM_IMAGEFX_BLACKBOARD,
+	MMAL_PARAM_IMAGEFX_SKETCH,
+	MMAL_PARAM_IMAGEFX_DENOISE,
+	MMAL_PARAM_IMAGEFX_EMBOSS,
+	MMAL_PARAM_IMAGEFX_OILPAINT,
+	MMAL_PARAM_IMAGEFX_HATCH,
+	MMAL_PARAM_IMAGEFX_GPEN,
+	MMAL_PARAM_IMAGEFX_PASTEL,
+	MMAL_PARAM_IMAGEFX_WATERCOLOUR,
+	MMAL_PARAM_IMAGEFX_FILM,
+	MMAL_PARAM_IMAGEFX_BLUR,
+	MMAL_PARAM_IMAGEFX_SATURATION,
+	MMAL_PARAM_IMAGEFX_COLOURSWAP,
+	MMAL_PARAM_IMAGEFX_WASHEDOUT,
+	MMAL_PARAM_IMAGEFX_POSTERISE,
+	MMAL_PARAM_IMAGEFX_COLOURPOINT,
+	MMAL_PARAM_IMAGEFX_COLOURBALANCE,
+	MMAL_PARAM_IMAGEFX_CARTOON,
+};
+
+enum MMAL_PARAM_FLICKERAVOID_T {
+	MMAL_PARAM_FLICKERAVOID_OFF,
+	MMAL_PARAM_FLICKERAVOID_AUTO,
+	MMAL_PARAM_FLICKERAVOID_50HZ,
+	MMAL_PARAM_FLICKERAVOID_60HZ,
+	MMAL_PARAM_FLICKERAVOID_MAX = 0x7FFFFFFF
+};
+
+struct mmal_parameter_awbgains {
+	struct mmal_parameter_rational r_gain;	/**< Red gain */
+	struct mmal_parameter_rational b_gain;	/**< Blue gain */
+};
+
+/** Manner of video rate control */
+enum mmal_parameter_rate_control_mode {
+	MMAL_VIDEO_RATECONTROL_DEFAULT,
+	MMAL_VIDEO_RATECONTROL_VARIABLE,
+	MMAL_VIDEO_RATECONTROL_CONSTANT,
+	MMAL_VIDEO_RATECONTROL_VARIABLE_SKIP_FRAMES,
+	MMAL_VIDEO_RATECONTROL_CONSTANT_SKIP_FRAMES
+};
+
+enum mmal_video_profile {
+	MMAL_VIDEO_PROFILE_H263_BASELINE,
+	MMAL_VIDEO_PROFILE_H263_H320CODING,
+	MMAL_VIDEO_PROFILE_H263_BACKWARDCOMPATIBLE,
+	MMAL_VIDEO_PROFILE_H263_ISWV2,
+	MMAL_VIDEO_PROFILE_H263_ISWV3,
+	MMAL_VIDEO_PROFILE_H263_HIGHCOMPRESSION,
+	MMAL_VIDEO_PROFILE_H263_INTERNET,
+	MMAL_VIDEO_PROFILE_H263_INTERLACE,
+	MMAL_VIDEO_PROFILE_H263_HIGHLATENCY,
+	MMAL_VIDEO_PROFILE_MP4V_SIMPLE,
+	MMAL_VIDEO_PROFILE_MP4V_SIMPLESCALABLE,
+	MMAL_VIDEO_PROFILE_MP4V_CORE,
+	MMAL_VIDEO_PROFILE_MP4V_MAIN,
+	MMAL_VIDEO_PROFILE_MP4V_NBIT,
+	MMAL_VIDEO_PROFILE_MP4V_SCALABLETEXTURE,
+	MMAL_VIDEO_PROFILE_MP4V_SIMPLEFACE,
+	MMAL_VIDEO_PROFILE_MP4V_SIMPLEFBA,
+	MMAL_VIDEO_PROFILE_MP4V_BASICANIMATED,
+	MMAL_VIDEO_PROFILE_MP4V_HYBRID,
+	MMAL_VIDEO_PROFILE_MP4V_ADVANCEDREALTIME,
+	MMAL_VIDEO_PROFILE_MP4V_CORESCALABLE,
+	MMAL_VIDEO_PROFILE_MP4V_ADVANCEDCODING,
+	MMAL_VIDEO_PROFILE_MP4V_ADVANCEDCORE,
+	MMAL_VIDEO_PROFILE_MP4V_ADVANCEDSCALABLE,
+	MMAL_VIDEO_PROFILE_MP4V_ADVANCEDSIMPLE,
+	MMAL_VIDEO_PROFILE_H264_BASELINE,
+	MMAL_VIDEO_PROFILE_H264_MAIN,
+	MMAL_VIDEO_PROFILE_H264_EXTENDED,
+	MMAL_VIDEO_PROFILE_H264_HIGH,
+	MMAL_VIDEO_PROFILE_H264_HIGH10,
+	MMAL_VIDEO_PROFILE_H264_HIGH422,
+	MMAL_VIDEO_PROFILE_H264_HIGH444,
+	MMAL_VIDEO_PROFILE_H264_CONSTRAINED_BASELINE,
+	MMAL_VIDEO_PROFILE_DUMMY = 0x7FFFFFFF
+};
+
+enum mmal_video_level {
+	MMAL_VIDEO_LEVEL_H263_10,
+	MMAL_VIDEO_LEVEL_H263_20,
+	MMAL_VIDEO_LEVEL_H263_30,
+	MMAL_VIDEO_LEVEL_H263_40,
+	MMAL_VIDEO_LEVEL_H263_45,
+	MMAL_VIDEO_LEVEL_H263_50,
+	MMAL_VIDEO_LEVEL_H263_60,
+	MMAL_VIDEO_LEVEL_H263_70,
+	MMAL_VIDEO_LEVEL_MP4V_0,
+	MMAL_VIDEO_LEVEL_MP4V_0b,
+	MMAL_VIDEO_LEVEL_MP4V_1,
+	MMAL_VIDEO_LEVEL_MP4V_2,
+	MMAL_VIDEO_LEVEL_MP4V_3,
+	MMAL_VIDEO_LEVEL_MP4V_4,
+	MMAL_VIDEO_LEVEL_MP4V_4a,
+	MMAL_VIDEO_LEVEL_MP4V_5,
+	MMAL_VIDEO_LEVEL_MP4V_6,
+	MMAL_VIDEO_LEVEL_H264_1,
+	MMAL_VIDEO_LEVEL_H264_1b,
+	MMAL_VIDEO_LEVEL_H264_11,
+	MMAL_VIDEO_LEVEL_H264_12,
+	MMAL_VIDEO_LEVEL_H264_13,
+	MMAL_VIDEO_LEVEL_H264_2,
+	MMAL_VIDEO_LEVEL_H264_21,
+	MMAL_VIDEO_LEVEL_H264_22,
+	MMAL_VIDEO_LEVEL_H264_3,
+	MMAL_VIDEO_LEVEL_H264_31,
+	MMAL_VIDEO_LEVEL_H264_32,
+	MMAL_VIDEO_LEVEL_H264_4,
+	MMAL_VIDEO_LEVEL_H264_41,
+	MMAL_VIDEO_LEVEL_H264_42,
+	MMAL_VIDEO_LEVEL_H264_5,
+	MMAL_VIDEO_LEVEL_H264_51,
+	MMAL_VIDEO_LEVEL_DUMMY = 0x7FFFFFFF
+};
+
+struct mmal_parameter_video_profile {
+	enum mmal_video_profile profile;
+	enum mmal_video_level level;
+};
+
+/* video parameters */
+
+enum mmal_parameter_video_type {
+	/** @ref MMAL_DISPLAYREGION_T */
+	MMAL_PARAMETER_DISPLAYREGION = MMAL_PARAMETER_GROUP_VIDEO,
+
+	/** @ref MMAL_PARAMETER_VIDEO_PROFILE_T */
+	MMAL_PARAMETER_SUPPORTED_PROFILES,
+
+	/** @ref MMAL_PARAMETER_VIDEO_PROFILE_T */
+	MMAL_PARAMETER_PROFILE,
+
+	/** @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_INTRAPERIOD,
+
+	/** @ref MMAL_PARAMETER_VIDEO_RATECONTROL_T */
+	MMAL_PARAMETER_RATECONTROL,
+
+	/** @ref MMAL_PARAMETER_VIDEO_NALUNITFORMAT_T */
+	MMAL_PARAMETER_NALUNITFORMAT,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_MINIMISE_FRAGMENTATION,
+
+	/** @ref MMAL_PARAMETER_UINT32_T.
+	 * Setting the value to zero resets to the default (one slice per frame).
+	 */
+	MMAL_PARAMETER_MB_ROWS_PER_SLICE,
+
+	/** @ref MMAL_PARAMETER_VIDEO_LEVEL_EXTENSION_T */
+	MMAL_PARAMETER_VIDEO_LEVEL_EXTENSION,
+
+	/** @ref MMAL_PARAMETER_VIDEO_EEDE_ENABLE_T */
+	MMAL_PARAMETER_VIDEO_EEDE_ENABLE,
+
+	/** @ref MMAL_PARAMETER_VIDEO_EEDE_LOSSRATE_T */
+	MMAL_PARAMETER_VIDEO_EEDE_LOSSRATE,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. Request an I-frame. */
+	MMAL_PARAMETER_VIDEO_REQUEST_I_FRAME,
+	/** @ref MMAL_PARAMETER_VIDEO_INTRA_REFRESH_T */
+	MMAL_PARAMETER_VIDEO_INTRA_REFRESH,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_IMMUTABLE_INPUT,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. Run-time bit rate control */
+	MMAL_PARAMETER_VIDEO_BIT_RATE,
+
+	/** @ref MMAL_PARAMETER_FRAME_RATE_T */
+	MMAL_PARAMETER_VIDEO_FRAME_RATE,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_MIN_QUANT,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_MAX_QUANT,
+
+	/** @ref MMAL_PARAMETER_VIDEO_ENCODE_RC_MODEL_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_RC_MODEL,
+
+	MMAL_PARAMETER_EXTRA_BUFFERS, /**< @ref MMAL_PARAMETER_UINT32_T. */
+	/** @ref MMAL_PARAMETER_UINT32_T.
+	 * Changing this parameter from the default can reduce frame rate
+	 * because image buffers need to be re-pitched.
+	 */
+	MMAL_PARAMETER_VIDEO_ALIGN_HORIZ,
+
+	/** @ref MMAL_PARAMETER_UINT32_T.
+	 * Changing this parameter from the default can reduce frame rate
+	 * because image buffers need to be re-pitched.
+	 */
+	MMAL_PARAMETER_VIDEO_ALIGN_VERT,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_DROPPABLE_PFRAMES,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_INITIAL_QUANT,
+
+	/**< @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_QP_P,
+
+	/**< @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_RC_SLICE_DQUANT,
+
+	/** @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_FRAME_LIMIT_BITS,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_PEAK_RATE,
+
+	/* H264 specific parameters */
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_DISABLE_CABAC,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_LOW_LATENCY,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_AU_DELIMITERS,
+
+	/** @ref MMAL_PARAMETER_UINT32_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_DEBLOCK_IDC,
+
+	/** @ref MMAL_PARAMETER_VIDEO_ENCODER_H264_MB_INTRA_MODES_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_MB_INTRA_MODE,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_HEADER_ON_OPEN,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_PRECODE_FOR_QP,
+
+	/** @ref MMAL_PARAMETER_VIDEO_DRM_INIT_INFO_T. */
+	MMAL_PARAMETER_VIDEO_DRM_INIT_INFO,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_TIMESTAMP_FIFO,
+
+	/** @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_DECODE_ERROR_CONCEALMENT,
+
+	/** @ref MMAL_PARAMETER_VIDEO_DRM_PROTECT_BUFFER_T. */
+	MMAL_PARAMETER_VIDEO_DRM_PROTECT_BUFFER,
+
+	/** @ref MMAL_PARAMETER_BYTES_T */
+	MMAL_PARAMETER_VIDEO_DECODE_CONFIG_VD3,
+
+	/**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_VCL_HRD_PARAMETERS,
+
+	/**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_H264_LOW_DELAY_HRD_FLAG,
+
+	/**< @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_INLINE_HEADER
+};
+
+/** Valid mirror modes */
+enum mmal_parameter_mirror {
+	MMAL_PARAM_MIRROR_NONE,
+	MMAL_PARAM_MIRROR_VERTICAL,
+	MMAL_PARAM_MIRROR_HORIZONTAL,
+	MMAL_PARAM_MIRROR_BOTH,
+};
+
+enum mmal_parameter_displaytransform {
+	MMAL_DISPLAY_ROT0 = 0,
+	MMAL_DISPLAY_MIRROR_ROT0 = 1,
+	MMAL_DISPLAY_MIRROR_ROT180 = 2,
+	MMAL_DISPLAY_ROT180 = 3,
+	MMAL_DISPLAY_MIRROR_ROT90 = 4,
+	MMAL_DISPLAY_ROT270 = 5,
+	MMAL_DISPLAY_ROT90 = 6,
+	MMAL_DISPLAY_MIRROR_ROT270 = 7,
+};
+
+enum mmal_parameter_displaymode {
+	MMAL_DISPLAY_MODE_FILL = 0,
+	MMAL_DISPLAY_MODE_LETTERBOX = 1,
+};
+
+enum mmal_parameter_displayset {
+	MMAL_DISPLAY_SET_NONE = 0,
+	MMAL_DISPLAY_SET_NUM = 1,
+	MMAL_DISPLAY_SET_FULLSCREEN = 2,
+	MMAL_DISPLAY_SET_TRANSFORM = 4,
+	MMAL_DISPLAY_SET_DEST_RECT = 8,
+	MMAL_DISPLAY_SET_SRC_RECT = 0x10,
+	MMAL_DISPLAY_SET_MODE = 0x20,
+	MMAL_DISPLAY_SET_PIXEL = 0x40,
+	MMAL_DISPLAY_SET_NOASPECT = 0x80,
+	MMAL_DISPLAY_SET_LAYER = 0x100,
+	MMAL_DISPLAY_SET_COPYPROTECT = 0x200,
+	MMAL_DISPLAY_SET_ALPHA = 0x400,
+};
+
+struct mmal_parameter_displayregion {
+	/** Bitfield that indicates which fields are set and should be
+	 * used. All other fields will maintain their current value.
+	 * \ref MMAL_DISPLAYSET_T defines the bits that can be
+	 * combined.
+	 */
+	u32 set;
+
+	/** Describes the display output device, with 0 typically
+	 * being a directly connected LCD display.  The actual values
+	 * will depend on the hardware.  Code using hard-wired numbers
+	 * (e.g. 2) is certain to fail.
+	 */
+
+	u32 display_num;
+	/** Indicates that we are using the full device screen area,
+	 * rather than a window of the display.  If zero, then
+	 * dest_rect is used to specify a region of the display to
+	 * use.
+	 */
+
+	s32 fullscreen;
+	/** Indicates any rotation or flipping used to map frames onto
+	 * the natural display orientation.
+	 */
+	u32 transform; /* enum mmal_parameter_displaytransform */
+
+	/** Where to display the frame within the screen, if
+	 * fullscreen is zero.
+	 */
+	struct vchiq_mmal_rect dest_rect;
+
+	/** Indicates which area of the frame to display. If all
+	 * values are zero, the whole frame will be used.
+	 */
+	struct vchiq_mmal_rect src_rect;
+
+	/** If set to non-zero, indicates that any display scaling
+	 * should disregard the aspect ratio of the frame region being
+	 * displayed.
+	 */
+	s32 noaspect;
+
+	/** Indicates how the image should be scaled to fit the
+	 * display. \code MMAL_DISPLAY_MODE_FILL \endcode indicates
+	 * that the image should fill the screen by potentially
+	 * cropping the frames.  Setting \code mode \endcode to \code
+	 * MMAL_DISPLAY_MODE_LETTERBOX \endcode indicates that all the
+	 * source region should be displayed and black bars added if
+	 * necessary.
+	 */
+	u32 mode; /* enum mmal_parameter_displaymode */
+
+	/** If non-zero, defines the width of a source pixel relative
+	 * to \code pixel_y \endcode.  If zero, then pixels default to
+	 * being square.
+	 */
+	u32 pixel_x;
+
+	/** If non-zero, defines the height of a source pixel relative
+	 * to \code pixel_x \endcode.  If zero, then pixels default to
+	 * being square.
+	 */
+	u32 pixel_y;
+
+	/** Sets the relative depth of the images, with greater values
+	 * being in front of smaller values.
+	 */
+	u32 layer;
+
+	/** Set to non-zero to ensure copy protection is used on
+	 * output.
+	 */
+	s32 copyprotect_required;
+
+	/** Level of opacity of the layer, where zero is fully
+	 * transparent and 255 is fully opaque.
+	 */
+	u32 alpha;
+};
+
+#define MMAL_MAX_IMAGEFX_PARAMETERS 5
+
+struct mmal_parameter_imagefx_parameters {
+	enum mmal_parameter_imagefx effect;
+	u32 num_effect_params;
+	u32 effect_parameter[MMAL_MAX_IMAGEFX_PARAMETERS];
+};
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-vchiq.c
@@ -0,0 +1,1916 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ *
+ * V4L2 driver MMAL vchiq interface code
+ */
+
+#define pr_fmt(fmt) KBUILD_MODNAME ": " fmt
+
+#include <linux/errno.h>
+#include <linux/kernel.h>
+#include <linux/mutex.h>
+#include <linux/mm.h>
+#include <linux/slab.h>
+#include <linux/completion.h>
+#include <linux/vmalloc.h>
+#include <asm/cacheflush.h>
+#include <media/videobuf2-vmalloc.h>
+
+#include "mmal-common.h"
+#include "mmal-vchiq.h"
+#include "mmal-msg.h"
+
+#define USE_VCHIQ_ARM
+#include "interface/vchi/vchi.h"
+
+/* maximum number of components supported */
+#define VCHIQ_MMAL_MAX_COMPONENTS 4
+
+/*#define FULL_MSG_DUMP 1*/
+
+#ifdef DEBUG
+static const char *const msg_type_names[] = {
+	"UNKNOWN",
+	"QUIT",
+	"SERVICE_CLOSED",
+	"GET_VERSION",
+	"COMPONENT_CREATE",
+	"COMPONENT_DESTROY",
+	"COMPONENT_ENABLE",
+	"COMPONENT_DISABLE",
+	"PORT_INFO_GET",
+	"PORT_INFO_SET",
+	"PORT_ACTION",
+	"BUFFER_FROM_HOST",
+	"BUFFER_TO_HOST",
+	"GET_STATS",
+	"PORT_PARAMETER_SET",
+	"PORT_PARAMETER_GET",
+	"EVENT_TO_HOST",
+	"GET_CORE_STATS_FOR_PORT",
+	"OPAQUE_ALLOCATOR",
+	"CONSUME_MEM",
+	"LMK",
+	"OPAQUE_ALLOCATOR_DESC",
+	"DRM_GET_LHS32",
+	"DRM_GET_TIME",
+	"BUFFER_FROM_HOST_ZEROLEN",
+	"PORT_FLUSH",
+	"HOST_LOG",
+};
+#endif
+
+static const char *const port_action_type_names[] = {
+	"UNKNOWN",
+	"ENABLE",
+	"DISABLE",
+	"FLUSH",
+	"CONNECT",
+	"DISCONNECT",
+	"SET_REQUIREMENTS",
+};
+
+#if defined(DEBUG)
+#if defined(FULL_MSG_DUMP)
+#define DBG_DUMP_MSG(MSG, MSG_LEN, TITLE)				\
+	do {								\
+		pr_debug(TITLE" type:%s(%d) length:%d\n",		\
+			 msg_type_names[(MSG)->h.type],			\
+			 (MSG)->h.type, (MSG_LEN));			\
+		print_hex_dump(KERN_DEBUG, "<<h: ", DUMP_PREFIX_OFFSET,	\
+			       16, 4, (MSG),				\
+			       sizeof(struct mmal_msg_header), 1);	\
+		print_hex_dump(KERN_DEBUG, "<<p: ", DUMP_PREFIX_OFFSET,	\
+			       16, 4,					\
+			       ((u8 *)(MSG)) + sizeof(struct mmal_msg_header),\
+			       (MSG_LEN) - sizeof(struct mmal_msg_header), 1); \
+	} while (0)
+#else
+#define DBG_DUMP_MSG(MSG, MSG_LEN, TITLE)				\
+	{								\
+		pr_debug(TITLE" type:%s(%d) length:%d\n",		\
+			 msg_type_names[(MSG)->h.type],			\
+			 (MSG)->h.type, (MSG_LEN));			\
+	}
+#endif
+#else
+#define DBG_DUMP_MSG(MSG, MSG_LEN, TITLE)
+#endif
+
+/* normal message context */
+struct mmal_msg_context {
+	union {
+		struct {
+			/* work struct for defered callback - must come first */
+			struct work_struct work;
+			/* mmal instance */
+			struct vchiq_mmal_instance *instance;
+			/* mmal port */
+			struct vchiq_mmal_port *port;
+			/* actual buffer used to store bulk reply */
+			struct mmal_buffer *buffer;
+			/* amount of buffer used */
+			unsigned long buffer_used;
+			/* MMAL buffer flags */
+			u32 mmal_flags;
+			/* Presentation and Decode timestamps */
+			s64 pts;
+			s64 dts;
+
+			int status;	/* context status */
+
+		} bulk;		/* bulk data */
+
+		struct {
+			/* message handle to release */
+			VCHI_HELD_MSG_T msg_handle;
+			/* pointer to received message */
+			struct mmal_msg *msg;
+			/* received message length */
+			u32 msg_len;
+			/* completion upon reply */
+			struct completion cmplt;
+		} sync;		/* synchronous response */
+	} u;
+
+};
+
+struct vchiq_mmal_instance {
+	VCHI_SERVICE_HANDLE_T handle;
+
+	/* ensure serialised access to service */
+	struct mutex vchiq_mutex;
+
+	/* ensure serialised access to bulk operations */
+	struct mutex bulk_mutex;
+
+	/* vmalloc page to receive scratch bulk xfers into */
+	void *bulk_scratch;
+
+	/* component to use next */
+	int component_idx;
+	struct vchiq_mmal_component component[VCHIQ_MMAL_MAX_COMPONENTS];
+};
+
+static struct mmal_msg_context *get_msg_context(struct vchiq_mmal_instance
+						*instance)
+{
+	struct mmal_msg_context *msg_context;
+
+	/* todo: should this be allocated from a pool to avoid kmalloc */
+	msg_context = kmalloc(sizeof(*msg_context), GFP_KERNEL);
+	memset(msg_context, 0, sizeof(*msg_context));
+
+	return msg_context;
+}
+
+static void release_msg_context(struct mmal_msg_context *msg_context)
+{
+	kfree(msg_context);
+}
+
+/* deals with receipt of event to host message */
+static void event_to_host_cb(struct vchiq_mmal_instance *instance,
+			     struct mmal_msg *msg, u32 msg_len)
+{
+	pr_debug("unhandled event\n");
+	pr_debug("component:%p port type:%d num:%d cmd:0x%x length:%d\n",
+		 msg->u.event_to_host.client_component,
+		 msg->u.event_to_host.port_type,
+		 msg->u.event_to_host.port_num,
+		 msg->u.event_to_host.cmd, msg->u.event_to_host.length);
+}
+
+/* workqueue scheduled callback
+ *
+ * we do this because it is important we do not call any other vchiq
+ * sync calls from witin the message delivery thread
+ */
+static void buffer_work_cb(struct work_struct *work)
+{
+	struct mmal_msg_context *msg_context = (struct mmal_msg_context *)work;
+
+	msg_context->u.bulk.port->buffer_cb(msg_context->u.bulk.instance,
+					    msg_context->u.bulk.port,
+					    msg_context->u.bulk.status,
+					    msg_context->u.bulk.buffer,
+					    msg_context->u.bulk.buffer_used,
+					    msg_context->u.bulk.mmal_flags,
+					    msg_context->u.bulk.dts,
+					    msg_context->u.bulk.pts);
+
+	/* release message context */
+	release_msg_context(msg_context);
+}
+
+/* enqueue a bulk receive for a given message context */
+static int bulk_receive(struct vchiq_mmal_instance *instance,
+			struct mmal_msg *msg,
+			struct mmal_msg_context *msg_context)
+{
+	unsigned long rd_len;
+	unsigned long flags = 0;
+	int ret;
+
+	/* bulk mutex stops other bulk operations while we have a
+	 * receive in progress - released in callback
+	 */
+	ret = mutex_lock_interruptible(&instance->bulk_mutex);
+	if (ret != 0)
+		return ret;
+
+	rd_len = msg->u.buffer_from_host.buffer_header.length;
+
+	/* take buffer from queue */
+	spin_lock_irqsave(&msg_context->u.bulk.port->slock, flags);
+	if (list_empty(&msg_context->u.bulk.port->buffers)) {
+		spin_unlock_irqrestore(&msg_context->u.bulk.port->slock, flags);
+		pr_err("buffer list empty trying to submit bulk receive\n");
+
+		/* todo: this is a serious error, we should never have
+		 * commited a buffer_to_host operation to the mmal
+		 * port without the buffer to back it up (underflow
+		 * handling) and there is no obvious way to deal with
+		 * this - how is the mmal servie going to react when
+		 * we fail to do the xfer and reschedule a buffer when
+		 * it arrives? perhaps a starved flag to indicate a
+		 * waiting bulk receive?
+		 */
+
+		mutex_unlock(&instance->bulk_mutex);
+
+		return -EINVAL;
+	}
+
+	msg_context->u.bulk.buffer =
+	    list_entry(msg_context->u.bulk.port->buffers.next,
+		       struct mmal_buffer, list);
+	list_del(&msg_context->u.bulk.buffer->list);
+
+	spin_unlock_irqrestore(&msg_context->u.bulk.port->slock, flags);
+
+	/* ensure we do not overrun the available buffer */
+	if (rd_len > msg_context->u.bulk.buffer->buffer_size) {
+		rd_len = msg_context->u.bulk.buffer->buffer_size;
+		pr_warn("short read as not enough receive buffer space\n");
+		/* todo: is this the correct response, what happens to
+		 * the rest of the message data?
+		 */
+	}
+
+	/* store length */
+	msg_context->u.bulk.buffer_used = rd_len;
+	msg_context->u.bulk.mmal_flags =
+	    msg->u.buffer_from_host.buffer_header.flags;
+	msg_context->u.bulk.dts = msg->u.buffer_from_host.buffer_header.dts;
+	msg_context->u.bulk.pts = msg->u.buffer_from_host.buffer_header.pts;
+
+	// only need to flush L1 cache here, as VCHIQ takes care of the L2
+	// cache.
+	__cpuc_flush_dcache_area(msg_context->u.bulk.buffer->buffer, rd_len);
+
+	/* queue the bulk submission */
+	vchi_service_use(instance->handle);
+	ret = vchi_bulk_queue_receive(instance->handle,
+				      msg_context->u.bulk.buffer->buffer,
+				      /* Actual receive needs to be a multiple
+				       * of 4 bytes
+				       */
+				      (rd_len + 3) & ~3,
+				      VCHI_FLAGS_CALLBACK_WHEN_OP_COMPLETE |
+				      VCHI_FLAGS_BLOCK_UNTIL_QUEUED,
+				      msg_context);
+
+	vchi_service_release(instance->handle);
+
+	if (ret != 0) {
+		/* callback will not be clearing the mutex */
+		mutex_unlock(&instance->bulk_mutex);
+	}
+
+	return ret;
+}
+
+/* enque a dummy bulk receive for a given message context */
+static int dummy_bulk_receive(struct vchiq_mmal_instance *instance,
+			      struct mmal_msg_context *msg_context)
+{
+	int ret;
+
+	/* bulk mutex stops other bulk operations while we have a
+	 * receive in progress - released in callback
+	 */
+	ret = mutex_lock_interruptible(&instance->bulk_mutex);
+	if (ret != 0)
+		return ret;
+
+	/* zero length indicates this was a dummy transfer */
+	msg_context->u.bulk.buffer_used = 0;
+
+	/* queue the bulk submission */
+	vchi_service_use(instance->handle);
+
+	ret = vchi_bulk_queue_receive(instance->handle,
+				      instance->bulk_scratch,
+				      8,
+				      VCHI_FLAGS_CALLBACK_WHEN_OP_COMPLETE |
+				      VCHI_FLAGS_BLOCK_UNTIL_QUEUED,
+				      msg_context);
+
+	vchi_service_release(instance->handle);
+
+	if (ret != 0) {
+		/* callback will not be clearing the mutex */
+		mutex_unlock(&instance->bulk_mutex);
+	}
+
+	return ret;
+}
+
+/* data in message, memcpy from packet into output buffer */
+static int inline_receive(struct vchiq_mmal_instance *instance,
+			  struct mmal_msg *msg,
+			  struct mmal_msg_context *msg_context)
+{
+	unsigned long flags = 0;
+
+	/* take buffer from queue */
+	spin_lock_irqsave(&msg_context->u.bulk.port->slock, flags);
+	if (list_empty(&msg_context->u.bulk.port->buffers)) {
+		spin_unlock_irqrestore(&msg_context->u.bulk.port->slock, flags);
+		pr_err("buffer list empty trying to receive inline\n");
+
+		/* todo: this is a serious error, we should never have
+		 * commited a buffer_to_host operation to the mmal
+		 * port without the buffer to back it up (with
+		 * underflow handling) and there is no obvious way to
+		 * deal with this. Less bad than the bulk case as we
+		 * can just drop this on the floor but...unhelpful
+		 */
+		return -EINVAL;
+	}
+
+	msg_context->u.bulk.buffer =
+	    list_entry(msg_context->u.bulk.port->buffers.next,
+		       struct mmal_buffer, list);
+	list_del(&msg_context->u.bulk.buffer->list);
+
+	spin_unlock_irqrestore(&msg_context->u.bulk.port->slock, flags);
+
+	memcpy(msg_context->u.bulk.buffer->buffer,
+	       msg->u.buffer_from_host.short_data,
+	       msg->u.buffer_from_host.payload_in_message);
+
+	msg_context->u.bulk.buffer_used =
+	    msg->u.buffer_from_host.payload_in_message;
+
+	return 0;
+}
+
+/* queue the buffer availability with MMAL_MSG_TYPE_BUFFER_FROM_HOST */
+static int
+buffer_from_host(struct vchiq_mmal_instance *instance,
+		 struct vchiq_mmal_port *port, struct mmal_buffer *buf)
+{
+	struct mmal_msg_context *msg_context;
+	struct mmal_msg m;
+	int ret;
+
+	pr_debug("instance:%p buffer:%p\n", instance->handle, buf);
+
+	/* bulk mutex stops other bulk operations while we
+	 * have a receive in progress
+	 */
+	if (mutex_lock_interruptible(&instance->bulk_mutex))
+		return -EINTR;
+
+	/* get context */
+	msg_context = get_msg_context(instance);
+	if (msg_context == NULL)
+		return -ENOMEM;
+
+	/* store bulk message context for when data arrives */
+	msg_context->u.bulk.instance = instance;
+	msg_context->u.bulk.port = port;
+	msg_context->u.bulk.buffer = NULL;	/* not valid until bulk xfer */
+	msg_context->u.bulk.buffer_used = 0;
+
+	/* initialise work structure ready to schedule callback */
+	INIT_WORK(&msg_context->u.bulk.work, buffer_work_cb);
+
+	/* prep the buffer from host message */
+	memset(&m, 0xbc, sizeof(m));	/* just to make debug clearer */
+
+	m.h.type = MMAL_MSG_TYPE_BUFFER_FROM_HOST;
+	m.h.magic = MMAL_MAGIC;
+	m.h.context = msg_context;
+	m.h.status = 0;
+
+	/* drvbuf is our private data passed back */
+	m.u.buffer_from_host.drvbuf.magic = MMAL_MAGIC;
+	m.u.buffer_from_host.drvbuf.component_handle = port->component->handle;
+	m.u.buffer_from_host.drvbuf.port_handle = port->handle;
+	m.u.buffer_from_host.drvbuf.client_context = msg_context;
+
+	/* buffer header */
+	m.u.buffer_from_host.buffer_header.cmd = 0;
+	m.u.buffer_from_host.buffer_header.data = buf->buffer;
+	m.u.buffer_from_host.buffer_header.alloc_size = buf->buffer_size;
+	m.u.buffer_from_host.buffer_header.length = 0;	/* nothing used yet */
+	m.u.buffer_from_host.buffer_header.offset = 0;	/* no offset */
+	m.u.buffer_from_host.buffer_header.flags = 0;	/* no flags */
+	m.u.buffer_from_host.buffer_header.pts = MMAL_TIME_UNKNOWN;
+	m.u.buffer_from_host.buffer_header.dts = MMAL_TIME_UNKNOWN;
+
+	/* clear buffer type sepecific data */
+	memset(&m.u.buffer_from_host.buffer_header_type_specific, 0,
+	       sizeof(m.u.buffer_from_host.buffer_header_type_specific));
+
+	/* no payload in message */
+	m.u.buffer_from_host.payload_in_message = 0;
+
+	vchi_service_use(instance->handle);
+
+	ret = vchi_msg_queue(instance->handle, &m,
+			     sizeof(struct mmal_msg_header) +
+			     sizeof(m.u.buffer_from_host),
+			     VCHI_FLAGS_BLOCK_UNTIL_QUEUED, NULL);
+
+	if (ret != 0) {
+		release_msg_context(msg_context);
+		/* todo: is this correct error value? */
+	}
+
+	vchi_service_release(instance->handle);
+
+	mutex_unlock(&instance->bulk_mutex);
+
+	return ret;
+}
+
+/* submit a buffer to the mmal sevice
+ *
+ * the buffer_from_host uses size data from the ports next available
+ * mmal_buffer and deals with there being no buffer available by
+ * incrementing the underflow for later
+ */
+static int port_buffer_from_host(struct vchiq_mmal_instance *instance,
+				 struct vchiq_mmal_port *port)
+{
+	int ret;
+	struct mmal_buffer *buf;
+	unsigned long flags = 0;
+
+	if (!port->enabled)
+		return -EINVAL;
+
+	/* peek buffer from queue */
+	spin_lock_irqsave(&port->slock, flags);
+	if (list_empty(&port->buffers)) {
+		port->buffer_underflow++;
+		spin_unlock_irqrestore(&port->slock, flags);
+		return -ENOSPC;
+	}
+
+	buf = list_entry(port->buffers.next, struct mmal_buffer, list);
+
+	spin_unlock_irqrestore(&port->slock, flags);
+
+	/* issue buffer to mmal service */
+	ret = buffer_from_host(instance, port, buf);
+	if (ret) {
+		pr_err("adding buffer header failed\n");
+		/* todo: how should this be dealt with */
+	}
+
+	return ret;
+}
+
+/* deals with receipt of buffer to host message */
+static void buffer_to_host_cb(struct vchiq_mmal_instance *instance,
+			      struct mmal_msg *msg, u32 msg_len)
+{
+	struct mmal_msg_context *msg_context;
+
+	pr_debug("buffer_to_host_cb: instance:%p msg:%p msg_len:%d\n",
+		 instance, msg, msg_len);
+
+	if (msg->u.buffer_from_host.drvbuf.magic == MMAL_MAGIC) {
+		msg_context = msg->u.buffer_from_host.drvbuf.client_context;
+	} else {
+		pr_err("MMAL_MSG_TYPE_BUFFER_TO_HOST with bad magic\n");
+		return;
+	}
+
+	if (msg->h.status != MMAL_MSG_STATUS_SUCCESS) {
+		/* message reception had an error */
+		pr_warn("error %d in reply\n", msg->h.status);
+
+		msg_context->u.bulk.status = msg->h.status;
+
+	} else if (msg->u.buffer_from_host.buffer_header.length == 0) {
+		/* empty buffer */
+		if (msg->u.buffer_from_host.buffer_header.flags &
+		    MMAL_BUFFER_HEADER_FLAG_EOS) {
+			msg_context->u.bulk.status =
+			    dummy_bulk_receive(instance, msg_context);
+			if (msg_context->u.bulk.status == 0)
+				return;	/* successful bulk submission, bulk
+					 * completion will trigger callback
+					 */
+		} else {
+			/* do callback with empty buffer - not EOS though */
+			msg_context->u.bulk.status = 0;
+			msg_context->u.bulk.buffer_used = 0;
+		}
+	} else if (msg->u.buffer_from_host.payload_in_message == 0) {
+		/* data is not in message, queue a bulk receive */
+		msg_context->u.bulk.status =
+		    bulk_receive(instance, msg, msg_context);
+		if (msg_context->u.bulk.status == 0)
+			return;	/* successful bulk submission, bulk
+				 * completion will trigger callback
+				 */
+
+		/* failed to submit buffer, this will end badly */
+		pr_err("error %d on bulk submission\n",
+		       msg_context->u.bulk.status);
+
+	} else if (msg->u.buffer_from_host.payload_in_message <=
+		   MMAL_VC_SHORT_DATA) {
+		/* data payload within message */
+		msg_context->u.bulk.status = inline_receive(instance, msg,
+							    msg_context);
+	} else {
+		pr_err("message with invalid short payload\n");
+
+		/* signal error */
+		msg_context->u.bulk.status = -EINVAL;
+		msg_context->u.bulk.buffer_used =
+		    msg->u.buffer_from_host.payload_in_message;
+	}
+
+	/* replace the buffer header */
+	port_buffer_from_host(instance, msg_context->u.bulk.port);
+
+	/* schedule the port callback */
+	schedule_work(&msg_context->u.bulk.work);
+}
+
+static void bulk_receive_cb(struct vchiq_mmal_instance *instance,
+			    struct mmal_msg_context *msg_context)
+{
+	/* bulk receive operation complete */
+	mutex_unlock(&msg_context->u.bulk.instance->bulk_mutex);
+
+	/* replace the buffer header */
+	port_buffer_from_host(msg_context->u.bulk.instance,
+			      msg_context->u.bulk.port);
+
+	msg_context->u.bulk.status = 0;
+
+	/* schedule the port callback */
+	schedule_work(&msg_context->u.bulk.work);
+}
+
+static void bulk_abort_cb(struct vchiq_mmal_instance *instance,
+			  struct mmal_msg_context *msg_context)
+{
+	pr_err("%s: bulk ABORTED msg_context:%p\n", __func__, msg_context);
+
+	/* bulk receive operation complete */
+	mutex_unlock(&msg_context->u.bulk.instance->bulk_mutex);
+
+	/* replace the buffer header */
+	port_buffer_from_host(msg_context->u.bulk.instance,
+			      msg_context->u.bulk.port);
+
+	msg_context->u.bulk.status = -EINTR;
+
+	schedule_work(&msg_context->u.bulk.work);
+}
+
+/* incoming event service callback */
+static void service_callback(void *param,
+			     const VCHI_CALLBACK_REASON_T reason,
+			     void *bulk_ctx)
+{
+	struct vchiq_mmal_instance *instance = param;
+	int status;
+	u32 msg_len;
+	struct mmal_msg *msg;
+	VCHI_HELD_MSG_T msg_handle;
+
+	if (!instance) {
+		pr_err("Message callback passed NULL instance\n");
+		return;
+	}
+
+	switch (reason) {
+	case VCHI_CALLBACK_MSG_AVAILABLE:
+		status = vchi_msg_hold(instance->handle, (void **)&msg,
+				       &msg_len, VCHI_FLAGS_NONE, &msg_handle);
+		if (status) {
+			pr_err("Unable to dequeue a message (%d)\n", status);
+			break;
+		}
+
+		DBG_DUMP_MSG(msg, msg_len, "<<< reply message");
+
+		/* handling is different for buffer messages */
+		switch (msg->h.type) {
+
+		case MMAL_MSG_TYPE_BUFFER_FROM_HOST:
+			vchi_held_msg_release(&msg_handle);
+			break;
+
+		case MMAL_MSG_TYPE_EVENT_TO_HOST:
+			event_to_host_cb(instance, msg, msg_len);
+			vchi_held_msg_release(&msg_handle);
+
+			break;
+
+		case MMAL_MSG_TYPE_BUFFER_TO_HOST:
+			buffer_to_host_cb(instance, msg, msg_len);
+			vchi_held_msg_release(&msg_handle);
+			break;
+
+		default:
+			/* messages dependant on header context to complete */
+
+			/* todo: the msg.context really ought to be sanity
+			 * checked before we just use it, afaict it comes back
+			 * and is used raw from the videocore. Perhaps it
+			 * should be verified the address lies in the kernel
+			 * address space.
+			 */
+			if (msg->h.context == NULL) {
+				pr_err("received message context was null!\n");
+				vchi_held_msg_release(&msg_handle);
+				break;
+			}
+
+			/* fill in context values */
+			msg->h.context->u.sync.msg_handle = msg_handle;
+			msg->h.context->u.sync.msg = msg;
+			msg->h.context->u.sync.msg_len = msg_len;
+
+			/* todo: should this check (completion_done()
+			 * == 1) for no one waiting? or do we need a
+			 * flag to tell us the completion has been
+			 * interrupted so we can free the message and
+			 * its context. This probably also solves the
+			 * message arriving after interruption todo
+			 * below
+			 */
+
+			/* complete message so caller knows it happened */
+			complete(&msg->h.context->u.sync.cmplt);
+			break;
+		}
+
+		break;
+
+	case VCHI_CALLBACK_BULK_RECEIVED:
+		bulk_receive_cb(instance, bulk_ctx);
+		break;
+
+	case VCHI_CALLBACK_BULK_RECEIVE_ABORTED:
+		bulk_abort_cb(instance, bulk_ctx);
+		break;
+
+	case VCHI_CALLBACK_SERVICE_CLOSED:
+		/* TODO: consider if this requires action if received when
+		 * driver is not explicitly closing the service
+		 */
+		break;
+
+	default:
+		pr_err("Received unhandled message reason %d\n", reason);
+		break;
+	}
+}
+
+static int send_synchronous_mmal_msg(struct vchiq_mmal_instance *instance,
+				     struct mmal_msg *msg,
+				     unsigned int payload_len,
+				     struct mmal_msg **msg_out,
+				     VCHI_HELD_MSG_T *msg_handle_out)
+{
+	struct mmal_msg_context msg_context;
+	int ret;
+
+	/* payload size must not cause message to exceed max size */
+	if (payload_len >
+	    (MMAL_MSG_MAX_SIZE - sizeof(struct mmal_msg_header))) {
+		pr_err("payload length %d exceeds max:%d\n", payload_len,
+			 (MMAL_MSG_MAX_SIZE - sizeof(struct mmal_msg_header)));
+		return -EINVAL;
+	}
+
+	init_completion(&msg_context.u.sync.cmplt);
+
+	msg->h.magic = MMAL_MAGIC;
+	msg->h.context = &msg_context;
+	msg->h.status = 0;
+
+	DBG_DUMP_MSG(msg, (sizeof(struct mmal_msg_header) + payload_len),
+		     ">>> sync message");
+
+	vchi_service_use(instance->handle);
+
+	ret = vchi_msg_queue(instance->handle,
+			     msg,
+			     sizeof(struct mmal_msg_header) + payload_len,
+			     VCHI_FLAGS_BLOCK_UNTIL_QUEUED, NULL);
+
+	vchi_service_release(instance->handle);
+
+	if (ret) {
+		pr_err("error %d queuing message\n", ret);
+		return ret;
+	}
+
+	ret = wait_for_completion_timeout(&msg_context.u.sync.cmplt, 3*HZ);
+	if (ret <= 0) {
+		pr_err("error %d waiting for sync completion\n", ret);
+		if (ret == 0)
+			ret = -ETIME;
+		/* todo: what happens if the message arrives after aborting */
+		return ret;
+	}
+
+	*msg_out = msg_context.u.sync.msg;
+	*msg_handle_out = msg_context.u.sync.msg_handle;
+
+	return 0;
+}
+
+static void dump_port_info(struct vchiq_mmal_port *port)
+{
+	pr_debug("port handle:0x%x enabled:%d\n", port->handle, port->enabled);
+
+	pr_debug("buffer minimum num:%d size:%d align:%d\n",
+		 port->minimum_buffer.num,
+		 port->minimum_buffer.size, port->minimum_buffer.alignment);
+
+	pr_debug("buffer recommended num:%d size:%d align:%d\n",
+		 port->recommended_buffer.num,
+		 port->recommended_buffer.size,
+		 port->recommended_buffer.alignment);
+
+	pr_debug("buffer current values num:%d size:%d align:%d\n",
+		 port->current_buffer.num,
+		 port->current_buffer.size, port->current_buffer.alignment);
+
+	pr_debug("elementry stream: type:%d encoding:0x%x varient:0x%x\n",
+		 port->format.type,
+		 port->format.encoding, port->format.encoding_variant);
+
+	pr_debug("		    bitrate:%d flags:0x%x\n",
+		 port->format.bitrate, port->format.flags);
+
+	if (port->format.type == MMAL_ES_TYPE_VIDEO) {
+		pr_debug
+		    ("es video format: width:%d height:%d colourspace:0x%x\n",
+		     port->es.video.width, port->es.video.height,
+		     port->es.video.color_space);
+
+		pr_debug("		 : crop xywh %d,%d,%d,%d\n",
+			 port->es.video.crop.x,
+			 port->es.video.crop.y,
+			 port->es.video.crop.width, port->es.video.crop.height);
+		pr_debug("		 : framerate %d/%d  aspect %d/%d\n",
+			 port->es.video.frame_rate.num,
+			 port->es.video.frame_rate.den,
+			 port->es.video.par.num, port->es.video.par.den);
+	}
+}
+
+static void port_to_mmal_msg(struct vchiq_mmal_port *port, struct mmal_port *p)
+{
+
+	/* todo do readonly fields need setting at all? */
+	p->type = port->type;
+	p->index = port->index;
+	p->index_all = 0;
+	p->is_enabled = port->enabled;
+	p->buffer_num_min = port->minimum_buffer.num;
+	p->buffer_size_min = port->minimum_buffer.size;
+	p->buffer_alignment_min = port->minimum_buffer.alignment;
+	p->buffer_num_recommended = port->recommended_buffer.num;
+	p->buffer_size_recommended = port->recommended_buffer.size;
+
+	/* only three writable fields in a port */
+	p->buffer_num = port->current_buffer.num;
+	p->buffer_size = port->current_buffer.size;
+	p->userdata = port;
+}
+
+static int port_info_set(struct vchiq_mmal_instance *instance,
+			 struct vchiq_mmal_port *port)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	pr_debug("setting port info port %p\n", port);
+	if (!port)
+		return -1;
+	dump_port_info(port);
+
+	m.h.type = MMAL_MSG_TYPE_PORT_INFO_SET;
+
+	m.u.port_info_set.component_handle = port->component->handle;
+	m.u.port_info_set.port_type = port->type;
+	m.u.port_info_set.port_index = port->index;
+
+	port_to_mmal_msg(port, &m.u.port_info_set.port);
+
+	/* elementry stream format setup */
+	m.u.port_info_set.format.type = port->format.type;
+	m.u.port_info_set.format.encoding = port->format.encoding;
+	m.u.port_info_set.format.encoding_variant =
+	    port->format.encoding_variant;
+	m.u.port_info_set.format.bitrate = port->format.bitrate;
+	m.u.port_info_set.format.flags = port->format.flags;
+
+	memcpy(&m.u.port_info_set.es, &port->es,
+	       sizeof(union mmal_es_specific_format));
+
+	m.u.port_info_set.format.extradata_size = port->format.extradata_size;
+	memcpy(&m.u.port_info_set.extradata, port->format.extradata,
+	       port->format.extradata_size);
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.port_info_set),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_INFO_SET) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	/* return operation status */
+	ret = -rmsg->u.port_info_get_reply.status;
+
+	pr_debug("%s:result:%d component:0x%x port:%d\n", __func__, ret,
+		 port->component->handle, port->handle);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+
+}
+
+/* use port info get message to retrive port information */
+static int port_info_get(struct vchiq_mmal_instance *instance,
+			 struct vchiq_mmal_port *port)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	/* port info time */
+	m.h.type = MMAL_MSG_TYPE_PORT_INFO_GET;
+	m.u.port_info_get.component_handle = port->component->handle;
+	m.u.port_info_get.port_type = port->type;
+	m.u.port_info_get.index = port->index;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.port_info_get),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_INFO_GET) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	/* return operation status */
+	ret = -rmsg->u.port_info_get_reply.status;
+	if (ret != MMAL_MSG_STATUS_SUCCESS)
+		goto release_msg;
+
+	if (rmsg->u.port_info_get_reply.port.is_enabled == 0)
+		port->enabled = false;
+	else
+		port->enabled = true;
+
+	/* copy the values out of the message */
+	port->handle = rmsg->u.port_info_get_reply.port_handle;
+
+	/* port type and index cached to use on port info set becuase
+	 * it does not use a port handle
+	 */
+	port->type = rmsg->u.port_info_get_reply.port_type;
+	port->index = rmsg->u.port_info_get_reply.port_index;
+
+	port->minimum_buffer.num =
+	    rmsg->u.port_info_get_reply.port.buffer_num_min;
+	port->minimum_buffer.size =
+	    rmsg->u.port_info_get_reply.port.buffer_size_min;
+	port->minimum_buffer.alignment =
+	    rmsg->u.port_info_get_reply.port.buffer_alignment_min;
+
+	port->recommended_buffer.alignment =
+	    rmsg->u.port_info_get_reply.port.buffer_alignment_min;
+	port->recommended_buffer.num =
+	    rmsg->u.port_info_get_reply.port.buffer_num_recommended;
+
+	port->current_buffer.num = rmsg->u.port_info_get_reply.port.buffer_num;
+	port->current_buffer.size =
+	    rmsg->u.port_info_get_reply.port.buffer_size;
+
+	/* stream format */
+	port->format.type = rmsg->u.port_info_get_reply.format.type;
+	port->format.encoding = rmsg->u.port_info_get_reply.format.encoding;
+	port->format.encoding_variant =
+	    rmsg->u.port_info_get_reply.format.encoding_variant;
+	port->format.bitrate = rmsg->u.port_info_get_reply.format.bitrate;
+	port->format.flags = rmsg->u.port_info_get_reply.format.flags;
+
+	/* elementry stream format */
+	memcpy(&port->es,
+	       &rmsg->u.port_info_get_reply.es,
+	       sizeof(union mmal_es_specific_format));
+	port->format.es = &port->es;
+
+	port->format.extradata_size =
+	    rmsg->u.port_info_get_reply.format.extradata_size;
+	memcpy(port->format.extradata,
+	       rmsg->u.port_info_get_reply.extradata,
+	       port->format.extradata_size);
+
+	pr_debug("received port info\n");
+	dump_port_info(port);
+
+release_msg:
+
+	pr_debug("%s:result:%d component:0x%x port:%d\n",
+		 __func__, ret, port->component->handle, port->handle);
+
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* create comonent on vc */
+static int create_component(struct vchiq_mmal_instance *instance,
+			    struct vchiq_mmal_component *component,
+			    const char *name)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	/* build component create message */
+	m.h.type = MMAL_MSG_TYPE_COMPONENT_CREATE;
+	m.u.component_create.client_component = component;
+	strncpy(m.u.component_create.name, name,
+		sizeof(m.u.component_create.name));
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.component_create),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != m.h.type) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.component_create_reply.status;
+	if (ret != MMAL_MSG_STATUS_SUCCESS)
+		goto release_msg;
+
+	/* a valid component response received */
+	component->handle = rmsg->u.component_create_reply.component_handle;
+	component->inputs = rmsg->u.component_create_reply.input_num;
+	component->outputs = rmsg->u.component_create_reply.output_num;
+	component->clocks = rmsg->u.component_create_reply.clock_num;
+
+	pr_debug("Component handle:0x%x in:%d out:%d clock:%d\n",
+		 component->handle,
+		 component->inputs, component->outputs, component->clocks);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* destroys a component on vc */
+static int destroy_component(struct vchiq_mmal_instance *instance,
+			     struct vchiq_mmal_component *component)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_COMPONENT_DESTROY;
+	m.u.component_destroy.component_handle = component->handle;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.component_destroy),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != m.h.type) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.component_destroy_reply.status;
+
+release_msg:
+
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* enable a component on vc */
+static int enable_component(struct vchiq_mmal_instance *instance,
+			    struct vchiq_mmal_component *component)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_COMPONENT_ENABLE;
+	m.u.component_enable.component_handle = component->handle;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.component_enable),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != m.h.type) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.component_enable_reply.status;
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* disable a component on vc */
+static int disable_component(struct vchiq_mmal_instance *instance,
+			     struct vchiq_mmal_component *component)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_COMPONENT_DISABLE;
+	m.u.component_disable.component_handle = component->handle;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.component_disable),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != m.h.type) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.component_disable_reply.status;
+
+release_msg:
+
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* get version of mmal implementation */
+static int get_version(struct vchiq_mmal_instance *instance,
+		       u32 *major_out, u32 *minor_out)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_GET_VERSION;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.version),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != m.h.type) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	*major_out = rmsg->u.version.major;
+	*minor_out = rmsg->u.version.minor;
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* do a port action with a port as a parameter */
+static int port_action_port(struct vchiq_mmal_instance *instance,
+			    struct vchiq_mmal_port *port,
+			    enum mmal_msg_port_action_type action_type)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_PORT_ACTION;
+	m.u.port_action_port.component_handle = port->component->handle;
+	m.u.port_action_port.port_handle = port->handle;
+	m.u.port_action_port.action = action_type;
+
+	port_to_mmal_msg(port, &m.u.port_action_port.port);
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.port_action_port),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_ACTION) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.port_action_reply.status;
+
+	pr_debug("%s:result:%d component:0x%x port:%d action:%s(%d)\n",
+		 __func__,
+		 ret, port->component->handle, port->handle,
+		 port_action_type_names[action_type], action_type);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* do a port action with handles as parameters */
+static int port_action_handle(struct vchiq_mmal_instance *instance,
+			      struct vchiq_mmal_port *port,
+			      enum mmal_msg_port_action_type action_type,
+			      u32 connect_component_handle,
+			      u32 connect_port_handle)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_PORT_ACTION;
+
+	m.u.port_action_handle.component_handle = port->component->handle;
+	m.u.port_action_handle.port_handle = port->handle;
+	m.u.port_action_handle.action = action_type;
+
+	m.u.port_action_handle.connect_component_handle =
+	    connect_component_handle;
+	m.u.port_action_handle.connect_port_handle = connect_port_handle;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(m.u.port_action_handle),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_ACTION) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.port_action_reply.status;
+
+	pr_debug("%s:result:%d component:0x%x port:%d action:%s(%d)" \
+		 " connect component:0x%x connect port:%d\n",
+		 __func__,
+		 ret, port->component->handle, port->handle,
+		 port_action_type_names[action_type],
+		 action_type, connect_component_handle, connect_port_handle);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+static int port_parameter_set(struct vchiq_mmal_instance *instance,
+			      struct vchiq_mmal_port *port,
+			      u32 parameter_id, void *value, u32 value_size)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_PORT_PARAMETER_SET;
+
+	m.u.port_parameter_set.component_handle = port->component->handle;
+	m.u.port_parameter_set.port_handle = port->handle;
+	m.u.port_parameter_set.id = parameter_id;
+	m.u.port_parameter_set.size = (2 * sizeof(u32)) + value_size;
+	memcpy(&m.u.port_parameter_set.value, value, value_size);
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					(4 * sizeof(u32)) + value_size,
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_PARAMETER_SET) {
+		/* got an unexpected message type in reply */
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.port_parameter_set_reply.status;
+
+	pr_debug("%s:result:%d component:0x%x port:%d parameter:%d\n",
+		 __func__,
+		 ret, port->component->handle, port->handle, parameter_id);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+static int port_parameter_get(struct vchiq_mmal_instance *instance,
+			      struct vchiq_mmal_port *port,
+			      u32 parameter_id, void *value, u32 *value_size)
+{
+	int ret;
+	struct mmal_msg m;
+	struct mmal_msg *rmsg;
+	VCHI_HELD_MSG_T rmsg_handle;
+
+	m.h.type = MMAL_MSG_TYPE_PORT_PARAMETER_GET;
+
+	m.u.port_parameter_get.component_handle = port->component->handle;
+	m.u.port_parameter_get.port_handle = port->handle;
+	m.u.port_parameter_get.id = parameter_id;
+	m.u.port_parameter_get.size = (2 * sizeof(u32)) + *value_size;
+
+	ret = send_synchronous_mmal_msg(instance, &m,
+					sizeof(struct
+					       mmal_msg_port_parameter_get),
+					&rmsg, &rmsg_handle);
+	if (ret)
+		return ret;
+
+	if (rmsg->h.type != MMAL_MSG_TYPE_PORT_PARAMETER_GET) {
+		/* got an unexpected message type in reply */
+		pr_err("Incorrect reply type %d\n", rmsg->h.type);
+		ret = -EINVAL;
+		goto release_msg;
+	}
+
+	ret = -rmsg->u.port_parameter_get_reply.status;
+	if (ret) {
+		/* Copy only as much as we have space for
+		 * but report true size of parameter
+		 */
+		memcpy(value, &rmsg->u.port_parameter_get_reply.value,
+		       *value_size);
+		*value_size = rmsg->u.port_parameter_get_reply.size;
+	} else
+		memcpy(value, &rmsg->u.port_parameter_get_reply.value,
+		       rmsg->u.port_parameter_get_reply.size);
+
+	pr_debug("%s:result:%d component:0x%x port:%d parameter:%d\n", __func__,
+	        ret, port->component->handle, port->handle, parameter_id);
+
+release_msg:
+	vchi_held_msg_release(&rmsg_handle);
+
+	return ret;
+}
+
+/* disables a port and drains buffers from it */
+static int port_disable(struct vchiq_mmal_instance *instance,
+			struct vchiq_mmal_port *port)
+{
+	int ret;
+	struct list_head *q, *buf_head;
+	unsigned long flags = 0;
+
+	if (!port->enabled)
+		return 0;
+
+	port->enabled = false;
+
+	ret = port_action_port(instance, port,
+			       MMAL_MSG_PORT_ACTION_TYPE_DISABLE);
+	if (ret == 0) {
+
+		/* drain all queued buffers on port */
+		spin_lock_irqsave(&port->slock, flags);
+
+		list_for_each_safe(buf_head, q, &port->buffers) {
+			struct mmal_buffer *mmalbuf;
+			mmalbuf = list_entry(buf_head, struct mmal_buffer,
+					     list);
+			list_del(buf_head);
+			if (port->buffer_cb)
+				port->buffer_cb(instance,
+						port, 0, mmalbuf, 0, 0,
+						MMAL_TIME_UNKNOWN,
+						MMAL_TIME_UNKNOWN);
+		}
+
+		spin_unlock_irqrestore(&port->slock, flags);
+
+		ret = port_info_get(instance, port);
+	}
+
+	return ret;
+}
+
+/* enable a port */
+static int port_enable(struct vchiq_mmal_instance *instance,
+		       struct vchiq_mmal_port *port)
+{
+	unsigned int hdr_count;
+	struct list_head *buf_head;
+	int ret;
+
+	if (port->enabled)
+		return 0;
+
+	/* ensure there are enough buffers queued to cover the buffer headers */
+	if (port->buffer_cb != NULL) {
+		hdr_count = 0;
+		list_for_each(buf_head, &port->buffers) {
+			hdr_count++;
+		}
+		if (hdr_count < port->current_buffer.num)
+			return -ENOSPC;
+	}
+
+	ret = port_action_port(instance, port,
+			       MMAL_MSG_PORT_ACTION_TYPE_ENABLE);
+	if (ret)
+		goto done;
+
+	port->enabled = true;
+
+	if (port->buffer_cb) {
+		/* send buffer headers to videocore */
+		hdr_count = 1;
+		list_for_each(buf_head, &port->buffers) {
+			struct mmal_buffer *mmalbuf;
+			mmalbuf = list_entry(buf_head, struct mmal_buffer,
+					     list);
+			ret = buffer_from_host(instance, port, mmalbuf);
+			if (ret)
+				goto done;
+
+			hdr_count++;
+			if (hdr_count > port->current_buffer.num)
+				break;
+		}
+	}
+
+	ret = port_info_get(instance, port);
+
+done:
+	return ret;
+}
+
+/* ------------------------------------------------------------------
+ * Exported API
+ *------------------------------------------------------------------*/
+
+int vchiq_mmal_port_set_format(struct vchiq_mmal_instance *instance,
+			       struct vchiq_mmal_port *port)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	ret = port_info_set(instance, port);
+	if (ret)
+		goto release_unlock;
+
+	/* read what has actually been set */
+	ret = port_info_get(instance, port);
+
+release_unlock:
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+
+}
+
+int vchiq_mmal_port_parameter_set(struct vchiq_mmal_instance *instance,
+				  struct vchiq_mmal_port *port,
+				  u32 parameter, void *value, u32 value_size)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	ret = port_parameter_set(instance, port, parameter, value, value_size);
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+int vchiq_mmal_port_parameter_get(struct vchiq_mmal_instance *instance,
+				  struct vchiq_mmal_port *port,
+				  u32 parameter, void *value, u32 *value_size)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	ret = port_parameter_get(instance, port, parameter, value, value_size);
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+/* enable a port
+ *
+ * enables a port and queues buffers for satisfying callbacks if we
+ * provide a callback handler
+ */
+int vchiq_mmal_port_enable(struct vchiq_mmal_instance *instance,
+			   struct vchiq_mmal_port *port,
+			   vchiq_mmal_buffer_cb buffer_cb)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	/* already enabled - noop */
+	if (port->enabled) {
+		ret = 0;
+		goto unlock;
+	}
+
+	port->buffer_cb = buffer_cb;
+
+	ret = port_enable(instance, port);
+
+unlock:
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+int vchiq_mmal_port_disable(struct vchiq_mmal_instance *instance,
+			    struct vchiq_mmal_port *port)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	if (!port->enabled) {
+		mutex_unlock(&instance->vchiq_mutex);
+		return 0;
+	}
+
+	ret = port_disable(instance, port);
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+/* ports will be connected in a tunneled manner so data buffers
+ * are not handled by client.
+ */
+int vchiq_mmal_port_connect_tunnel(struct vchiq_mmal_instance *instance,
+				   struct vchiq_mmal_port *src,
+				   struct vchiq_mmal_port *dst)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	/* disconnect ports if connected */
+	if (src->connected != NULL) {
+		ret = port_disable(instance, src);
+		if (ret) {
+			pr_err("failed disabling src port(%d)\n", ret);
+			goto release_unlock;
+		}
+
+		/* do not need to disable the destination port as they
+		 * are connected and it is done automatically
+		 */
+
+		ret = port_action_handle(instance, src,
+					 MMAL_MSG_PORT_ACTION_TYPE_DISCONNECT,
+					 src->connected->component->handle,
+					 src->connected->handle);
+		if (ret < 0) {
+			pr_err("failed disconnecting src port\n");
+			goto release_unlock;
+		}
+		src->connected->enabled = false;
+		src->connected = NULL;
+	}
+
+	if (dst == NULL) {
+		/* do not make new connection */
+		ret = 0;
+		pr_debug("not making new connection\n");
+		goto release_unlock;
+	}
+
+	/* copy src port format to dst */
+	dst->format.encoding = src->format.encoding;
+	dst->es.video.width = src->es.video.width;
+	dst->es.video.height = src->es.video.height;
+	dst->es.video.crop.x = src->es.video.crop.x;
+	dst->es.video.crop.y = src->es.video.crop.y;
+	dst->es.video.crop.width = src->es.video.crop.width;
+	dst->es.video.crop.height = src->es.video.crop.height;
+	dst->es.video.frame_rate.num = src->es.video.frame_rate.num;
+	dst->es.video.frame_rate.den = src->es.video.frame_rate.den;
+
+	/* set new format */
+	ret = port_info_set(instance, dst);
+	if (ret) {
+		pr_debug("setting port info failed\n");
+		goto release_unlock;
+	}
+
+	/* read what has actually been set */
+	ret = port_info_get(instance, dst);
+	if (ret) {
+		pr_debug("read back port info failed\n");
+		goto release_unlock;
+	}
+
+	/* connect two ports together */
+	ret = port_action_handle(instance, src,
+				 MMAL_MSG_PORT_ACTION_TYPE_CONNECT,
+				 dst->component->handle, dst->handle);
+	if (ret < 0) {
+		pr_debug("connecting port %d:%d to %d:%d failed\n",
+			 src->component->handle, src->handle,
+			 dst->component->handle, dst->handle);
+		goto release_unlock;
+	}
+	src->connected = dst;
+
+release_unlock:
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+int vchiq_mmal_submit_buffer(struct vchiq_mmal_instance *instance,
+			     struct vchiq_mmal_port *port,
+			     struct mmal_buffer *buffer)
+{
+	unsigned long flags = 0;
+
+	spin_lock_irqsave(&port->slock, flags);
+	list_add_tail(&buffer->list, &port->buffers);
+	spin_unlock_irqrestore(&port->slock, flags);
+
+	/* the port previously underflowed because it was missing a
+	 * mmal_buffer which has just been added, submit that buffer
+	 * to the mmal service.
+	 */
+	if (port->buffer_underflow) {
+		port_buffer_from_host(instance, port);
+		port->buffer_underflow--;
+	}
+
+	return 0;
+}
+
+/* Initialise a mmal component and its ports
+ *
+ */
+int vchiq_mmal_component_init(struct vchiq_mmal_instance *instance,
+			      const char *name,
+			      struct vchiq_mmal_component **component_out)
+{
+	int ret;
+	int idx;		/* port index */
+	struct vchiq_mmal_component *component;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	if (instance->component_idx == VCHIQ_MMAL_MAX_COMPONENTS) {
+		ret = -EINVAL;	/* todo is this correct error? */
+		goto unlock;
+	}
+
+	component = &instance->component[instance->component_idx];
+
+	ret = create_component(instance, component, name);
+	if (ret < 0)
+		goto unlock;
+
+	/* ports info needs gathering */
+	component->control.type = MMAL_PORT_TYPE_CONTROL;
+	component->control.index = 0;
+	component->control.component = component;
+	spin_lock_init(&component->control.slock);
+	INIT_LIST_HEAD(&component->control.buffers);
+	ret = port_info_get(instance, &component->control);
+	if (ret < 0)
+		goto release_component;
+
+	for (idx = 0; idx < component->inputs; idx++) {
+		component->input[idx].type = MMAL_PORT_TYPE_INPUT;
+		component->input[idx].index = idx;
+		component->input[idx].component = component;
+		spin_lock_init(&component->input[idx].slock);
+		INIT_LIST_HEAD(&component->input[idx].buffers);
+		ret = port_info_get(instance, &component->input[idx]);
+		if (ret < 0)
+			goto release_component;
+	}
+
+	for (idx = 0; idx < component->outputs; idx++) {
+		component->output[idx].type = MMAL_PORT_TYPE_OUTPUT;
+		component->output[idx].index = idx;
+		component->output[idx].component = component;
+		spin_lock_init(&component->output[idx].slock);
+		INIT_LIST_HEAD(&component->output[idx].buffers);
+		ret = port_info_get(instance, &component->output[idx]);
+		if (ret < 0)
+			goto release_component;
+	}
+
+	for (idx = 0; idx < component->clocks; idx++) {
+		component->clock[idx].type = MMAL_PORT_TYPE_CLOCK;
+		component->clock[idx].index = idx;
+		component->clock[idx].component = component;
+		spin_lock_init(&component->clock[idx].slock);
+		INIT_LIST_HEAD(&component->clock[idx].buffers);
+		ret = port_info_get(instance, &component->clock[idx]);
+		if (ret < 0)
+			goto release_component;
+	}
+
+	instance->component_idx++;
+
+	*component_out = component;
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return 0;
+
+release_component:
+	destroy_component(instance, component);
+unlock:
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+/*
+ * cause a mmal component to be destroyed
+ */
+int vchiq_mmal_component_finalise(struct vchiq_mmal_instance *instance,
+				  struct vchiq_mmal_component *component)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	if (component->enabled)
+		ret = disable_component(instance, component);
+
+	ret = destroy_component(instance, component);
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+/*
+ * cause a mmal component to be enabled
+ */
+int vchiq_mmal_component_enable(struct vchiq_mmal_instance *instance,
+				struct vchiq_mmal_component *component)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	if (component->enabled) {
+		mutex_unlock(&instance->vchiq_mutex);
+		return 0;
+	}
+
+	ret = enable_component(instance, component);
+	if (ret == 0)
+		component->enabled = true;
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+/*
+ * cause a mmal component to be enabled
+ */
+int vchiq_mmal_component_disable(struct vchiq_mmal_instance *instance,
+				 struct vchiq_mmal_component *component)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	if (!component->enabled) {
+		mutex_unlock(&instance->vchiq_mutex);
+		return 0;
+	}
+
+	ret = disable_component(instance, component);
+	if (ret == 0)
+		component->enabled = false;
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+int vchiq_mmal_version(struct vchiq_mmal_instance *instance,
+		       u32 *major_out, u32 *minor_out)
+{
+	int ret;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	ret = get_version(instance, major_out, minor_out);
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	return ret;
+}
+
+int vchiq_mmal_finalise(struct vchiq_mmal_instance *instance)
+{
+	int status = 0;
+
+	if (instance == NULL)
+		return -EINVAL;
+
+	if (mutex_lock_interruptible(&instance->vchiq_mutex))
+		return -EINTR;
+
+	vchi_service_use(instance->handle);
+
+	status = vchi_service_close(instance->handle);
+	if (status != 0)
+		pr_err("mmal-vchiq: VCHIQ close failed");
+
+	mutex_unlock(&instance->vchiq_mutex);
+
+	vfree(instance->bulk_scratch);
+
+	kfree(instance);
+
+	return status;
+}
+
+int vchiq_mmal_init(struct vchiq_mmal_instance **out_instance)
+{
+	int status;
+	struct vchiq_mmal_instance *instance;
+	static VCHI_CONNECTION_T *vchi_connection;
+	static VCHI_INSTANCE_T vchi_instance;
+	SERVICE_CREATION_T params = {
+		VCHI_VERSION_EX(VC_MMAL_VER, VC_MMAL_MIN_VER),
+		VC_MMAL_SERVER_NAME,
+		vchi_connection,
+		0,		/* rx fifo size (unused) */
+		0,		/* tx fifo size (unused) */
+		service_callback,
+		NULL,		/* service callback parameter */
+		1,		/* unaligned bulk receives */
+		1,		/* unaligned bulk transmits */
+		0		/* want crc check on bulk transfers */
+	};
+
+	/* compile time checks to ensure structure size as they are
+	 * directly (de)serialised from memory.
+	 */
+
+	/* ensure the header structure has packed to the correct size */
+	BUILD_BUG_ON(sizeof(struct mmal_msg_header) != 24);
+
+	/* ensure message structure does not exceed maximum length */
+	BUILD_BUG_ON(sizeof(struct mmal_msg) > MMAL_MSG_MAX_SIZE);
+
+	/* mmal port struct is correct size */
+	BUILD_BUG_ON(sizeof(struct mmal_port) != 64);
+
+	/* create a vchi instance */
+	status = vchi_initialise(&vchi_instance);
+	if (status) {
+		pr_err("Failed to initialise VCHI instance (status=%d)\n",
+		       status);
+		return -EIO;
+	}
+
+	status = vchi_connect(NULL, 0, vchi_instance);
+	if (status) {
+		pr_err("Failed to connect VCHI instance (status=%d)\n", status);
+		return -EIO;
+	}
+
+	instance = kmalloc(sizeof(*instance), GFP_KERNEL);
+	memset(instance, 0, sizeof(*instance));
+
+	mutex_init(&instance->vchiq_mutex);
+	mutex_init(&instance->bulk_mutex);
+
+	instance->bulk_scratch = vmalloc(PAGE_SIZE);
+
+	params.callback_param = instance;
+
+	status = vchi_service_open(vchi_instance, &params, &instance->handle);
+	if (status) {
+		pr_err("Failed to open VCHI service connection (status=%d)\n",
+		       status);
+		goto err_close_services;
+	}
+
+	vchi_service_release(instance->handle);
+
+	*out_instance = instance;
+
+	return 0;
+
+err_close_services:
+
+	vchi_service_close(instance->handle);
+	vfree(instance->bulk_scratch);
+	kfree(instance);
+	return -ENODEV;
+}
--- /dev/null
+++ b/drivers/media/platform/bcm2835/mmal-vchiq.h
@@ -0,0 +1,178 @@
+/*
+ * Broadcom BM2835 V4L2 driver
+ *
+ * Copyright © 2013 Raspberry Pi (Trading) Ltd.
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file COPYING in the main directory of this archive
+ * for more details.
+ *
+ * Authors: Vincent Sanders <vincent.sanders@collabora.co.uk>
+ *          Dave Stevenson <dsteve@broadcom.com>
+ *          Simon Mellor <simellor@broadcom.com>
+ *          Luke Diamand <luked@broadcom.com>
+ *
+ * MMAL interface to VCHIQ message passing
+ */
+
+#ifndef MMAL_VCHIQ_H
+#define MMAL_VCHIQ_H
+
+#include "mmal-msg-format.h"
+
+#define MAX_PORT_COUNT 4
+
+/* Maximum size of the format extradata. */
+#define MMAL_FORMAT_EXTRADATA_MAX_SIZE 128
+
+struct vchiq_mmal_instance;
+
+enum vchiq_mmal_es_type {
+	MMAL_ES_TYPE_UNKNOWN,     /**< Unknown elementary stream type */
+	MMAL_ES_TYPE_CONTROL,     /**< Elementary stream of control commands */
+	MMAL_ES_TYPE_AUDIO,       /**< Audio elementary stream */
+	MMAL_ES_TYPE_VIDEO,       /**< Video elementary stream */
+	MMAL_ES_TYPE_SUBPICTURE   /**< Sub-picture elementary stream */
+};
+
+/* rectangle, used lots so it gets its own struct */
+struct vchiq_mmal_rect {
+	s32 x;
+	s32 y;
+	s32 width;
+	s32 height;
+};
+
+struct vchiq_mmal_port_buffer {
+	unsigned int num; /* number of buffers */
+	u32 size; /* size of buffers */
+	u32 alignment; /* alignment of buffers */
+};
+
+struct vchiq_mmal_port;
+
+typedef void (*vchiq_mmal_buffer_cb)(
+		struct vchiq_mmal_instance  *instance,
+		struct vchiq_mmal_port *port,
+		int status, struct mmal_buffer *buffer,
+		unsigned long length, u32 mmal_flags, s64 dts, s64 pts);
+
+struct vchiq_mmal_port {
+	bool enabled;
+	u32 handle;
+	u32 type; /* port type, cached to use on port info set */
+	u32 index; /* port index, cached to use on port info set */
+
+	/* component port belongs to, allows simple deref */
+	struct vchiq_mmal_component *component;
+
+	struct vchiq_mmal_port *connected; /* port conencted to */
+
+	/* buffer info */
+	struct vchiq_mmal_port_buffer minimum_buffer;
+	struct vchiq_mmal_port_buffer recommended_buffer;
+	struct vchiq_mmal_port_buffer current_buffer;
+
+	/* stream format */
+	struct mmal_es_format format;
+	/* elementry stream format */
+	union mmal_es_specific_format es;
+
+	/* data buffers to fill */
+	struct list_head buffers;
+	/* lock to serialise adding and removing buffers from list */
+	spinlock_t slock;
+	/* count of how many buffer header refils have failed because
+	 * there was no buffer to satisfy them
+	 */
+	int buffer_underflow;
+	/* callback on buffer completion */
+	vchiq_mmal_buffer_cb buffer_cb;
+	/* callback context */
+	void *cb_ctx;
+};
+
+struct vchiq_mmal_component {
+	bool enabled;
+	u32 handle;  /* VideoCore handle for component */
+	u32 inputs;  /* Number of input ports */
+	u32 outputs; /* Number of output ports */
+	u32 clocks;  /* Number of clock ports */
+	struct vchiq_mmal_port control; /* control port */
+	struct vchiq_mmal_port input[MAX_PORT_COUNT]; /* input ports */
+	struct vchiq_mmal_port output[MAX_PORT_COUNT]; /* output ports */
+	struct vchiq_mmal_port clock[MAX_PORT_COUNT]; /* clock ports */
+};
+
+
+int vchiq_mmal_init(struct vchiq_mmal_instance **out_instance);
+int vchiq_mmal_finalise(struct vchiq_mmal_instance *instance);
+
+/* Initialise a mmal component and its ports
+*
+*/
+int vchiq_mmal_component_init(
+		struct vchiq_mmal_instance *instance,
+		const char *name,
+		struct vchiq_mmal_component **component_out);
+
+int vchiq_mmal_component_finalise(
+		struct vchiq_mmal_instance *instance,
+		struct vchiq_mmal_component *component);
+
+int vchiq_mmal_component_enable(
+		struct vchiq_mmal_instance *instance,
+		struct vchiq_mmal_component *component);
+
+int vchiq_mmal_component_disable(
+		struct vchiq_mmal_instance *instance,
+		struct vchiq_mmal_component *component);
+
+
+
+/* enable a mmal port
+ *
+ * enables a port and if a buffer callback provided enque buffer
+ * headers as apropriate for the port.
+ */
+int vchiq_mmal_port_enable(
+		struct vchiq_mmal_instance *instance,
+		struct vchiq_mmal_port *port,
+		vchiq_mmal_buffer_cb buffer_cb);
+
+/* disable a port
+ *
+ * disable a port will dequeue any pending buffers
+ */
+int vchiq_mmal_port_disable(struct vchiq_mmal_instance *instance,
+			   struct vchiq_mmal_port *port);
+
+
+int vchiq_mmal_port_parameter_set(struct vchiq_mmal_instance *instance,
+				  struct vchiq_mmal_port *port,
+				  u32 parameter,
+				  void *value,
+				  u32 value_size);
+
+int vchiq_mmal_port_parameter_get(struct vchiq_mmal_instance *instance,
+				  struct vchiq_mmal_port *port,
+				  u32 parameter,
+				  void *value,
+				  u32 *value_size);
+
+int vchiq_mmal_port_set_format(struct vchiq_mmal_instance *instance,
+			       struct vchiq_mmal_port *port);
+
+int vchiq_mmal_port_connect_tunnel(struct vchiq_mmal_instance *instance,
+			    struct vchiq_mmal_port *src,
+			    struct vchiq_mmal_port *dst);
+
+int vchiq_mmal_version(struct vchiq_mmal_instance *instance,
+		       u32 *major_out,
+		       u32 *minor_out);
+
+int vchiq_mmal_submit_buffer(struct vchiq_mmal_instance *instance,
+			     struct vchiq_mmal_port *port,
+			     struct mmal_buffer *buf);
+
+#endif /* MMAL_VCHIQ_H */
