From f8cda0bc698706413b5dd6fde827f9a2601ac61b Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 31 Mar 2016 06:07:01 +0200
Subject: [PATCH 056/102] arm: mediatek: make a7 timer work Signed-off-by:
 John Crispin <blogic@openwrt.org>

---
 arch/arm/mach-mediatek/Kconfig    |    1 +
 arch/arm/mach-mediatek/mediatek.c |    1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/mach-mediatek/Kconfig
+++ b/arch/arm/mach-mediatek/Kconfig
@@ -24,6 +24,7 @@ config MACH_MT6592
 config MACH_MT7623
 	bool "MediaTek MT7623 SoCs support"
 	default ARCH_MEDIATEK
+	select HAVE_ARM_ARCH_TIMER
 	select MIGHT_HAVE_PCI
 
 config MACH_MT8127
--- a/arch/arm/mach-mediatek/mediatek.c
+++ b/arch/arm/mach-mediatek/mediatek.c
@@ -29,6 +29,7 @@ static void __init mediatek_timer_init(v
 	void __iomem *gpt_base;
 
 	if (of_machine_is_compatible("mediatek,mt6589") ||
+	    of_machine_is_compatible("mediatek,mt7623") ||
 	    of_machine_is_compatible("mediatek,mt8135") ||
 	    of_machine_is_compatible("mediatek,mt8127")) {
 		/* turn on GPT6 which ungates arch timer clocks */
