--- a/arch/arm/mach-ixp4xx/coyote-setup.c
+++ b/arch/arm/mach-ixp4xx/coyote-setup.c
@@ -14,6 +14,7 @@
 #include <linux/serial.h>
 #include <linux/tty.h>
 #include <linux/serial_8250.h>
+#include <linux/dma-mapping.h>
 
 #include <asm/types.h>
 #include <asm/setup.h>
@@ -81,9 +82,39 @@ static struct platform_device coyote_uar
 	.resource	= &coyote_uart_resource,
 };
 
+/* Built-in 10/100 Ethernet MAC interfaces */
+static struct eth_plat_info ixdpg425_plat_eth[] = {
+        {
+                .phy            = 5,
+                .rxq            = 3,
+                .txreadyq       = 20,
+        }, {
+                .phy            = 4,
+                .rxq            = 4,
+                .txreadyq       = 21,
+        }
+};
+
+static struct platform_device ixdpg425_eth[] = {
+	{
+		.name			= "ixp4xx_eth",
+		.id			= IXP4XX_ETH_NPEB,
+		.dev.platform_data	= ixdpg425_plat_eth,
+		.dev.coherent_dma_mask	= DMA_BIT_MASK(32),
+	}, {
+		.name			= "ixp4xx_eth",
+		.id			= IXP4XX_ETH_NPEC,
+		.dev.platform_data	= ixdpg425_plat_eth + 1,
+		.dev.coherent_dma_mask	= DMA_BIT_MASK(32),
+	}
+};
+
+
 static struct platform_device *coyote_devices[] __initdata = {
 	&coyote_flash,
-	&coyote_uart
+	&coyote_uart,
+	&ixdpg425_eth[0],
+	&ixdpg425_eth[1],
 };
 
 static void __init coyote_init(void)
