From 70fe24ed93fa90eb407d18a5fc9d9ad85ac9184c Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wens@csie.org>
Date: Wed, 27 Jan 2016 16:34:43 +0800
Subject: [PATCH] sunxi: Support SID e-fuses on A83T and H3

On the A83T and H3, the SID block is at a different address.
Furthurmore, the e-fuses are at an offset of 0x200 within the
hardware's address space.

Signed-off-by: Chen-Yu Tsai <wens@csie.org>
Acked-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/include/asm/arch-sunxi/cpu_sun4i.h | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/include/asm/arch-sunxi/cpu_sun4i.h b/arch/arm/include/asm/arch-sunxi/cpu_sun4i.h
index b6e11eb..65c0441 100644
--- a/arch/arm/include/asm/arch-sunxi/cpu_sun4i.h
+++ b/arch/arm/include/asm/arch-sunxi/cpu_sun4i.h
@@ -82,7 +82,14 @@
 #define SUNXI_AD_DA_BASE		0x01c22c00
 #define SUNXI_KEYPAD_BASE		0x01c23000
 #define SUNXI_TZPC_BASE			0x01c23400
+
+#if defined(CONFIG_MACH_SUN8I_A83T) || defined(CONFIG_MACH_SUN8I_H3)
+/* SID address space starts at 0x01c1400, but e-fuse is at offset 0x200 */
+#define SUNXI_SID_BASE			0x01c14200
+#else
 #define SUNXI_SID_BASE			0x01c23800
+#endif
+
 #define SUNXI_SJTAG_BASE		0x01c23c00
 
 #define SUNXI_TP_BASE			0x01c25000
