// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "ravpower,rp-wd009", "mediatek,mt7628an-soc";
	model = "RAVPower RP-WD009";

	aliases {
		led-boot = &led_globe;
		led-failsafe = &led_globe;
		led-running = &led_globe;
		led-upgrade = &led_globe;
	};

	chosen {
		bootargs = "console=ttyS0,57600";
	};

	leds {
		compatible = "gpio-leds";

		led_globe: globe {
			label = "white:globe";
			gpios = <&gpio 43 GPIO_ACTIVE_LOW>;
		};

		wlan2 {
			label = "white:wlan2";
			gpios = <&gpio 44 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5 {
			label = "white:wlan5";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		sd_white {
			label = "white:sd";
			gpios = <&gpio 41 GPIO_ACTIVE_LOW>;
		};

		sd_red {
			label = "red:sd";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 46 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		/* Power interrupt on Pin 39 */

		rfkill {
			label = "rfkill";
			gpios = <&gpio 21 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};

		backup {
			label = "backup";
			gpios = <&gpio 40 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_COPY>;
		};
	};
};

&gpio {
	mt7610-power {
		gpio-hog;
		gpios = <20 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "mt7610-power";
	};
};

&state_default {
	gpio {
		groups = "uart1", "wled_an", "p0led_an", "p2led_an", "p3led_an",
				"p4led_an", "uart2", "pwm0", "i2s";
		function = "gpio";
	};
};

&sdhci {
	status = "okay";
};

&i2c {
	status = "okay";

	/* Custom PMIC at 0x0a */
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5470000 6000000>;
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "bootloader";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "loader";
				reg = <0x50000 0x180000>;
			};

			partition@1d0000 {
				label = "params";
				reg = <0x1d0000 0x10000>;
				read-only;
			};

			partition@1e0000 {
				label = "user_backup";
				reg = <0x1e0000 0x10000>;
				read-only;
			};

			partition@1f0000 {
				label = "user";
				reg = <0x1f0000 0x10000>;
				read-only;
			};

			partition@200000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x200000 0xdf0000>;
			};

			partition@ff0000 {
				label = "mode";
				reg = <0xff0000 0x10000>;
				read-only;
			};
		};
	};
};

&wmac {
	status = "okay";
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
};
