From fa578d4e9fbef8928a45edd904dafb1e3334417e Mon Sep 17 00:00:00 2001
From: Yangbo Lu <yangbo.lu@nxp.com>
Date: Thu, 30 Apr 2020 10:56:46 +0800
Subject: [PATCH] arm64: dts: ls1043a-rdb: add compatible for board

Add compatible for board to identify.

Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
Signed-off-by: Shawn Guo <shawnguo@kernel.org>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
@@ -13,6 +13,7 @@
 
 / {
 	model = "LS1043A RDB Board";
+	compatible = "fsl,ls1043a-rdb", "fsl,ls1043a";
 
 	aliases {
 		serial0 = &duart0;
