// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9341.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Engenius EAP300 v2";
	compatible = "engenius,eap300-v2", "qca,ar9341";

	aliases {
		serial0 = &uart;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "blue:power";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan {
			label = "blue:wlan";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		lan {
			label = "blue:lan";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "openwrt,okli";
				label = "firmware";
				reg = <0x0 0x0>;
			};
		};
	};
};

&ref {
	clock-frequency = <40000000>;
};

&uart {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <20000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@50000 {
				label = "custom";
				reg = <0x050000 0x050000>;
				read-only;
			};

			partition@a0000 {
				label = "loader";
				reg = <0x0a0000 0x010000>;
				read-only;
			};

			fwconcat1: partition@b0000 {
				label = "fwconcat1";
				reg = <0x0b0000 0x170000>;
			};

			partition@220000 {
				label = "fakeroot";
				reg = <0x220000 0x010000>;
				read-only;
			};

			fwconcat0: partition@230000 {
				label = "fwconcat0";
				reg = <0x230000 0xbc0000>;
			};

			partition@df0000 {
				label = "failsafe";
				reg = <0xdf0000 0x200000>;
				read-only;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&art 0x0>;

	phy-handle = <&swphy0>;

	gmac-config {
		device = <&gmac>;
		switch-phy-swap = <1>;
	};
};

&eth1 {
	compatible = "syscon", "simple-mfd";
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};
