From: Felix Fietkau <nbd@nbd.name>
Date: Wed, 24 Mar 2021 02:30:48 +0100
Subject: [PATCH] netfilter: flowtable: bridge vlan hardware offload and
 switchdev

The switch might have already added the VLAN tag through PVID hardware
offload. Keep this extra VLAN in the flowtable but skip it on egress.

Signed-off-by: Felix Fietkau <nbd@nbd.name>
Signed-off-by: Pablo Neira Ayuso <pablo@netfilter.org>
---

--- a/include/linux/netdevice.h
+++ b/include/linux/netdevice.h
@@ -863,6 +863,7 @@ struct net_device_path {
 				DEV_PATH_BR_VLAN_KEEP,
 				DEV_PATH_BR_VLAN_TAG,
 				DEV_PATH_BR_VLAN_UNTAG,
+				DEV_PATH_BR_VLAN_UNTAG_HW,
 			}		vlan_mode;
 			u16		vlan_id;
 			__be16		vlan_proto;
--- a/include/net/netfilter/nf_flow_table.h
+++ b/include/net/netfilter/nf_flow_table.h
@@ -123,9 +123,10 @@ struct flow_offload_tuple {
 	/* All members above are keys for lookups, see flow_offload_hash(). */
 	struct { }			__hash;
 
-	u8				dir:4,
+	u8				dir:2,
 					xmit_type:2,
-					encap_num:2;
+					encap_num:2,
+					in_vlan_ingress:2;
 	u16				mtu;
 	union {
 		struct dst_entry	*dst_cache;
@@ -184,7 +185,8 @@ struct nf_flow_route {
 				u16		id;
 				__be16		proto;
 			} encap[NF_FLOW_TABLE_ENCAP_MAX];
-			u8			num_encaps;
+			u8			num_encaps:2,
+						ingress_vlans:2;
 		} in;
 		struct {
 			u32			ifindex;
--- a/net/bridge/br_device.c
+++ b/net/bridge/br_device.c
@@ -435,6 +435,7 @@ static int br_fill_forward_path(struct n
 		ctx->vlan[ctx->num_vlans].proto = path->bridge.vlan_proto;
 		ctx->num_vlans++;
 		break;
+	case DEV_PATH_BR_VLAN_UNTAG_HW:
 	case DEV_PATH_BR_VLAN_UNTAG:
 		ctx->num_vlans--;
 		break;
--- a/net/bridge/br_vlan.c
+++ b/net/bridge/br_vlan.c
@@ -1397,6 +1397,8 @@ int br_vlan_fill_forward_path_mode(struc
 
 	if (path->bridge.vlan_mode == DEV_PATH_BR_VLAN_TAG)
 		path->bridge.vlan_mode = DEV_PATH_BR_VLAN_KEEP;
+	else if (v->priv_flags & BR_VLFLAG_ADDED_BY_SWITCHDEV)
+		path->bridge.vlan_mode = DEV_PATH_BR_VLAN_UNTAG_HW;
 	else
 		path->bridge.vlan_mode = DEV_PATH_BR_VLAN_UNTAG;
 
--- a/net/netfilter/nf_flow_table_core.c
+++ b/net/netfilter/nf_flow_table_core.c
@@ -95,6 +95,8 @@ static int flow_offload_fill_route(struc
 	for (i = route->tuple[dir].in.num_encaps - 1; i >= 0; i--) {
 		flow_tuple->encap[j].id = route->tuple[dir].in.encap[i].id;
 		flow_tuple->encap[j].proto = route->tuple[dir].in.encap[i].proto;
+		if (route->tuple[dir].in.ingress_vlans & BIT(i))
+			flow_tuple->in_vlan_ingress |= BIT(j);
 		j++;
 	}
 	flow_tuple->encap_num = route->tuple[dir].in.num_encaps;
--- a/net/netfilter/nf_flow_table_offload.c
+++ b/net/netfilter/nf_flow_table_offload.c
@@ -594,8 +594,12 @@ nf_flow_rule_route_common(struct net *ne
 	other_tuple = &flow->tuplehash[!dir].tuple;
 
 	for (i = 0; i < other_tuple->encap_num; i++) {
-		struct flow_action_entry *entry = flow_action_entry_next(flow_rule);
+		struct flow_action_entry *entry;
 
+		if (other_tuple->in_vlan_ingress & BIT(i))
+			continue;
+
+		entry = flow_action_entry_next(flow_rule);
 		entry->id = FLOW_ACTION_VLAN_PUSH;
 		entry->vlan.vid = other_tuple->encap[i].id;
 		entry->vlan.proto = other_tuple->encap[i].proto;
--- a/net/netfilter/nft_flow_offload.c
+++ b/net/netfilter/nft_flow_offload.c
@@ -72,6 +72,7 @@ struct nft_forward_info {
 		__be16	proto;
 	} encap[NF_FLOW_TABLE_ENCAP_MAX];
 	u8 num_encaps;
+	u8 ingress_vlans;
 	u8 h_source[ETH_ALEN];
 	u8 h_dest[ETH_ALEN];
 	enum flow_offload_xmit_type xmit_type;
@@ -130,6 +131,9 @@ static void nft_dev_path_info(const stru
 				memcpy(info->h_source, path->dev->dev_addr, ETH_ALEN);
 
 			switch (path->bridge.vlan_mode) {
+			case DEV_PATH_BR_VLAN_UNTAG_HW:
+				info->ingress_vlans |= BIT(info->num_encaps - 1);
+				break;
 			case DEV_PATH_BR_VLAN_TAG:
 				info->encap[info->num_encaps].id = path->bridge.vlan_id;
 				info->encap[info->num_encaps].proto = path->bridge.vlan_proto;
@@ -198,6 +202,7 @@ static void nft_dev_forward_path(struct
 		route->tuple[!dir].in.encap[i].proto = info.encap[i].proto;
 	}
 	route->tuple[!dir].in.num_encaps = info.num_encaps;
+	route->tuple[!dir].in.ingress_vlans = info.ingress_vlans;
 
 	if (info.xmit_type == FLOW_OFFLOAD_XMIT_DIRECT) {
 		memcpy(route->tuple[dir].out.h_source, info.h_source, ETH_ALEN);
