// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/mtd/partitions/uimage.h>

/ {
	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &eth1;
	};

	leds {
		compatible = "gpio-leds";

		usb {
			label = "green:usb2";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port0>;
			linux,default-trigger = "usbport";
		};

		status {
			label = "amber:status";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		wps-amber {
			label = "amber:wps";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		wps-blue {
			label = "blue:wps";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};

		led_system: system {
			label = "blue:system";
			gpios = <&gpio 20 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-export {
		compatible = "gpio-export";
		#size-cells = <0>;

		usb2_power {
			gpio-export,name = "usb2:power";
			gpio-export,output = <1>;
			gpios = <&gpio 21 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "WPS button";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		reset {
			label = "Reset button";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&fwconcat0 &fwconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "openwrt,uimage", "denx,uimage";
				openwrt,ih-magic = <IH_MAGIC_OKLI>;
				label = "firmware";
				reg = <0x0 0x0>;
			};
		};
	};
};

&pcie1 {
	status = "okay";
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	hub_port0: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <80000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			fwconcat0: partition@50000 {
				label = "fwconcat0";
				reg = <0x050000 0xe20000>;
			};

			partition@e70000 {
				label = "loader";
				reg = <0xe70000 0x10000>;
				read-only;
			};

			fwconcat1: partition@e80000 {
				label = "fwconcat1";
				reg = <0xe80000 0x170000>;
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
			};
		};
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;

		qca,ar8327-initvals = <
			0x04 0x00080080 /* PORT0 PAD MODE CTRL */
			0x0c 0x07600000 /* PORT6 PAD MODE CTRL */
			0x50 0xc737c737 /* LED_CTRL0 */
			0x54 0x00000000 /* LED_CTRL1 */
			0x58 0x00000000 /* LED_CTRL2 */
			0x5c 0x0030c300 /* LED_CTRL3 */
			0x7c 0x0000007e /* PORT0_STATUS */
			0x94 0x0000007e /* PORT6 STATUS */
			>;
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&art 0x0>;
	phy-handle = <&phy0>;
	pll-data = <0xa6000000 0x00000101 0x00001616>;

	gmac-config {
		device = <&gmac>;
		rgmii-enabled = <1>;
	};
};

&eth1 {
	status = "okay";

	mtd-mac-address = <&art 0x0>;
	mtd-mac-address-increment = <(-1)>;
	pll-data = <0x03000101 0x00000101 0x00001616>;

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0 0 0 0 0>;
	};
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};
