From a99acc11751ea640c7687155e964612b232bc492 Mon Sep 17 00:00:00 2001
From: Zhang Ying-22455 <ying.zhang22455@nxp.com>
Date: Mon, 29 Oct 2018 10:37:03 +0800
Subject: [PATCH] arm64: dts: lx2160a: correct scl-gpios property

Signed-off-by: Zhang Ying-22455 <ying.zhang22455@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi
@@ -508,7 +508,7 @@
 			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "i2c";
 			clocks = <&clockgen 4 15>;
-			scl-gpio = <&gpio2 15 GPIO_ACTIVE_HIGH>;
+			scl-gpios = <&gpio2 15 GPIO_ACTIVE_HIGH>;
 			status = "disabled";
 		};
 
@@ -553,7 +553,7 @@
 			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
 			clock-names = "i2c";
 			clocks = <&clockgen 4 15>;
-			scl-gpio = <&gpio2 16 GPIO_ACTIVE_HIGH>;
+			scl-gpios = <&gpio2 16 GPIO_ACTIVE_HIGH>;
 			status = "disabled";
 		};
 
