From 095b4dabff2a929cefd330110c5c578956213188 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Wed, 24 Feb 2021 09:02:10 +0100
Subject: [PATCH] mtd: rawnand: brcmnand: fix OOB R/W with Hamming ECC
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Hamming ECC doesn't cover the OOB data, so reading or writing OOB shall
always be done without ECC enabled.
This is a problem when adding JFFS2 cleanmarkers to erased blocks. If JFFS2
clenmarkers are added to the OOB with ECC enabled, OOB bytes will be changed
from ff ff ff to 00 00 00, reporting incorrect ECC errors.

Fixes: 27c5b17cd1b1 ("mtd: nand: add NAND driver "library" for Broadcom STB NAND controller")
Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Acked-by: Brian Norris <computersforpeace@gmail.com>
Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Link: https://lore.kernel.org/linux-mtd/20210224080210.23686-1-noltari@gmail.com
---
 drivers/mtd/nand/raw/brcmnand/brcmnand.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/mtd/nand/raw/brcmnand/brcmnand.c
+++ b/drivers/mtd/nand/raw/brcmnand/brcmnand.c
@@ -2688,6 +2688,12 @@ static int brcmnand_attach_chip(struct n
 
 	ret = brcmstb_choose_ecc_layout(host);
 
+	/* If OOB is written with ECC enabled it will cause ECC errors */
+	if (is_hamming_ecc(host->ctrl, &host->hwcfg)) {
+		chip->ecc.write_oob = brcmnand_write_oob_raw;
+		chip->ecc.read_oob = brcmnand_read_oob_raw;
+	}
+
 	return ret;
 }
 
