--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -71,6 +71,17 @@ config PANDA
 	  This board is a Concurrent Dual-Band wireless access point with a
 	  Freescale P1020 SoC.
 
+config WS_AP3710I
+	bool "Enterasys WS-AP3710i"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	help
+	  This option enables support for the Enterasys WS-AP3710i board.
+
+	  This board is a Concurrent Dual-Band wireless access point with a
+	  Freescale P1020 SoC.
+
 config MPC8540_ADS
 	bool "Freescale MPC8540 ADS"
 	select DEFAULT_UIMAGE
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -24,6 +24,7 @@ obj-$(CONFIG_P1022_RDK)   += p1022_rdk.o
 obj-$(CONFIG_P1023_RDB)   += p1023_rdb.o
 obj-$(CONFIG_PANDA)       += panda.o
 obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
+obj-$(CONFIG_WS_AP3710I)  += ws-ap3710i.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
 obj-$(CONFIG_FB_FSL_DIU)	+= t1042rdb_diu.o
 obj-$(CONFIG_RED_15W_REV1)	+= red15w_rev1.o
