// SPDX-License-Identifier: GPL-2.0-or-later

#include "bcm6358.dtsi"

/ {
	compatible = "huawei,hg556a-b", "brcm,bcm6358";
	model = "Huawei EchoLife HG556a (version B)";

	aliases {
		led-boot = &power_red;
		led-failsafe = &power_red;
		led-running = &power_red;
		led-upgrade = &power_red;

		led-dsl = &dsl_red;
		led-internet = &dsl_red;
		led-usb = &hspa_red;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x00000000 0x04000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		help {
			label = "help";
			gpios = <&pinctrl 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_HELP>;
			debounce-interval = <60>;
		};

		wlan {
			label = "wlan";
			gpios = <&pinctrl 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		restart {
			label = "restart";
			gpios = <&pinctrl 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_CONFIG>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led@0 {
			label = "red:message";
			gpios = <&pinctrl 0 GPIO_ACTIVE_LOW>;
		};

		hspa_red: led@1 {
			label = "red:hspa";
			gpios = <&pinctrl 1 GPIO_ACTIVE_LOW>;
		};

		dsl_red: led@2 {
			label = "red:dsl";
			gpios = <&pinctrl 2 GPIO_ACTIVE_LOW>;
		};

		power_red: led@3 {
			label = "red:power";
			gpios = <&pinctrl 3 GPIO_ACTIVE_LOW>;
		};

		led@6 {
			label = "all";
			gpios = <&pinctrl 6 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		led@12 {
			label = "green:lan1";
			gpios = <&pinctrl 12 GPIO_ACTIVE_LOW>;
		};

		led@13 {
			label = "red:lan1";
			gpios = <&pinctrl 13 GPIO_ACTIVE_LOW>;
		};

		led@15 {
			label = "green:lan2";
			gpios = <&pinctrl 15 GPIO_ACTIVE_LOW>;
		};

		led@22 {
			label = "red:lan2";
			gpios = <&pinctrl 22 GPIO_ACTIVE_LOW>;
		};

		led@23 {
			label = "green:lan3";
			gpios = <&pinctrl 23 GPIO_ACTIVE_LOW>;
		};

		led@26 {
			label = "red:lan3";
			gpios = <&pinctrl 26 GPIO_ACTIVE_LOW>;
		};

		led@27 {
			label = "green:lan4";
			gpios = <&pinctrl 27 GPIO_ACTIVE_LOW>;
		};

		led@28 {
			label = "red:lan4";
			gpios = <&pinctrl 28 GPIO_ACTIVE_LOW>;
		};
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe: partition@0 {
			label = "cfe";
			reg = <0x000000 0x020000>;
			read-only;
		};

		partition@20000 {
			label = "firmware";
			reg = <0x020000 0xec0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		cal_data: partition@ee0000 {
			label = "cal_data";
			reg = <0xee0000 0x100000>;
			read-only;
		};

		partition@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};

&usbh {
	status = "okay";
};
