From ea94fb0b5693c354e5281eb3fcdbc9700cdd3d7f Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 28 Nov 2019 15:49:08 +0000
Subject: [PATCH] arm/dts: 2711: Add 'pcie0' alias

It is useful for the firmware to be able to locate the pcie DT node,
so add an alias pointing to it in the same way that "ethernet0"
points to the genet.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm2711-rpi-4-b.dts | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
+++ b/arch/arm/boot/dts/bcm2711-rpi-4-b.dts
@@ -30,6 +30,7 @@
 		/delete-property/ ethernet;
 		/delete-property/ intc;
 		ethernet0 = &genet;
+		pcie0 = &pcie_0;
 	};
 };
 
