// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca953x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "compex,wpj531-16m", "qca,qca9531";
	model = "Compex WPJ531 (16MB flash)";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_sig4;
		led-failsafe = &led_sig4;
		led-running = &led_sig4;
		led-upgrade = &led_sig4;
	};

	beeper {
		compatible = "gpio-beeper";
		gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		pinctrl-names = "default";
		pinctrl-0 = <&pinmux_led_eth_pins>;

		sig1 {
			label = "red:sig1";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		sig2 {
			label = "yellow:sig2";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
		};

		sig3 {
			label = "green:sig3";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_sig4: sig4 {
			label = "green:sig4";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};
};

&pinmux {
	pinmux_led_eth_pins: pinmux_led_eth_pins {
		pinctrl-single,bits = <0x8 0x2b000000 0xff000000>, <0xc 0x00002d00 0x0000ff00>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				label = "u-boot";
				reg = <0x000000 0x030000>;
				read-only;
			};

			partition@30000 {
				label = "firmware";
				reg = <0x030000 0xfc0000>;
				compatible = "denx,uimage";
			};

			art: partition@ff0000 {
				label = "art";
				reg = <0xff0000 0x010000>;
				read-only;
			};
		};
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&swphy4>;

	mtd-mac-address = <&uboot 0x2e010>;
};

&eth1 {
	mtd-mac-address = <&uboot 0x2e018>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci168c,003c";
		reg = <0x0000 0 0 0 0>;
	};
};

&usb_phy {
	status = "okay";
};

&usb0 {
	status = "okay";
};
