From 2c262ae9cfd82b5b65bbb86a98da6a10c11db367 Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wens@csie.org>
Date: Thu, 14 May 2020 17:39:30 +0800
Subject: [PATCH] ARM: dts: bcm2711-rpi: Remove downstream thermal
 sensor node

Signed-off-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm/boot/dts/bcm2711-rpi.dtsi | 14 --------------
 1 file changed, 14 deletions(-)

--- a/arch/arm/boot/dts/bcm2711-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2711-rpi.dtsi
@@ -50,16 +50,6 @@
 };
 
 &soc {
-	thermal: thermal@7d5d2200 {
-		compatible = "brcm,avs-tmon-bcm2711";
-		reg = <0x7d5d2200 0x2c>;
-		interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
-		interrupt-names = "tmon";
-		clocks = <&clocks BCM2835_CLOCK_TSENS>;
-		#thermal-sensor-cells = <0>;
-		status = "okay";
-	};
-
 	/delete-node/ audio;
 };
 
@@ -177,10 +167,6 @@
 		     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
 };
 
-&cpu_thermal {
-	 thermal-sensors = <&thermal>;
-};
-
 &genet {
 	compatible = "brcm,bcm2711-genet-v5", "brcm,genet-v5";
 };
