From 88eee9b7b42e69fb622ddb3ff6f37e8e4347f5b2 Mon Sep 17 00:00:00 2001
From: Lech Perczak <lech.perczak@gmail.com>
Date: Tue, 23 Feb 2021 19:34:56 +0100
Subject: net: usb: qmi_wwan: support ZTE P685M modem
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Now that interface 3 in "option" driver is no longer mapped, add device
ID matching it to qmi_wwan.

The modem is used inside ZTE MF283+ router and carriers identify it as
such.
Interface mapping is:
0: QCDM, 1: AT (PCUI), 2: AT (Modem), 3: QMI, 4: ADB

T:  Bus=02 Lev=02 Prnt=02 Port=05 Cnt=01 Dev#=  3 Spd=480  MxCh= 0
D:  Ver= 2.01 Cls=00(>ifc ) Sub=00 Prot=00 MxPS=64 #Cfgs=  1
P:  Vendor=19d2 ProdID=1275 Rev=f0.00
S:  Manufacturer=ZTE,Incorporated
S:  Product=ZTE Technologies MSM
S:  SerialNumber=P685M510ZTED0000CP&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&&0
C:* #Ifs= 5 Cfg#= 1 Atr=a0 MxPwr=500mA
I:* If#= 0 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=ff Prot=ff Driver=option
E:  Ad=81(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E:  Ad=01(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 1 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=00 Prot=00 Driver=option
E:  Ad=83(I) Atr=03(Int.) MxPS=  10 Ivl=32ms
E:  Ad=82(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E:  Ad=02(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 2 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=00 Prot=00 Driver=option
E:  Ad=85(I) Atr=03(Int.) MxPS=  10 Ivl=32ms
E:  Ad=84(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E:  Ad=03(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 3 Alt= 0 #EPs= 3 Cls=ff(vend.) Sub=ff Prot=ff Driver=qmi_wwan
E:  Ad=87(I) Atr=03(Int.) MxPS=   8 Ivl=32ms
E:  Ad=86(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E:  Ad=04(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms
I:* If#= 4 Alt= 0 #EPs= 2 Cls=ff(vend.) Sub=42 Prot=01 Driver=(none)
E:  Ad=88(I) Atr=02(Bulk) MxPS= 512 Ivl=0ms
E:  Ad=05(O) Atr=02(Bulk) MxPS= 512 Ivl=0ms

Acked-by: Bjørn Mork <bjorn@mork.no>
Signed-off-by: Lech Perczak <lech.perczak@gmail.com>
Link: https://lore.kernel.org/r/20210223183456.6377-1-lech.perczak@gmail.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/usb/qmi_wwan.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/usb/qmi_wwan.c
+++ b/drivers/net/usb/qmi_wwan.c
@@ -1258,6 +1258,7 @@ static const struct usb_device_id produc
 	{QMI_FIXED_INTF(0x19d2, 0x1255, 4)},
 	{QMI_FIXED_INTF(0x19d2, 0x1256, 4)},
 	{QMI_FIXED_INTF(0x19d2, 0x1270, 5)},	/* ZTE MF667 */
+	{QMI_FIXED_INTF(0x19d2, 0x1275, 3)},	/* ZTE P685M */
 	{QMI_FIXED_INTF(0x19d2, 0x1401, 2)},
 	{QMI_FIXED_INTF(0x19d2, 0x1402, 2)},	/* ZTE MF60 */
 	{QMI_FIXED_INTF(0x19d2, 0x1424, 2)},
