From 9704292ed3230ee19dc4dd64f7484301b728ffb7 Mon Sep 17 00:00:00 2001
From: Rui Salvaterra <rsalvaterra@gmail.com>
Date: Wed, 17 Feb 2021 15:19:30 +0000
Subject: [PATCH] ARM: dts: turris-omnia: fix hardware buffer management

Hardware buffer management has never worked on the Turris Omnia, as the
required MBus window hadn't been reserved. Fix thusly.

Fixes: 018b88eee1a2 ("ARM: dts: turris-omnia: enable HW buffer management")

Signed-off-by: Rui Salvaterra <rsalvaterra@gmail.com>
---
 arch/arm/boot/dts/armada-385-turris-omnia.dts | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/arch/arm/boot/dts/armada-385-turris-omnia.dts
+++ b/arch/arm/boot/dts/armada-385-turris-omnia.dts
@@ -31,7 +31,8 @@
 		ranges = <MBUS_ID(0xf0, 0x01) 0 0xf1000000 0x100000
 			  MBUS_ID(0x01, 0x1d) 0 0xfff00000 0x100000
 			  MBUS_ID(0x09, 0x19) 0 0xf1100000 0x10000
-			  MBUS_ID(0x09, 0x15) 0 0xf1110000 0x10000>;
+			  MBUS_ID(0x09, 0x15) 0 0xf1110000 0x10000
+			  MBUS_ID(0x0c, 0x04) 0 0xf1200000 0x100000>;
 
 		internal-regs {
 
