From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 15 Feb 2021 19:52:58 +0100
Subject: [PATCH] arm64: dts: broadcom: bcm4908: describe Netgear R8000P switch
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

R8000P model has 4 LAN ports and 1 WAN port.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---
 .../bcm4908/bcm4906-netgear-r8000p.dts        | 25 +++++++++++++++++++
 1 file changed, 25 insertions(+)

--- a/arch/arm64/boot/dts/broadcom/bcm4908/bcm4906-netgear-r8000p.dts
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/bcm4906-netgear-r8000p.dts
@@ -43,6 +43,31 @@
 	status = "okay";
 };
 
+&ports {
+	port@0 {
+		label = "lan4";
+	};
+
+	port@1 {
+		label = "lan3";
+	};
+
+	port@2 {
+		label = "lan2";
+	};
+
+	port@3 {
+		label = "lan1";
+	};
+
+	port@7 {
+		reg = <7>;
+		phy-mode = "internal";
+		phy-handle = <&phy12>;
+		label = "wan";
+	};
+};
+
 &nandcs {
 	nand-ecc-strength = <4>;
 	nand-ecc-step-size = <512>;
