// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "iodata,wn-dx1200gr", "mediatek,mt7621-soc";
	model = "I-O DATA WN-DX1200GR";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &wan;
	};

	leds {
		compatible = "gpio-leds";

		wps {
			label = "blue:wps";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_power: power {
			label = "green:power";
			gpios = <&gpio 9 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		repeater {
			label = "repeater";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x100000>;
			read-only;
		};

		partition@100000 {
			label = "u-boot-env";
			reg = <0x100000 0x100000>;
			read-only;
		};

		factory: partition@200000 {
			label = "factory";
			reg = <0x200000 0x200000>;
		};

		partition@400000 {
			label = "kernel";
			reg = <0x400000 0x400000>;
		};

		partition@800000 {
			label = "ubi";
			reg = <0x800000 0x2e00000>;
		};

		partition@3600000 {
			label = "Config";
			reg = <0x3600000 0x100000>;
			read-only;
		};

		partition@3700000 {
			label = "firmware_2";
			reg = <0x3700000 0x3200000>;
		};

		partition@6900000 {
			label = "Config_2";
			reg = <0x6900000 0x100000>;
			read-only;
		};

		partition@6a00000 {
			label = "persist";
			reg = <0x6a00000 0x100000>;
		};

		partition@6b00000 {
			label = "idmkey";
			reg = <0x6b00000 0x100000>;
			read-only;
		};

		partition@6c00000 {
			label = "Backup";
			reg = <0x6c00000 0x1380000>;
			read-only;
		};
	};
};

&gmac0 {
	mtd-mac-address = <&factory 0x1e000>;
};

&switch0 {
	ports {
		wan: port@0 {
			status = "okay";
			label = "wan";
			mtd-mac-address = <&factory 0x1e006>;
		};

		port@1 {
			status = "okay";
			label = "lan4";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan2";
		};

		port@4 {
			status = "okay";
			label = "lan1";
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;

		mediatek,mtd-eeprom = <&factory 0x0>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;

		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&state_default {
	gpio {
		groups = "uart2", "uart3", "wdt";
		function = "gpio";
	};
};

&xhci {
	status = "disabled";
};
