--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1118,6 +1118,7 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h3-orangepi-plus2e.dtb \
 	sun8i-h3-orangepi-zero-plus2.dtb \
 	sun8i-h3-rervision-dvk.dtb \
+	sun8i-h3-zeropi.dtb \
 	sun8i-r16-bananapi-m2m.dtb \
 	sun8i-r16-nintendo-nes-classic.dtb \
 	sun8i-r16-nintendo-super-nes-classic.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h3-zeropi.dts
@@ -0,0 +1,66 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+
+#include "sun8i-h3-nanopi.dtsi"
+
+/ {
+	model = "FriendlyElec ZeroPi";
+	compatible = "friendlyarm,zeropi", "allwinner,sun8i-h3";
+
+	aliases {
+		ethernet0 = &emac;
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gmac_power_pin_nanopi>;
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&pio {
+	gmac_power_pin_nanopi: gmac_power_pin@0 {
+		pins = "PD6";
+		function = "gpio_out";
+	};
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&usb_otg {
+	status = "okay";
+	dr_mode = "peripheral";
+};
+
+&usbphy {
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+};
