From fd6dfd0af2ab83d8df5d7b17a52fbf0284e42f2b Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Mon, 28 Dec 2015 14:34:44 -0800
Subject: [PATCH 276/423] drm/vc4: Move the plane clipping/scaling setup to a
 separate function.

As we add actual scaling, this is going to get way more complicated.

Signed-off-by: Eric Anholt <eric@anholt.net>
(cherry picked from commit 5c6799942003df91801b1d2277bba34d71f99603)
---
 drivers/gpu/drm/vc4/vc4_plane.c | 78 +++++++++++++++++++++++++++--------------
 1 file changed, 52 insertions(+), 26 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_plane.c
+++ b/drivers/gpu/drm/vc4/vc4_plane.c
@@ -40,6 +40,14 @@ struct vc4_plane_state {
 	 * hardware at vc4_crtc_atomic_flush() time.
 	 */
 	u32 __iomem *hw_dlist;
+
+	/* Clipped coordinates of the plane on the display. */
+	int crtc_x, crtc_y, crtc_w, crtc_h;
+
+	/* Offset to start scanning out from the start of the plane's
+	 * BO.
+	 */
+	u32 offset;
 };
 
 static inline struct vc4_plane_state *
@@ -167,22 +175,17 @@ static void vc4_dlist_write(struct vc4_p
 	vc4_state->dlist[vc4_state->dlist_count++] = val;
 }
 
-/* Writes out a full display list for an active plane to the plane's
- * private dlist state.
- */
-static int vc4_plane_mode_set(struct drm_plane *plane,
-			      struct drm_plane_state *state)
+static int vc4_plane_setup_clipping_and_scaling(struct drm_plane_state *state)
 {
 	struct vc4_plane_state *vc4_state = to_vc4_plane_state(state);
 	struct drm_framebuffer *fb = state->fb;
-	struct drm_gem_cma_object *bo = drm_fb_cma_get_gem_obj(fb, 0);
-	u32 ctl0_offset = vc4_state->dlist_count;
-	const struct hvs_format *format = vc4_get_hvs_format(fb->pixel_format);
-	uint32_t offset = fb->offsets[0];
-	int crtc_x = state->crtc_x;
-	int crtc_y = state->crtc_y;
-	int crtc_w = state->crtc_w;
-	int crtc_h = state->crtc_h;
+
+	vc4_state->offset = fb->offsets[0];
+
+	vc4_state->crtc_x = state->crtc_x;
+	vc4_state->crtc_y = state->crtc_y;
+	vc4_state->crtc_w = state->crtc_w;
+	vc4_state->crtc_h = state->crtc_h;
 
 	if (state->crtc_w << 16 != state->src_w ||
 	    state->crtc_h << 16 != state->src_h) {
@@ -194,18 +197,41 @@ static int vc4_plane_mode_set(struct drm
 		return -EINVAL;
 	}
 
-	if (crtc_x < 0) {
-		offset += drm_format_plane_cpp(fb->pixel_format, 0) * -crtc_x;
-		crtc_w += crtc_x;
-		crtc_x = 0;
+	if (vc4_state->crtc_x < 0) {
+		vc4_state->offset += (drm_format_plane_cpp(fb->pixel_format,
+							   0) *
+				      -vc4_state->crtc_x);
+		vc4_state->crtc_w += vc4_state->crtc_x;
+		vc4_state->crtc_x = 0;
 	}
 
-	if (crtc_y < 0) {
-		offset += fb->pitches[0] * -crtc_y;
-		crtc_h += crtc_y;
-		crtc_y = 0;
+	if (vc4_state->crtc_y < 0) {
+		vc4_state->offset += fb->pitches[0] * -vc4_state->crtc_y;
+		vc4_state->crtc_h += vc4_state->crtc_y;
+		vc4_state->crtc_y = 0;
 	}
 
+	return 0;
+}
+
+
+/* Writes out a full display list for an active plane to the plane's
+ * private dlist state.
+ */
+static int vc4_plane_mode_set(struct drm_plane *plane,
+			      struct drm_plane_state *state)
+{
+	struct vc4_plane_state *vc4_state = to_vc4_plane_state(state);
+	struct drm_framebuffer *fb = state->fb;
+	struct drm_gem_cma_object *bo = drm_fb_cma_get_gem_obj(fb, 0);
+	u32 ctl0_offset = vc4_state->dlist_count;
+	const struct hvs_format *format = vc4_get_hvs_format(fb->pixel_format);
+	int ret;
+
+	ret = vc4_plane_setup_clipping_and_scaling(state);
+	if (ret)
+		return ret;
+
 	vc4_dlist_write(vc4_state,
 			SCALER_CTL0_VALID |
 			(format->pixel_order << SCALER_CTL0_ORDER_SHIFT) |
@@ -215,8 +241,8 @@ static int vc4_plane_mode_set(struct drm
 	/* Position Word 0: Image Positions and Alpha Value */
 	vc4_dlist_write(vc4_state,
 			VC4_SET_FIELD(0xff, SCALER_POS0_FIXED_ALPHA) |
-			VC4_SET_FIELD(crtc_x, SCALER_POS0_START_X) |
-			VC4_SET_FIELD(crtc_y, SCALER_POS0_START_Y));
+			VC4_SET_FIELD(vc4_state->crtc_x, SCALER_POS0_START_X) |
+			VC4_SET_FIELD(vc4_state->crtc_y, SCALER_POS0_START_Y));
 
 	/* Position Word 1: Scaled Image Dimensions.
 	 * Skipped due to SCALER_CTL0_UNITY scaling.
@@ -228,8 +254,8 @@ static int vc4_plane_mode_set(struct drm
 				      SCALER_POS2_ALPHA_MODE_PIPELINE :
 				      SCALER_POS2_ALPHA_MODE_FIXED,
 				      SCALER_POS2_ALPHA_MODE) |
-			VC4_SET_FIELD(crtc_w, SCALER_POS2_WIDTH) |
-			VC4_SET_FIELD(crtc_h, SCALER_POS2_HEIGHT));
+			VC4_SET_FIELD(vc4_state->crtc_w, SCALER_POS2_WIDTH) |
+			VC4_SET_FIELD(vc4_state->crtc_h, SCALER_POS2_HEIGHT));
 
 	/* Position Word 3: Context.  Written by the HVS. */
 	vc4_dlist_write(vc4_state, 0xc0c0c0c0);
@@ -237,7 +263,7 @@ static int vc4_plane_mode_set(struct drm
 	vc4_state->pw0_offset = vc4_state->dlist_count;
 
 	/* Pointer Word 0: RGB / Y Pointer */
-	vc4_dlist_write(vc4_state, bo->paddr + offset);
+	vc4_dlist_write(vc4_state, bo->paddr + vc4_state->offset);
 
 	/* Pointer Context Word 0: Written by the HVS */
 	vc4_dlist_write(vc4_state, 0xc0c0c0c0);
