From 3b2e7c7c83873f4c073d501c2fff80518e264240 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 4 Jan 2016 20:24:00 +0100
Subject: [PATCH] MIPS: ralink: Add a few missing clocks

Signed-off-by: John Crispin <blogic@openwrt.org>
Cc: linux-mips@linux-mips.org
Patchwork: https://patchwork.linux-mips.org/patch/11995/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ralink/mt7620.c | 3 +++
 arch/mips/ralink/rt305x.c | 1 +
 arch/mips/ralink/rt3883.c | 1 +
 3 files changed, 5 insertions(+)

--- a/arch/mips/ralink/mt7620.c
+++ b/arch/mips/ralink/mt7620.c
@@ -436,7 +436,10 @@ void __init ralink_clk_init(void)
 	ralink_clk_add("10000100.timer", periph_rate);
 	ralink_clk_add("10000120.watchdog", periph_rate);
 	ralink_clk_add("10000b00.spi", sys_rate);
+	ralink_clk_add("10000b40.spi", sys_rate);
 	ralink_clk_add("10000c00.uartlite", periph_rate);
+	ralink_clk_add("10000d00.uart1", periph_rate);
+	ralink_clk_add("10000e00.uart2", periph_rate);
 	ralink_clk_add("10180000.wmac", xtal_rate);
 
 	if (IS_ENABLED(CONFIG_USB) && is_mt76x8()) {
--- a/arch/mips/ralink/rt305x.c
+++ b/arch/mips/ralink/rt305x.c
@@ -201,6 +201,7 @@ void __init ralink_clk_init(void)
 	ralink_clk_add("cpu", cpu_rate);
 	ralink_clk_add("sys", sys_rate);
 	ralink_clk_add("10000b00.spi", sys_rate);
+	ralink_clk_add("10000b40.spi", sys_rate);
 	ralink_clk_add("10000100.timer", wdt_rate);
 	ralink_clk_add("10000120.watchdog", wdt_rate);
 	ralink_clk_add("10000500.uart", uart_rate);
--- a/arch/mips/ralink/rt3883.c
+++ b/arch/mips/ralink/rt3883.c
@@ -109,6 +109,7 @@ void __init ralink_clk_init(void)
 	ralink_clk_add("10000120.watchdog", sys_rate);
 	ralink_clk_add("10000500.uart", 40000000);
 	ralink_clk_add("10000b00.spi", sys_rate);
+	ralink_clk_add("10000b40.spi", sys_rate);
 	ralink_clk_add("10000c00.uartlite", 40000000);
 	ralink_clk_add("10100000.ethernet", sys_rate);
 	ralink_clk_add("10180000.wmac", 40000000);
