From: Dmitri Epshtein <dima@marvell.com>
Date: Sat, 12 Mar 2016 18:44:19 +0100
Subject: [PATCH] net: mvneta: fix error messages in mvneta_port_down function

This commit corrects error printing when shutting down the port.

[gregory.clement@free-electrons.com: split initial commit in two
individual changes]
Signed-off-by: Dmitri Epshtein <dima@marvell.com>
Signed-off-by: Gregory CLEMENT <gregory.clement@free-electrons.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -1105,7 +1105,7 @@ static void mvneta_port_down(struct mvne
 	do {
 		if (count++ >= MVNETA_RX_DISABLE_TIMEOUT_MSEC) {
 			netdev_warn(pp->dev,
-				    "TIMEOUT for RX stopped ! rx_queue_cmd: 0x08%x\n",
+				    "TIMEOUT for RX stopped ! rx_queue_cmd: 0x%08x\n",
 				    val);
 			break;
 		}
@@ -1144,7 +1144,7 @@ static void mvneta_port_down(struct mvne
 	do {
 		if (count++ >= MVNETA_TX_FIFO_EMPTY_TIMEOUT) {
 			netdev_warn(pp->dev,
-				    "TX FIFO empty timeout status=0x08%x\n",
+				    "TX FIFO empty timeout status=0x%08x\n",
 				    val);
 			break;
 		}
