From: Felix Fietkau <nbd@nbd.name>
Date: Mon, 8 Jun 2020 17:01:12 +0200
Subject: [PATCH] net: ethernet: mtk_eth_soc: use napi_consume_skb

Should improve performance, since it can use bulk free

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -853,7 +853,8 @@ static int txd_to_idx(struct mtk_tx_ring
 	return ((void *)dma - (void *)ring->dma) / sizeof(*dma);
 }
 
-static void mtk_tx_unmap(struct mtk_eth *eth, struct mtk_tx_buf *tx_buf)
+static void mtk_tx_unmap(struct mtk_eth *eth, struct mtk_tx_buf *tx_buf,
+			 bool napi)
 {
 	if (MTK_HAS_CAPS(eth->soc->caps, MTK_QDMA)) {
 		if (tx_buf->flags & MTK_TX_FLAGS_SINGLE0) {
@@ -885,8 +886,12 @@ static void mtk_tx_unmap(struct mtk_eth
 
 	tx_buf->flags = 0;
 	if (tx_buf->skb &&
-	    (tx_buf->skb != (struct sk_buff *)MTK_DMA_DUMMY_DESC))
-		dev_kfree_skb_any(tx_buf->skb);
+	    (tx_buf->skb != (struct sk_buff *)MTK_DMA_DUMMY_DESC)) {
+		if (napi)
+			napi_consume_skb(tx_buf->skb, napi);
+		else
+			dev_kfree_skb_any(tx_buf->skb);
+	}
 	tx_buf->skb = NULL;
 }
 
@@ -1064,7 +1069,7 @@ err_dma:
 		tx_buf = mtk_desc_to_tx_buf(ring, itxd);
 
 		/* unmap dma */
-		mtk_tx_unmap(eth, tx_buf);
+		mtk_tx_unmap(eth, tx_buf, false);
 
 		itxd->txd3 = TX_DMA_LS0 | TX_DMA_OWNER_CPU;
 		if (!MTK_HAS_CAPS(eth->soc->caps, MTK_QDMA))
@@ -1382,7 +1387,7 @@ static int mtk_poll_tx_qdma(struct mtk_e
 			done[mac]++;
 			budget--;
 		}
-		mtk_tx_unmap(eth, tx_buf);
+		mtk_tx_unmap(eth, tx_buf, true);
 
 		ring->last_free = desc;
 		atomic_inc(&ring->free_count);
@@ -1419,7 +1424,7 @@ static int mtk_poll_tx_pdma(struct mtk_e
 			budget--;
 		}
 
-		mtk_tx_unmap(eth, tx_buf);
+		mtk_tx_unmap(eth, tx_buf, true);
 
 		desc = &ring->dma[cpu];
 		ring->last_free = desc;
@@ -1621,7 +1626,7 @@ static void mtk_tx_clean(struct mtk_eth
 
 	if (ring->buf) {
 		for (i = 0; i < MTK_DMA_SIZE; i++)
-			mtk_tx_unmap(eth, &ring->buf[i]);
+			mtk_tx_unmap(eth, &ring->buf[i], false);
 		kfree(ring->buf);
 		ring->buf = NULL;
 	}
