From: Felix Fietkau <nbd@nbd.name>
Date: Thu, 15 Mar 2018 20:49:58 +0100
Subject: [PATCH] net: 8021q: support hardware flow table offload

Add the VLAN ID and protocol information

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/8021q/vlan_dev.c
+++ b/net/8021q/vlan_dev.c
@@ -27,6 +27,11 @@
 #include <linux/phy.h>
 #include <net/arp.h>
 
+#if IS_ENABLED(CONFIG_NF_FLOW_TABLE)
+#include <linux/netfilter.h>
+#include <net/netfilter/nf_flow_table.h>
+#endif
+
 #include "vlan.h"
 #include "vlanproc.h"
 #include <linux/if_vlan.h>
@@ -744,6 +749,27 @@ static int vlan_dev_get_iflink(const str
 	return real_dev->ifindex;
 }
 
+#if IS_ENABLED(CONFIG_NF_FLOW_TABLE)
+static int vlan_dev_flow_offload_check(struct flow_offload_hw_path *path)
+{
+	struct net_device *dev = path->dev;
+	struct vlan_dev_priv *vlan = vlan_dev_priv(dev);
+
+	if (path->flags & FLOW_OFFLOAD_PATH_VLAN)
+		return -EEXIST;
+
+	path->flags |= FLOW_OFFLOAD_PATH_VLAN;
+	path->vlan_proto = vlan->vlan_proto;
+	path->vlan_id = vlan->vlan_id;
+	path->dev = vlan->real_dev;
+
+	if (vlan->real_dev->netdev_ops->ndo_flow_offload_check)
+		return vlan->real_dev->netdev_ops->ndo_flow_offload_check(path);
+
+	return 0;
+}
+#endif /* CONFIG_NF_FLOW_TABLE */
+
 static const struct ethtool_ops vlan_ethtool_ops = {
 	.get_link_ksettings	= vlan_ethtool_get_link_ksettings,
 	.get_drvinfo	        = vlan_ethtool_get_drvinfo,
@@ -782,6 +808,9 @@ static const struct net_device_ops vlan_
 #endif
 	.ndo_fix_features	= vlan_dev_fix_features,
 	.ndo_get_iflink		= vlan_dev_get_iflink,
+#if IS_ENABLED(CONFIG_NF_FLOW_TABLE)
+	.ndo_flow_offload_check = vlan_dev_flow_offload_check,
+#endif
 };
 
 static void vlan_dev_free(struct net_device *dev)
