From e5745143a2984cf44fbfc0b3aedb49e57873f109 Mon Sep 17 00:00:00 2001
From: Sam Shih <sam.shih@mediatek.com>
Date: Mon, 20 Apr 2020 17:17:04 +0800
Subject: [PATCH 3/3] configs: enable mtd and mtk_spi_nand in defconfig

This patch enable mtk and mtk_spi_nand in mt7622_rfb defconfig

Signed-off-by: Sam Shih <sam.shih@mediatek.com>
---
 configs/mt7622_rfb_defconfig | 5 +++++
 1 file changed, 5 insertions(+)

--- a/configs/mt7622_rfb_defconfig
+++ b/configs/mt7622_rfb_defconfig
@@ -13,6 +13,7 @@ CONFIG_DEFAULT_FDT_FILE="mt7622-rfb"
 CONFIG_SYS_PROMPT="MT7622> "
 CONFIG_CMD_BOOTMENU=y
 CONFIG_CMD_MMC=y
+CONFIG_CMD_NAND=y
 CONFIG_CMD_PCI=y
 CONFIG_CMD_SF_TEST=y
 CONFIG_CMD_PING=y
