From 31ca877744d95713e4925de542e1c686ab08a542 Mon Sep 17 00:00:00 2001
From: "Jason A. Donenfeld" <Jason@zx2c4.com>
Date: Sat, 27 Feb 2021 13:20:24 +0100
Subject: [PATCH] MIPS: select CPU_MIPS64 for remaining MIPS64 CPUs

The CPU_MIPS64 and CPU_MIPS32 variables are supposed to be able to
distinguish broadly between 64-bit and 32-bit MIPS CPUs. However, they
weren't selected by the specialty CPUs, Octeon and Loongson, which meant
it was possible to hit a weird state of:

    MIPS=y, CONFIG_64BIT=y, CPU_MIPS64=n

This commit rectifies the issue by having CPU_MIPS64 be selected when
the missing Octeon or Loongson models are selected.

Cc: Thomas Bogendoerfer <tsbogend@alpha.franken.de>
Cc: Ralf Baechle <ralf@linux-mips.org>
Cc: George Cherian <gcherian@marvell.com>
Cc: Huacai Chen <chenhuacai@kernel.org>
Cc: Jiaxun Yang <jiaxun.yang@flygoat.com>
Signed-off-by: Jason A. Donenfeld <Jason@zx2c4.com>
---
 arch/mips/Kconfig | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -2036,7 +2036,8 @@ config CPU_MIPS32
 
 config CPU_MIPS64
 	bool
-	default y if CPU_MIPS64_R1 || CPU_MIPS64_R2 || CPU_MIPS64_R6
+	default y if CPU_MIPS64_R1 || CPU_MIPS64_R2 || CPU_MIPS64_R6 || \
+		     CPU_LOONGSON64 || CPU_CAVIUM_OCTEON
 
 #
 # These indicate the revision of the architecture
